(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A5")
  (title_block
    (title "CIMDIT")
    (date "2022-02-08")
    (rev "1.0")
    (comment 1 "@grumpydevelop@contentnation.net")
    (comment 2 "https://contentnation.net/en/grumpydevelop/cimdit_1")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory "out/")
    )
  )

  (net 0 "")
  (net 1 "GND")
  (net 2 "+5V")
  (net 3 "/I2C_DATA")
  (net 4 "/I2C_CLOCK")
  (net 5 "unconnected-(U2-Pad11)")
  (net 6 "unconnected-(U2-Pad14)")
  (net 7 "unconnected-(U2-Pad19)")
  (net 8 "unconnected-(U2-Pad20)")
  (net 9 "/ANALOG_MUX2")
  (net 10 "/ANALOG_MUX1")
  (net 11 "/ANALOG_MUX0")
  (net 12 "/Rotary Encoder/I2C_CLOCK_ROT")
  (net 13 "/Rotary Encoder/I2C_DATA_ROT")
  (net 14 "/Rotary Encoder/GND_ROT")
  (net 15 "/Rotary Encoder/+5V_ROT")
  (net 16 "/Rotary Encoder/INT_ROT")
  (net 17 "Net-(DKD1-Pad1)")
  (net 18 "unconnected-(U3-Pad19)")
  (net 19 "/SCLK")
  (net 20 "/MISO")
  (net 21 "/INT")
  (net 22 "unconnected-(U3-Pad11)")
  (net 23 "unconnected-(U3-Pad14)")
  (net 24 "Net-(DKD10-Pad1)")
  (net 25 "Net-(DKD11-Pad1)")
  (net 26 "Net-(DKD12-Pad1)")
  (net 27 "Net-(DKD13-Pad1)")
  (net 28 "Net-(DKD14-Pad1)")
  (net 29 "Net-(DKD15-Pad1)")
  (net 30 "/EINK_SEL")
  (net 31 "/ANALOG_MUX3")
  (net 32 "/MOSI")
  (net 33 "/ANALOG_IN")
  (net 34 "Net-(DKD16-Pad1)")
  (net 35 "/KeyMatrix Ext Diodes/I2C_DATA_KEY")
  (net 36 "/KeyMatrix Ext Diodes/I2C_CLOCK_KEY")
  (net 37 "/KeyMatrix Ext Diodes/GND_KEY")
  (net 38 "/KeyMatrix Ext Diodes/+5V_KEY")
  (net 39 "/Analog Multiplexer/ANALOG_MUX1")
  (net 40 "/Analog Multiplexer/ANALOG_MUX2")
  (net 41 "/Analog Multiplexer/ANALOG_MUX0")
  (net 42 "/Analog Multiplexer/GND_ANALOG")
  (net 43 "/Analog Multiplexer/+5V_ANALOG")
  (net 44 "/Analog Multiplexer/ANALOG_ENABLE")
  (net 45 "/Analog Multiplexer/ANALOG_OUT")
  (net 46 "/Analog Multiplexer/ANALOG_MUX3")
  (net 47 "Net-(JD4-Pad1)")
  (net 48 "Net-(JK1-Pad1)")
  (net 49 "Net-(JK2-Pad1)")
  (net 50 "Net-(JK3-Pad1)")
  (net 51 "Net-(JK4-Pad1)")
  (net 52 "Net-(JK5-Pad1)")
  (net 53 "unconnected-(U4-Pad19)")
  (net 54 "unconnected-(U4-Pad20)")
  (net 55 "unconnected-(U4-Pad11)")
  (net 56 "unconnected-(U4-Pad14)")
  (net 57 "Net-(JK6-Pad1)")
  (net 58 "Net-(JK7-Pad1)")
  (net 59 "Net-(JK8-Pad1)")
  (net 60 "Net-(JK11-Pad1)")
  (net 61 "Net-(JK12-Pad1)")
  (net 62 "Net-(JK13-Pad1)")
  (net 63 "Net-(JK14-Pad1)")
  (net 64 "Net-(JK15-Pad1)")
  (net 65 "Net-(JK16-Pad1)")
  (net 66 "Net-(JK17-Pad1)")
  (net 67 "Net-(JK18-Pad1)")
  (net 68 "Net-(JKD1-Pad1)")
  (net 69 "Net-(JKD2-Pad1)")
  (net 70 "Net-(JKD3-Pad1)")
  (net 71 "Net-(JKD5-Pad1)")
  (net 72 "Net-(JKD6-Pad1)")
  (net 73 "Net-(JKD7-Pad1)")
  (net 74 "Net-(JKD8-Pad1)")
  (net 75 "Net-(J6-Pad1)")
  (net 76 "Net-(J7-Pad1)")
  (net 77 "Net-(J8-Pad1)")
  (net 78 "Net-(J9-Pad1)")
  (net 79 "/Key Matrix Diode/+5V_KEY")
  (net 80 "/Key Matrix Diode/GND_KEY")
  (net 81 "/Key Matrix Diode/I2C_CLOCK_KEY")
  (net 82 "/Key Matrix Diode/I2C_DATA_KEY")
  (net 83 "Net-(DKD1-Pad2)")
  (net 84 "Net-(DKD9-Pad2)")
  (net 85 "Net-(DKD2-Pad2)")
  (net 86 "Net-(DKD10-Pad2)")
  (net 87 "Net-(DKD3-Pad2)")
  (net 88 "Net-(DKD11-Pad2)")
  (net 89 "Net-(DKD4-Pad2)")
  (net 90 "Net-(DKD12-Pad2)")
  (net 91 "Net-(DKD5-Pad2)")
  (net 92 "Net-(DKD13-Pad2)")
  (net 93 "Net-(DKD6-Pad2)")
  (net 94 "Net-(DKD14-Pad2)")
  (net 95 "Net-(DKD7-Pad2)")
  (net 96 "Net-(DKD15-Pad2)")
  (net 97 "Net-(DKD8-Pad2)")
  (net 98 "Net-(DKD16-Pad2)")
  (net 99 "Net-(J10-Pad1)")
  (net 100 "Net-(J11-Pad1)")
  (net 101 "Net-(J12-Pad1)")
  (net 102 "Net-(J13-Pad1)")
  (net 103 "Net-(DKD17-Pad2)")
  (net 104 "Net-(DKD18-Pad2)")
  (net 105 "Net-(DKD19-Pad2)")
  (net 106 "Net-(DKD20-Pad2)")
  (net 107 "Net-(DKD21-Pad2)")
  (net 108 "Net-(DKD22-Pad2)")
  (net 109 "Net-(DKD23-Pad2)")
  (net 110 "Net-(DKD24-Pad2)")
  (net 111 "Net-(DKD25-Pad2)")
  (net 112 "Net-(DKD26-Pad2)")
  (net 113 "Net-(DKD27-Pad2)")
  (net 114 "Net-(DKD28-Pad2)")
  (net 115 "Net-(DKD29-Pad2)")
  (net 116 "Net-(DKD30-Pad2)")
  (net 117 "Net-(DKD31-Pad2)")
  (net 118 "Net-(DKD32-Pad2)")
  (net 119 "Net-(DKD33-Pad2)")
  (net 120 "Net-(DKD34-Pad2)")
  (net 121 "Net-(DKD35-Pad2)")
  (net 122 "Net-(DKD36-Pad2)")
  (net 123 "Net-(DKD37-Pad2)")
  (net 124 "Net-(DKD38-Pad2)")
  (net 125 "Net-(DKD39-Pad2)")
  (net 126 "Net-(DKD40-Pad2)")
  (net 127 "Net-(DKD41-Pad2)")
  (net 128 "Net-(DKD42-Pad2)")
  (net 129 "Net-(DKD43-Pad2)")
  (net 130 "Net-(DKD44-Pad2)")
  (net 131 "Net-(DKD45-Pad2)")
  (net 132 "Net-(DKD46-Pad2)")
  (net 133 "Net-(DKD47-Pad2)")
  (net 134 "Net-(DKD48-Pad2)")
  (net 135 "Net-(DKD49-Pad2)")
  (net 136 "Net-(DKD50-Pad2)")
  (net 137 "Net-(DKD51-Pad2)")
  (net 138 "Net-(DKD52-Pad2)")
  (net 139 "Net-(DKD53-Pad2)")
  (net 140 "Net-(DKD54-Pad2)")
  (net 141 "Net-(DKD55-Pad2)")
  (net 142 "Net-(DKD56-Pad2)")
  (net 143 "Net-(DKD57-Pad2)")
  (net 144 "Net-(DKD58-Pad2)")
  (net 145 "Net-(DKD59-Pad2)")
  (net 146 "Net-(DKD60-Pad2)")
  (net 147 "Net-(DKD61-Pad2)")
  (net 148 "Net-(DKD62-Pad2)")
  (net 149 "Net-(DKD63-Pad2)")
  (net 150 "Net-(DKD64-Pad2)")
  (net 151 "Net-(J14-Pad1)")
  (net 152 "Net-(J15-Pad1)")
  (net 153 "Net-(J16-Pad1)")
  (net 154 "Net-(J17-Pad1)")
  (net 155 "Net-(J18-Pad1)")
  (net 156 "Net-(J19-Pad1)")
  (net 157 "Net-(J20-Pad1)")
  (net 158 "Net-(J23-Pad1)")
  (net 159 "unconnected-(J100-Pad1)")
  (net 160 "unconnected-(J100-Pad2)")
  (net 161 "unconnected-(J100-Pad3)")
  (net 162 "unconnected-(J100-Pad7)")
  (net 163 "unconnected-(J100-Pad8)")
  (net 164 "unconnected-(J101-Pad7)")
  (net 165 "unconnected-(J101-Pad8)")
  (net 166 "unconnected-(J101-Pad10)")
  (net 167 "unconnected-(J101-Pad12)")
  (net 168 "/KeyMatrix wired/+5V_KEY")
  (net 169 "Net-(J30-Pad1)")
  (net 170 "Net-(J31-Pad1)")
  (net 171 "Net-(J32-Pad1)")
  (net 172 "Net-(J33-Pad1)")
  (net 173 "Net-(J34-Pad1)")
  (net 174 "Net-(J35-Pad1)")
  (net 175 "Net-(J36-Pad1)")
  (net 176 "Net-(J37-Pad1)")
  (net 177 "Net-(J38-Pad1)")
  (net 178 "Net-(J39-Pad1)")
  (net 179 "Net-(J40-Pad1)")
  (net 180 "Net-(J41-Pad1)")
  (net 181 "Net-(J42-Pad1)")
  (net 182 "Net-(J43-Pad1)")
  (net 183 "Net-(J44-Pad1)")
  (net 184 "Net-(J45-Pad1)")
  (net 185 "/KeyMatrix wired/GND_KEY")
  (net 186 "/KeyMatrix wired/I2C_DATA_KEY")
  (net 187 "/KeyMatrix wired/I2C_CLOCK_KEY")
  (net 188 "unconnected-(U1-Pad11)")
  (net 189 "unconnected-(U1-Pad14)")
  (net 190 "unconnected-(U1-Pad19)")
  (net 191 "unconnected-(U1-Pad20)")

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429) (tstamp 00000000-0000-0000-0000-000061fdfa80)
    (at 63.5 96.52)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/27de3dac-3961-4a93-bc2f-08d7f9d0c9e7")
    (attr through_hole)
    (fp_text reference "J22" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 793a5c8e-e35a-48bf-b3ce-7150d8d81329)
    )
    (fp_text value "KEY" (at 0 -2.54) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92360226-9a8f-403a-8a31-06f251c161ed)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14dfe1df-9130-408b-8e92-e333eab5e657)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 1b1625fa-0b5f-4473-9681-8e3d4efb727f))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 3baa497f-167e-42dc-b5f1-4fac4b1e25d0))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 71e71012-14b0-426f-999a-ebce6363d104))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 85003bd5-c652-454f-8fa2-f25a8362adf5))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 942e6610-8521-4e71-b768-bee49d38818a))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp dd8a2435-de15-4152-95d2-3c93f2aa3ff5))
    (fp_line (start -1.8 9.4) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 079c94ab-c0fe-45e4-b152-fa21d9c7dd57))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 35e024d9-3222-4176-945e-f05189f3d172))
    (fp_line (start 1.75 -1.8) (end 1.75 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 6f9180cf-15ba-4fe0-aac0-c0c15bccbef8))
    (fp_line (start 1.75 9.4) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 9fb4993c-1a95-4346-8936-10a2052044c6))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 12038284-fef2-4ba8-8d68-477752068032))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 143043a2-d41b-42d5-af5e-9c7e32fd1524))
    (fp_line (start 1.27 -0.635) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 4ac5f4ab-f271-4d93-9d90-9371518377ee))
    (fp_line (start -1.27 8.89) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 82c21d94-c942-4e75-a775-d50699c9ccbc))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ebd2d722-b1f4-4660-8688-03bcc8dd0369))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/KeyMatrix Ext Diodes/I2C_DATA_KEY") (pinfunction "Pin_1") (pintype "passive") (tstamp 90778d24-7d72-4e05-9f17-5b3edfbbaebf))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/KeyMatrix Ext Diodes/I2C_CLOCK_KEY") (pinfunction "Pin_2") (pintype "passive") (tstamp 0a5988ff-be2f-47d6-ae81-4946cccccf6f))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/KeyMatrix Ext Diodes/GND_KEY") (pinfunction "Pin_3") (pintype "passive") (tstamp 837d1dd1-7d93-48e9-a1c0-ac450e2f5cf2))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/KeyMatrix Ext Diodes/+5V_KEY") (pinfunction "Pin_4") (pintype "passive") (tstamp 9358a53e-a337-4ac5-b1a7-7742caa43548))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429) (tstamp 00000000-0000-0000-0000-000061fdfad1)
    (at 137.16 71.12 -90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/b4f31029-aadc-49e1-aae0-4cc5be4e6966")
    (attr through_hole)
    (fp_text reference "J21" (at 0 -2.77 -90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b32fb5c-4087-4f44-bca4-03989aac998c)
    )
    (fp_text value "KEY DIODE" (at 2.54 -2.54) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f1561a2-3df0-4a72-8af1-fb9dfe3644ae)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d5e8a182-c2e3-47ec-9243-0194c428e8d1)
    )
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 19ac0b8c-1097-48f9-a966-ff74fb085035))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8214629c-c3c3-4987-8ef2-fd09e044d35f))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp d975e6dc-e5b9-4b40-8b19-218e7ac009a7))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp db8333a5-5cda-44d3-9772-23c019a50c8d))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp e1d3c6a7-dc1e-4359-969f-73a022567641))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp fdf67426-187b-491f-ba12-b3e3b275048d))
    (fp_line (start 1.75 9.4) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 0cfdcf7c-3418-434d-b896-31dbbee522d4))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 6536d06e-d14b-4fd3-9e01-cabbb27017ff))
    (fp_line (start -1.8 9.4) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 7d4c867e-2676-4743-8ac2-dbda526e6ed1))
    (fp_line (start 1.75 -1.8) (end 1.75 9.4) (layer "F.CrtYd") (width 0.05) (tstamp ac281f1d-8be4-4d3a-b949-316419233d2e))
    (fp_line (start -1.27 8.89) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 25b21e98-eee9-4b38-b500-581c3c72056e))
    (fp_line (start 1.27 -0.635) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 6aac5960-bdbf-4d51-92d2-f310c7e7fad2))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 7b9d2445-204c-40bc-a68a-6836fc6e06db))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp c9009e31-8e3b-44b2-bcf8-7a88af7d2124))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp d19d8082-4b21-4793-b7ca-d0b0d1276712))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "/Key Matrix Diode/+5V_KEY") (pinfunction "Pin_1") (pintype "passive") (tstamp d2df2a56-cd3b-43c4-b04c-9c985f91cb06))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "/Key Matrix Diode/GND_KEY") (pinfunction "Pin_2") (pintype "passive") (tstamp ac583067-de37-4edc-b2d9-e8246e4bfe52))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "/Key Matrix Diode/I2C_CLOCK_KEY") (pinfunction "Pin_3") (pintype "passive") (tstamp 349a8260-8a78-4133-9550-256559bd633a))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "/Key Matrix Diode/I2C_DATA_KEY") (pinfunction "Pin_4") (pintype "passive") (tstamp e1a7871c-e644-4898-82c2-0435ccd3c2b1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 00000000-0000-0000-0000-000061fef633)
    (at 68.58 55.88 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000068677448")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10202d55-3664-4109-9668-6e7e716ac505)
    )
    (fp_text value "ANALOG" (at -2.54 17.78) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f7b6d95-8417-42db-ba83-785b467955eb)
    )
    (fp_text user "${REFERENCE}" (at 0 11.2 180) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19af9b1c-2df3-40ff-a97a-f6567f6bb6cc)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 065a3890-a91b-437c-8fd3-338149430300))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 50ed3717-1be5-4bd5-be93-14d59f82695a))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 5e41e0c1-ab9c-4b86-95da-b42e2d22e7c9))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 8f63c59e-496f-4d07-881d-950dddedb342))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c1d369f3-60c6-4980-86ca-a81c3fcc68d1))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp f3119cd7-c265-407b-8ffb-cb6e3e912d44))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 0b55d3c0-46c6-4797-b13d-d1267e2011fd))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 27e2f0a5-5760-407f-a270-8e94d9d608d3))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 5f04c54e-f1b5-452d-8132-635d1568b48c))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp d118d9b9-3dbd-4326-b668-d6df066a3155))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 0200d232-6950-4b02-addf-abbbd0231c00))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 3276cf8e-d078-4ac2-a2bf-aa0ae3c05e56))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 98b62c04-64d9-4844-a0ba-694b5c069afd))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 9bdb0021-1aff-4b7d-83cc-383af40ff337))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp d593d3f3-1835-4ba4-85d7-26e478285165))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/ANALOG_MUX1") (pinfunction "Pin_1") (pintype "passive") (tstamp b50272ab-d68b-4a92-a4b7-13d73c46fc69))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/ANALOG_MUX2") (pinfunction "Pin_2") (pintype "passive") (tstamp d61cae1a-6c7f-49e0-a1b9-7d1c54c43856))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/ANALOG_MUX0") (pinfunction "Pin_3") (pintype "passive") (tstamp fcbcb773-e0d1-4b53-a42f-14c4f0711231))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 59176017-1acc-471f-a4bf-ea8f11c715cd))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive") (tstamp c93cd49c-b481-4da4-a2a8-b2ee484ca8d8))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "Pin_6") (pintype "passive") (tstamp c2f995d2-e2e8-4ebe-b4d1-e1ff254cddfa))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/ANALOG_IN") (pinfunction "Pin_7") (pintype "passive") (tstamp 37a9ef44-52d8-49d0-a3fd-929c5217076e))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/ANALOG_MUX3") (pinfunction "Pin_8") (pintype "passive") (tstamp 16e2f23e-2a63-42da-bcaf-c7d49092b8e9))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A430) (tstamp 00000000-0000-0000-0000-000061fef717)
    (at 91.44 38.1)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000069103554")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cb56e162-0233-457e-841d-d3eb427485b3)
    )
    (fp_text value "E-INK" (at 0 15.47) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3062fb8c-147a-4ff6-8427-6e1a425eb08c)
    )
    (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f91ea82b-b2a1-433f-8c23-1b0466cee4e3)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 59424b95-19b9-4b71-b238-59a22a8b8533))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 66843928-373e-440e-960a-e90028903cb9))
    (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 6c58d5f8-69bf-485f-bfd0-c51c6a1bfb85))
    (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 6d79ddf8-b3f2-44bb-8e75-3bf4e260b3a5))
    (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 816464f1-94cd-4b6b-8a22-bb46f77b44a3))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp eaa6940c-a7ad-4bc9-be6d-b98e44c5a17e))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 081de8e0-6256-4756-93b0-d733bed4091c))
    (fp_line (start 1.75 14.45) (end -1.8 14.45) (layer "F.CrtYd") (width 0.05) (tstamp 8354d2fe-3d64-4507-960b-58c595a33701))
    (fp_line (start 1.75 -1.8) (end 1.75 14.45) (layer "F.CrtYd") (width 0.05) (tstamp a42fec27-ea7c-440f-bb39-75dc4a60a465))
    (fp_line (start -1.8 14.45) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b2cd85ab-949f-469c-907f-6e82a18ab8a9))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 34f8ff8e-433e-49e7-a14f-c669d70a17ab))
    (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp 72a0bf1d-5222-4ecb-8c04-19d4fd7fd864))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 86a0db0a-4cd5-4e42-971c-8eb8e53af3eb))
    (fp_line (start 1.27 -0.635) (end 1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp d9b72fbc-a8a0-4a79-be4f-fb50d8a14331))
    (fp_line (start -1.27 13.97) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f1fefc34-8732-4ecf-a21b-a2bafeec3a57))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp b687fa07-c96c-4dfe-88d9-a049d5829c21))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "Pin_2") (pintype "passive") (tstamp 0be210f7-6558-44fc-b57f-956eebc43f10))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/EINK_SEL") (pinfunction "Pin_3") (pintype "passive") (tstamp 9da3f5b3-b3ab-4652-bdd3-3dab0e5457f3))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/SCLK") (pinfunction "Pin_4") (pintype "passive") (tstamp 23b4eca1-2435-4d9e-b27f-f3ecbda92e65))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/MISO") (pinfunction "Pin_5") (pintype "passive") (tstamp 67fb0bb1-f8b4-49bb-bff9-6d2201ebef61))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/MOSI") (pinfunction "Pin_6") (pintype "passive") (tstamp aecbf2dd-6c05-462e-b1c7-f03615818dc2))
    (model "${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429) (tstamp 00000000-0000-0000-0000-000061fef75d)
    (at 63.5 33.02)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000670ca11c")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bdf2280b-4ec8-40a2-81b8-d625ac134a3a)
    )
    (fp_text value "KEY" (at 0 -2.54 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp e6ccd886-710f-4952-a5bc-fad58a2ea232)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f4c8e7d-6342-4dbe-a150-78f771ec0fcd)
    )
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 4256dabe-56a0-4ae0-a658-822e9b80381a))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 74607a4a-dedd-446f-b2c5-9b11205a15b6))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8edbd68f-8a8d-43be-bcc5-0817e4b70346))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp b2c1a84b-e47a-4e86-b02f-a04188d7b6a8))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp ed882da1-6b9b-4b7e-bfc9-090a38e88502))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp fd0ffb28-00f8-41b3-898a-f9c522678c6a))
    (fp_line (start 1.75 9.4) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 7695201e-3562-425e-b434-74f8305fe11e))
    (fp_line (start 1.75 -1.8) (end 1.75 9.4) (layer "F.CrtYd") (width 0.05) (tstamp a11cf41f-e4ed-4768-bec4-bcd4c711a2b6))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp e31b6cd0-e2fb-414d-9b6b-62045d8b1da2))
    (fp_line (start -1.8 9.4) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp ef06afe5-a679-4e12-a453-76f4768226a8))
    (fp_line (start -1.27 8.89) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 0d49dc06-80a2-44dc-93af-c131c838a7cb))
    (fp_line (start 1.27 -0.635) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 1c83caaf-fc97-4e43-988b-20c41760be68))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 733673fb-1c65-4b96-acc6-e5587c286613))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 74a2baea-4917-4dde-9bd0-09e204e331b2))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ee46ee75-74e5-456a-98d8-30c34615c7dc))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 414f590a-a6ee-430b-b559-4461324e7bd3))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/I2C_DATA") (pinfunction "Pin_2") (pintype "passive") (tstamp e1e9a77f-62f1-4710-a269-bf2c729a80d6))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/I2C_CLOCK") (pinfunction "Pin_3") (pintype "passive") (tstamp 819532b0-7f62-4a03-a2ff-591ff9251b90))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "Pin_4") (pintype "passive") (tstamp 8e3618d1-21e8-41e2-8f6d-e2a69cee67c3))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 00000000-0000-0000-0000-000061fef7d9)
    (at 68.58 33.02)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000065eca221")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fc2d9045-2bb1-49c7-b001-8b7218a5d95a)
    )
    (fp_text value "ROTARY" (at 0 -2.54 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp f994863b-9d52-46af-b8a0-bc4cc48fde44)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0f3775e-3de1-4636-a1e0-dd61fb196712)
    )
    (fp_line (start 1.33 1.27) (end 1.33 11.49) (layer "F.SilkS") (width 0.12) (tstamp 618f8279-0b3c-4f2d-ae2a-686b1b674c8c))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 8bce1125-f948-470c-9d73-d81c19e5098e))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp a8c96937-0466-44fe-8655-41bfe365e0ea))
    (fp_line (start -1.33 1.27) (end -1.33 11.49) (layer "F.SilkS") (width 0.12) (tstamp aa20df50-f64b-4858-8a3c-bf15bf8156e3))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp dadbba20-afae-48be-9c5a-ead00d6a20ab))
    (fp_line (start -1.33 11.49) (end 1.33 11.49) (layer "F.SilkS") (width 0.12) (tstamp dfd6729e-2e73-4537-b6ea-1255a00cd50f))
    (fp_line (start 1.75 11.9) (end -1.8 11.9) (layer "F.CrtYd") (width 0.05) (tstamp 1a9a7328-219d-4613-82ae-fb7a75958347))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 51130bc6-2d83-427b-9b6c-395564d691d6))
    (fp_line (start -1.8 11.9) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 97dd6a6e-fb01-47e2-82a9-cc110341a9c1))
    (fp_line (start 1.75 -1.8) (end 1.75 11.9) (layer "F.CrtYd") (width 0.05) (tstamp d795d519-56dc-4e92-8977-17ded04f0276))
    (fp_line (start 1.27 -0.635) (end 1.27 11.43) (layer "F.Fab") (width 0.1) (tstamp 4a97083c-31ff-4dca-b043-b78dee74b2e3))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 77dd66ea-bad5-4d9b-bf36-9bea0b2800a0))
    (fp_line (start -1.27 11.43) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 9917a9ca-bc68-49dc-b6ed-fb106bc17483))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp a5104a75-8cb6-4e93-b549-93aa7d799a3c))
    (fp_line (start 1.27 11.43) (end -1.27 11.43) (layer "F.Fab") (width 0.1) (tstamp a67e6f68-7330-44cf-b2dc-583b22bda3b3))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 27f7857e-dde2-46e8-8ad7-1b13c62ff900))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/I2C_DATA") (pinfunction "Pin_2") (pintype "passive") (tstamp 14106271-abb1-443d-b66d-2ea362c28b37))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/I2C_CLOCK") (pinfunction "Pin_3") (pintype "passive") (tstamp 938d4243-3735-4678-91c9-431e1c63f1b8))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "Pin_4") (pintype "passive") (tstamp 7b43765f-3bff-44f3-94f1-ad6abcfe54fc))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/INT") (pinfunction "Pin_5") (pintype "passive") (tstamp 6ff4c607-d95c-4b76-8acd-348cd106dd55))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429) (tstamp 00000000-0000-0000-0000-000061fef84a)
    (at 66.04 33.02)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000644cabdf")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5759dd25-9b98-4319-9da7-b52c80150cea)
    )
    (fp_text value "DISPLAY" (at 0 -2.54 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp d5413610-096c-4b93-a1d2-e85e12af6a9e)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7aa94d46-2396-4304-8f02-8d9c8916fd38)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 1aaa50ba-4d88-4df5-ad95-cd680d7420b1))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 415131fe-7a66-4f64-8c92-9b46c96375b1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 7fe675d0-7ea6-4586-b8dc-3892bb3bd198))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 82f91cba-af64-413d-9d68-c021f3573abc))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 89323af1-0af9-42b5-b371-06632d047ff4))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp cbcf0cff-6a85-416f-add7-e19192edf700))
    (fp_line (start -1.8 9.4) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp ab5cfa80-0f39-47df-9c7b-53452c948f73))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c92a1b3c-e542-4021-8941-38cb8c36233c))
    (fp_line (start 1.75 9.4) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp d87c0e99-86d9-4f7d-9185-7d9f76bcfacf))
    (fp_line (start 1.75 -1.8) (end 1.75 9.4) (layer "F.CrtYd") (width 0.05) (tstamp e7e642f8-26df-4de8-adbb-a03e2cf3d36c))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 2e54513d-74c4-48a2-969f-344010c9c678))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 60c0c77d-fe1d-4cfc-aed0-b71f5692fa42))
    (fp_line (start -1.27 8.89) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6a707ee9-777f-4149-b9f3-37cf102454f7))
    (fp_line (start 1.27 -0.635) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp d5a5ab7a-9a8c-4afe-bf54-1b6f0d114895))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp f0691e0e-4386-4dcb-985c-f6c63d1a67ab))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 98fa416a-d16b-4167-b54f-a9ab8fd62bc1))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/I2C_DATA") (pinfunction "Pin_2") (pintype "passive") (tstamp 3d1cd422-8a90-4ab4-8324-08c1f0082dfa))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/I2C_CLOCK") (pinfunction "Pin_3") (pintype "passive") (tstamp 63ad0261-9a4d-4a3c-8914-82d7f4343393))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "Pin_4") (pintype "passive") (tstamp 68bfe324-7507-4d93-a17a-c6e70acb32f5))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 00cefaff-e3f5-4759-a14c-ff07f5bc86d6)
    (at 149.86 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815bc3e")
    (attr through_hole)
    (fp_text reference "DKD53" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a79e9fcd-ed0a-461d-898e-b76d34de10f6)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b322d6be-0f25-4007-a18a-39bbe92f4bfd)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 719f702d-d7cc-422e-bc6b-ad1189bc9166)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3d78efc8-dbcc-47c2-aa6a-b6fb219fbe0c)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d01af9c4-31c3-4897-8955-3dc90557dd70)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 6e314c98-bc1d-499b-a017-628e9c71d343))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp b869b28d-fe09-4ea3-9854-0b0ee19e90ff))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 253dabdf-62b5-4c89-9f2d-352226238813))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b30c004d-769d-467a-a03f-6e90b6f3fcf1))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp bf152153-b04f-4685-b91b-77f09c77cb73))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e375fa3c-8d84-44cc-865d-840ea3e1a7c2))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp fa2bfde0-a692-478b-8a0f-dd0381fdf94e))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp ccee52c0-d80c-4824-8967-4cfed6009383))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 57df04bd-0e28-4b16-9eac-aa1e9707d9db))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(DKD53-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 0c7c55e5-56fb-4038-ab66-0617e4e65715))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 036fe0a3-a8f2-46e6-b0fe-195c089bac2c)
    (at 114.3 55.88)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062c1259b")
    (attr through_hole)
    (fp_text reference "JKD5" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c12e23f-6423-49d7-b43d-84644a3eac91)
    )
    (fp_text value "ROW5" (at 0 -5.08 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b051aa59-08b3-47f8-add7-81f81fdfdbc8)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f672dcf-1f56-4b2c-8e1d-04fec01031d6)
    )
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 01621a74-54fa-483f-8761-bd7404e4ddd7))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 19daa621-78d2-4808-bd49-0945d8507aee))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1dae24e0-0e41-484d-a07c-b801aff69381))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 3e2ddb60-fb87-40eb-9c9b-160a8d5325b7))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp bf110ca7-e871-4c59-ac0b-510f4304f5c2))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp d76e4458-f42b-429d-9bc3-ddc6ac2d0e74))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 1d119bf1-3814-4ed8-92e5-69ac28d93b36))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 38c69bdc-a635-4399-977d-0b3693479bd0))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 9aa89729-2ddb-4740-9886-30e3ead89577))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp d4c65cc9-f649-4e0f-baae-f5e830d4ca85))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 194786d1-50eb-4cf3-90fe-263aeacf0432))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 4a4f89ef-8886-43bc-b89f-76184a98734f))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 4c949792-1389-4b1a-9b70-236b6ec838e2))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp b610657a-eef8-4493-9fdc-7a2b3baad5f4))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp c4614116-4193-4686-ba27-dfddc856efdd))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 6629cc98-c5ce-4837-b139-3e591295784b))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 2448df7d-a377-4a5a-bee3-58e479b8da4e))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp fae49d69-5dc3-4f5f-84cd-d07e5e2d0041))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp a3fe9641-f7e2-4161-99d0-69fc2de4cf86))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 343d4240-ae68-4cfe-911f-cd40fbcae535))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 9b3a9f75-09a8-4aac-99ef-0b98f66c69e5))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 31276494-c870-48cd-881a-db3728dd6dfc))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 55798b22-2a23-4e49-adaa-084d23016643))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 039b722e-d5d5-4545-92c9-231fc931a43b)
    (at 160.02 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681573ea")
    (attr through_hole)
    (fp_text reference "DKD43" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 454ae0a3-100b-405e-9567-5a6f1b5ae7f2)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3810a67-1f2d-45fa-ba35-1b18108c5199)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 237a8c8c-f6f8-4945-a8c6-268c215c2de8)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9b89d09e-4326-488a-8143-ffd76f5389e4)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e080db25-255e-4505-a834-d43fb867ff9f)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp b9e355ca-4e33-4f92-97b2-56da34e69b07))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 44b10002-5154-43fb-954e-e91f7597f3fe))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 396c1b79-be0e-47ee-af34-9d937361aef2))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6b08448d-57ae-44ea-9643-11dbb0b7116e))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ab983b03-50ea-4dbf-a575-4cc1a3de6d64))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b744f976-26b5-4d38-885c-9c97e7169678))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 1a8293ae-be7a-4384-b841-a46f96f1cb38))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a82fa9e8-322e-47d1-8867-b2f2acc30624))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp a65deb8f-3e35-464e-ab77-63de68a1a559))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(DKD43-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a80bbea2-f754-4b85-b747-450c1893d58d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 0d3e03ea-bedd-4fc8-9a21-e4737705489b)
    (at 152.4 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814addf")
    (attr through_hole)
    (fp_text reference "DKD17" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 987288be-7e45-488e-b48c-35c64d7c96e9)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ff5647b4-5aae-44a6-88b2-a2b05de5d7f4)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7622133e-43c6-4dd5-8e1d-6143530d6ad7)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cecfbc4b-02cf-4fdd-bee8-791d6fb27b29)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d647df7e-e10f-42b0-8514-dc19cf1109d5)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp d37bfb75-bd8a-4739-9653-a5ad843e3a18))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2808de08-31ef-4c19-bc67-1af5b6b45cbf))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 12782127-339c-4406-9303-5a82171b61be))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4f8ff617-dafc-4dd1-808f-09412ebbc7df))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 509b8af9-7c0d-4ea7-b348-c849eb157ed4))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c5aee17f-03cd-4500-878e-68abdab21600))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp e3c03b8d-5486-46a8-9304-ed3d6ae8e798))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp c6d4963d-7b6e-4c29-a29f-41e4582fd978))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp bca8c2ed-67cf-4505-8cbf-33459ca2c5b4))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(DKD17-Pad2)") (pinfunction "A") (pintype "passive") (tstamp ff62eac5-2c12-4431-ae6e-6b3a176041f3))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 0ec7ecea-1eb7-446b-a8e3-cfbe4228889a)
    (at 30.48 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/94fdd15c-87b2-446c-b1e3-ea23bfcc286f")
    (attr through_hole)
    (fp_text reference "J28" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ae7b2497-1736-4aa7-9c92-c79b4a2ba12e)
    )
    (fp_text value "CLK" (at 2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e829b2e-79c1-4650-838f-977c7fbc34ca)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c40cd61-9106-4e87-8021-9529e806a4fa)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 451d1f81-9b2b-4af5-8728-d381ceb9fa2a))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 4fe6981b-b29c-4bff-8414-9cf327d56d31))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 725d4335-a8df-4de6-b22d-adf90c885ed7))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp ec24305a-fe45-40a8-bced-f8a7c12c6997))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp f502d467-1eea-4740-aa02-5ec768378ee2))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 0c6addf4-b6fc-4def-8466-3dfac9c38931))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 36f072da-5cf4-42b3-8b46-ce0a76085163))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 6557ea9e-c90e-4ed9-984e-32c4c2bf5b2d))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp b7b49d45-1872-42fc-a893-cfaa03379edd))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 30232234-b76c-4ef5-be01-5b9ed89bac9a))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 5301d788-3064-49ec-9a31-f5ee69083ef1))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 7280a6b6-2838-4619-9a09-170c1ee98a4b))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp d6e24b4e-e165-441b-92f7-0a67c0529c28))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "/Rotary Encoder/I2C_CLOCK_ROT") (pinfunction "Pin_1") (pintype "passive") (tstamp 823bdb72-b3da-47c7-8be1-d919cd2d99f3))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 11d3e685-7cd8-45d7-b177-6fa1a10d4678)
    (at 45.72 127 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/d62c8def-2104-48cb-be0b-4df1dbf1aeff")
    (attr through_hole)
    (fp_text reference "JK18" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b4d0789f-b3bc-4f20-b553-f82ad1608bfb)
    )
    (fp_text value "COL8" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9dd3ab7-1f4e-4e35-8e26-4299e8482a48)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56bad6ff-8fb1-4d5d-b4cb-6c86aee3caf9)
    )
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 384466e2-a59b-43b6-9008-39daddd02674))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 570dfa9a-e758-4617-bdcb-4f6a0d35c119))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 597f5069-63ad-4318-bbcf-9ce450d96e75))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp a1ded75d-f4e8-4687-99cf-aa06941360e5))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp c49ba7a3-f6d2-43d1-ae6a-ab1d698a6154))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp fca59a2a-3c15-4f92-a0c4-e51d86256ac3))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 2e1845aa-4170-421d-b1c2-b593d1b1ffb7))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 964e7b27-3b83-41fa-a349-ae79b4ba19ae))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp e0adf158-3e8e-439f-a7a8-389096a65fd1))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp fd5467f6-7838-4959-96e6-39785e31f9d4))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 1c4eb4ff-7576-401f-befd-e02f81778daf))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 287fc25f-8880-4e37-b84f-e56cfaca9b5b))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 57d862fb-b97a-4294-8ee6-e0c4c02546b1))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp a612b906-e840-4e52-865a-2fb7b60b23b8))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp ab576e45-f81f-4202-85e2-3e8a7b52482d))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 7983748a-b0b7-4e76-ab65-1dd7d7b22204))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 437f4763-eff7-41fb-aac6-3917ee011cb0))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp a0755c88-c86f-46f8-86f5-7ebffda3aaf7))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp b3d9ba28-fa2e-4105-8c13-85a2d7dc3746))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 4b3df2bd-6122-4d77-9431-2f7de7159c30))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 741963cb-a892-47d0-aceb-af393112160b))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp b59802bf-011b-413e-be68-ba5e3aebb98b))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp e860b77a-1b5f-445f-ad54-53809659f0ae))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 1236c0e8-97a3-46b1-8328-161b8c54d0a2)
    (at 185.42 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815faac")
    (attr through_hole)
    (fp_text reference "DKD60" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5eb6389b-df51-4291-9a53-c86c8dcbda62)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e468a41d-3b06-4fdf-ab79-7d5c88b6cb08)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp baad0c05-c48f-4f29-b351-332cbd3bd9ca)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c9f7f382-47eb-4080-8a09-a1f2aa4430a0)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f94e71d5-7f47-445c-9531-9a8f92f61f72)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp a8244529-0db1-4fb8-8b3a-97d4f336226f))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 6028e8a6-282d-4105-927b-92298fd905df))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4be2ee3a-66b8-4b1e-a159-5f29cbe0a68e))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c0d959dd-7e25-472f-a53d-314bc381fe26))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e533f2ae-38a4-4f66-a1f9-827cd1a98fdf))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp f6e8bded-99b0-4ced-8cd5-31816bac0125))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 3ace10ea-92f2-44b4-859d-d6505e7bfb54))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 63502fd4-bbe9-44ac-aa90-2210115f19c0))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp ad44cc16-f615-412f-9f59-a45c461877bb))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 146 "Net-(DKD60-Pad2)") (pinfunction "A") (pintype "passive") (tstamp f244901d-8414-47de-a4ad-8e9e85281bee))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 148d4173-b063-4b10-8a8d-efdde1f30322)
    (at 50.8 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/f1e08948-6b85-492c-99de-5fd6a459b81f")
    (attr through_hole)
    (fp_text reference "J9" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d5b3e10-9b65-4abf-803e-969a546fc8e3)
    )
    (fp_text value "B1" (at -0.025 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 18648368-8315-41f6-b287-55706b48f79e)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 69814d9b-0367-4de8-9718-43b37031d240)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 3bb6370c-713d-4d7f-8232-809c9ec621ba))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 5b17d47a-a4a2-4ddf-966a-e6b5821094ec))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 69b9c43b-f07d-440f-a8c0-3e74d8fe8255))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp a4016004-dc80-4dea-8e6b-d39f67a11e91))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp facfc131-66c7-4b5b-b59f-7d81e0c94438))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 5880b9b0-aa32-4505-8669-deb95429be37))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8eb5e770-d904-422f-814b-21543d34976a))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp c8fb0e8c-a702-4abf-8afe-bedb64abe0e1))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp de9814ea-c668-40c7-a581-41a00d5ad413))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 13ca6f98-495b-4848-a1b9-619bdbf2e008))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 207f3729-b16f-4bed-8e25-6323ca6af59d))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 3969f1a4-cee5-45d1-af73-48102fab1b79))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp c7f16784-da95-4ab7-905d-9889694975ee))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 78 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp abdf1fc0-a5f4-4a26-adc8-ba7216defb10))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5) (tstamp 149894f6-4705-4c0d-a25a-682eb998df21)
    (at 127 35.56)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000061fa6e27")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ad61c07-c85d-4b5a-899e-080b1d5d6cdc)
    )
    (fp_text value "MCP23017_SP" (at 3.81 12.7 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5faac71f-00d9-4b26-9c27-73a01f65a371)
    )
    (fp_text user "${REFERENCE}" (at 3.81 16.51) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2bb16b2-b755-4605-9ac7-1e3b03e15a8d)
    )
    (fp_line (start 1.16 34.35) (end 6.46 34.35) (layer "F.SilkS") (width 0.12) (tstamp 3f11811f-8989-4913-a5b8-518dd7a09213))
    (fp_line (start 6.46 34.35) (end 6.46 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 49aaa0e3-ace0-4771-98f6-7907477f70af))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 508deff8-3d88-4357-b564-0964d1a3d64e))
    (fp_line (start 1.16 -1.33) (end 1.16 34.35) (layer "F.SilkS") (width 0.12) (tstamp 68075478-1191-4daa-a1b1-4b4fdf1b0d7d))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp b4a704db-6997-4b22-8553-52651d118f39))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 6bd75102-2811-4c96-a4f6-d67acf2b2e3e))
    (fp_line (start -1.1 34.55) (end 8.7 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 066b37af-91d5-41af-8aa2-34d6eb789fe4))
    (fp_line (start -1.1 -1.55) (end -1.1 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 863294ae-f8a6-4b1c-80da-1717c4fbb39e))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp a00edde9-316a-444c-8d44-cc9f9b0f5218))
    (fp_line (start 8.7 34.55) (end 8.7 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp a7f3da0b-1f94-4fa6-86b2-c380bd5f8c49))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer "F.Fab") (width 0.1) (tstamp 0c868194-2f51-460b-b653-ee4c98450f64))
    (fp_line (start 0.635 34.29) (end 0.635 -0.27) (layer "F.Fab") (width 0.1) (tstamp 43e7b497-8c30-490c-8e81-2728c68bb079))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ac584619-8e0a-4cc7-8bb5-65dfe53fa21b))
    (fp_line (start 6.985 34.29) (end 0.635 34.29) (layer "F.Fab") (width 0.1) (tstamp baa3e5cb-3f3d-4329-8413-5ed4cd162f17))
    (fp_line (start 6.985 -1.27) (end 6.985 34.29) (layer "F.Fab") (width 0.1) (tstamp f79173c9-b1ae-4472-8758-b3907321e3cc))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "GPB0") (pintype "bidirectional") (tstamp 35a80dab-f6fd-4c43-9987-30228bac2f3f))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "GPB1") (pintype "bidirectional") (tstamp 6dc6287f-b51a-480e-a237-29dad274c2fe))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "GPB2") (pintype "bidirectional") (tstamp 16c1ddb9-7eb4-45ce-a848-907cf6d2057d))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "GPB3") (pintype "bidirectional") (tstamp 3085f617-b99c-4346-9d5e-5033592882c2))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(JKD5-Pad1)") (pinfunction "GPB4") (pintype "bidirectional") (tstamp 9613bd7e-7ed6-410e-88e0-aceafb5d29a6))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "GPB5") (pintype "bidirectional") (tstamp e09684bf-405f-4c92-9ae5-a580cfff7785))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "GPB6") (pintype "bidirectional") (tstamp 396d5ba8-6fe1-4451-9f11-eb79baa806fc))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "GPB7") (pintype "bidirectional") (tstamp 0658036b-aa6f-4498-8457-b95b919e8f6d))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "/Key Matrix Diode/+5V_KEY") (pinfunction "VDD") (pintype "power_in") (tstamp 6b9fba57-1553-4c2e-b07a-e84c4bfe6281))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "/Key Matrix Diode/GND_KEY") (pinfunction "VSS") (pintype "power_in") (tstamp 72c9bb2c-2d7c-4fad-9554-a29fb43a957c))
    (pad "11" thru_hole oval locked (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "unconnected-(U2-Pad11)") (pinfunction "NC") (pintype "no_connect") (tstamp dbca5e9c-048f-47f2-8e3c-8c89fe7d077a))
    (pad "12" thru_hole oval locked (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "/Key Matrix Diode/I2C_CLOCK_KEY") (pinfunction "SCK") (pintype "input") (tstamp 5d9753b8-97df-4b4b-b0a5-e0b3b215d7bd))
    (pad "13" thru_hole oval locked (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "/Key Matrix Diode/I2C_DATA_KEY") (pinfunction "SDA") (pintype "bidirectional") (tstamp 4c56e9b2-83ce-4cc2-ac25-7f4c3288ffe3))
    (pad "14" thru_hole oval locked (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "unconnected-(U2-Pad14)") (pinfunction "NC") (pintype "no_connect") (tstamp 92ace8e5-0b10-41e5-ae56-7770183deaf4))
    (pad "15" thru_hole oval locked (at 7.62 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "/Key Matrix Diode/GND_KEY") (pinfunction "A0") (pintype "input") (tstamp 5a04a1fa-a52a-468e-9c62-f093821b6c12))
    (pad "16" thru_hole oval locked (at 7.62 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "/Key Matrix Diode/GND_KEY") (pinfunction "A1") (pintype "input") (tstamp 4b604d2b-ca9f-4a55-b07a-f94ef9915e36))
    (pad "17" thru_hole oval locked (at 7.62 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "/Key Matrix Diode/GND_KEY") (pinfunction "A2") (pintype "input") (tstamp 68c9e55a-8f80-4870-840b-3b76128e81a7))
    (pad "18" thru_hole oval locked (at 7.62 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "/Key Matrix Diode/+5V_KEY") (pinfunction "~{RESET}") (pintype "input") (tstamp 2dbabf52-d8ed-453e-bf49-462ab4f52c22))
    (pad "19" thru_hole oval locked (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "unconnected-(U2-Pad19)") (pinfunction "INTB") (pintype "tri_state+no_connect") (tstamp 5fc275bb-e815-4e34-b9ad-c4fb779855ce))
    (pad "20" thru_hole oval locked (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "unconnected-(U2-Pad20)") (pinfunction "INTA") (pintype "tri_state+no_connect") (tstamp 36e44255-d72f-4f65-be9c-54b3a22f0a40))
    (pad "21" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "GPA0") (pintype "bidirectional") (tstamp 5985fd17-7dd3-4a22-9ad0-9fa2144b8a03))
    (pad "22" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "GPA1") (pintype "bidirectional") (tstamp e6265768-7626-4f88-b4bb-91a055fc78c7))
    (pad "23" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "GPA2") (pintype "bidirectional") (tstamp 0f863a3f-3194-4d0c-bf1b-b0fb684d962f))
    (pad "24" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "GPA3") (pintype "bidirectional") (tstamp a049cb43-6b1c-45ea-9a7a-5d0075ef0f38))
    (pad "25" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "GPA4") (pintype "bidirectional") (tstamp ecc45fd0-b7df-4930-8915-6b6956bde144))
    (pad "26" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "GPA5") (pintype "bidirectional") (tstamp 912da118-d7f3-4870-a859-e57c3f9b4e67))
    (pad "27" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "GPA6") (pintype "bidirectional") (tstamp 8610eade-c06f-4cd7-be4a-0353060797ae))
    (pad "28" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "GPA7") (pintype "bidirectional") (tstamp 6778998e-4c72-454a-b4a3-607e68871b12))
    (model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 1787e360-829c-4743-a274-84e89a86760b)
    (at 121.92 25.4 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062e52375")
    (attr through_hole)
    (fp_text reference "JD4" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ef96cd0-8f4c-41a8-8745-09e5363ae470)
    )
    (fp_text value "ROW4" (at 0 22.86 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b1882ce2-92e5-4e01-967f-ad7f271007d8)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0ab7792-62f2-4703-8754-78d54487de80)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 054e7206-b17c-48a4-8dca-a09be19d89e0))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 558485cf-53f3-4a12-a729-9f77427c9fd0))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 5982d8eb-b62b-4278-995d-1eea1045161f))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp eb6dd49c-058a-4a06-b6e6-8755a8706e8e))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp ee9d2bb2-8f21-47fc-9cea-08f3298af1cf))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp f4aa4de0-4dd1-4ec5-bfc8-8007195c1dd8))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 1d5f7371-bf61-46f6-b5d2-9ed51907ffd8))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 35f14986-84e9-4b8d-b93e-05dae5309d93))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 7557da72-f6db-4d3a-b7ea-fdc95d6b0ce9))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp dc731b9e-4511-4eb7-a4ae-2f9a9f3ce6b9))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 25adc9de-3070-41c0-a864-ea3459924e5f))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 6475a1e6-8bd5-44d3-bfd0-320d530e7f43))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 7d78c052-1098-4580-a98d-3043091cab4e))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 87920ab4-7187-4bb7-bacf-d67d9fa1dccf))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp dfb36977-98ef-40b5-824c-697cbf9bf5e9))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 511dc211-4659-4ddd-847a-92439f170b81))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 558a2967-ab1f-40c9-b839-e5f63277d716))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp a931768f-d8eb-41b4-84e4-dc61a04bc969))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp ec917dee-6566-48a1-b894-894637f4d5f1))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 218d9a3e-f745-4c85-a48a-048bc673334c))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 9a81dedb-565b-452a-ba3c-c88a277ddb29))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp f52b1f62-298b-436a-91f0-744e788359a6))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(JD4-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 30c8d1c7-c0c1-4fc8-a0fa-dcbf10e17372))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 188bd81e-55cf-4eb8-ac51-32c0165c3b7f)
    (at 48.26 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/355984fe-c4ef-4584-9c88-7aed9a4b1db8")
    (attr through_hole)
    (fp_text reference "J10" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cb625889-a39e-48a1-b5ca-64b654415724)
    )
    (fp_text value "A2" (at -0.025 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f8398d1-1fcb-4b17-b71c-c5df98433848)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 253438e1-b2d5-45c8-bcfc-742c8344ecea)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 0bc4a849-5f93-40a7-8f00-efd98ea94086))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 20b6f547-8f23-4ca0-8198-b15b71fba76d))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 95576a76-91bb-4db4-bcad-45ffa1fb7580))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 9c614a92-4db0-4682-b200-e8121deaa926))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp ce1871bd-0dbe-421e-af45-ef8b1716fbf2))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 102c4f15-f7f0-47b3-b463-90324a621426))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp d92a0282-1577-4ce4-be7e-0b4d890f47ad))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp dc2f95e5-e18b-4da3-b935-6bac0924cb34))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp deb67a9b-326e-4e7c-9ffe-380d8b743b4a))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 0f8c7f8e-c569-41d5-a9c5-be2602986fec))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 2a3045fd-49b2-4e17-94bf-b5864659b054))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 422c943d-0851-47e8-8fa0-a7c617f12578))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp e6c57be4-076b-4791-b5f7-950dec1eba7d))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 99 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp fbc71af7-de54-4238-9761-e2dd07bc84ed))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 191475d3-9362-42bc-8055-82669e94bcd9)
    (at 27.94 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/4562bbed-1cf5-48d3-8b27-4accd2fdf26c")
    (attr through_hole)
    (fp_text reference "J47" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f9f3f60-56a1-45cf-882f-50aaebfa09cb)
    )
    (fp_text value "DATA" (at -2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4d1b2393-824a-499b-a95f-2075bb4b4583)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c03df382-5cbe-4fcd-950a-f61491833ee4)
    )
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 12c13ea8-2139-4fe5-ba69-406b77e8074b))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 6685bc04-b56a-4eaa-9536-e9db5e23803c))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 8502e297-d4a6-4d0e-94de-15fa33cfb187))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 8755f4c6-2784-4bcd-ac51-f52ffbf56b7a))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp acda603d-d9d1-48db-bfba-528d53cbad4d))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 5ef62951-7280-429e-9e7c-900f1d4e2e62))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp a3f19e3e-ad93-4f99-b053-425bd0781702))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp b1350e58-ab13-4b6f-b458-5c9b665953a0))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp d11a93ee-bbc5-47df-b420-3dc32c01aa6b))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 0a5849e2-6070-4fe2-9b63-a7e959741eb3))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 0f2e9923-80f5-4cf4-833f-1a6fa7fed589))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 12bbc2b2-5bac-413d-a185-45f0b0010405))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp c60f863c-7626-4df3-8cef-7c2d084b634b))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 186 "/KeyMatrix wired/I2C_DATA_KEY") (pinfunction "Pin_1") (pintype "passive") (tstamp 76505e0f-c9fd-4712-acff-3f53e6a70db8))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 19550ef8-e46a-41a3-b33c-7bafbbd02474)
    (at 53.34 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/e203d836-01b9-4742-95b0-b818b8d5ad1d")
    (attr through_hole)
    (fp_text reference "J43" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a8bc2b00-f952-401e-bdbb-23fdb63a0fbd)
    )
    (fp_text value "C5" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28b9b428-cba2-4b43-bbef-20f7c140ab5b)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 17c9c32b-822d-40a3-bf45-1a05c9f42d6f)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 21584ec6-80e5-4dd6-ba7d-50a1a21763eb))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 660b79fd-0c3e-4fcd-9ea5-eb3a6f080691))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp d0e5cb06-b4ca-4f44-97ec-26352abfdc84))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp d4258bcb-b075-46b2-9a52-dc9c21a8da12))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp e53aeee7-3e42-43bf-864e-ced55aaf1e15))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 630dd9b0-cb67-4fac-b74e-117bc032e9a7))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8438854e-39ec-4b1b-bc8e-daf8fba9160d))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp d5170e75-d9bc-49e3-bd92-f94f596ffa01))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp f6173929-82fe-4f42-a09f-38683d840ce0))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 2ed7eb1a-7e7e-4013-a754-41fc54eb2207))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 7978c4a0-cf66-4cf0-8ba1-e6609225f7d5))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 7b850855-a177-4b2f-8e3e-e7958232dc46))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 7bf1e578-3c95-4f34-91af-bb8faa5d187b))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 182 "Net-(J43-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 7e725ec7-da05-4975-a58d-fd6af4f65ab0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 19f4b8b4-be0c-4288-abe5-c17502fc672f)
    (at 40.64 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/0e20cbc1-6cd0-4252-8a14-c1d9146f2a63")
    (attr through_hole)
    (fp_text reference "J14" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2e16797-bb9c-43d0-8751-7646864e22e4)
    )
    (fp_text value "A4" (at -0.025 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 73eb1d6b-3e2d-4317-bc4c-c77f232aa2cf)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d64a0a0-384d-4e31-a03a-22264a524862)
    )
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 0aadf54d-dacf-4007-aabb-7ac26ba5bd37))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 96fd148c-2abd-4da2-a739-1fc716e496e9))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp af925654-dfb9-45aa-816e-cb4703dcab2f))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp e07d5869-f4e0-43a4-8e08-83daa6e67700))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp f8d4ba33-e493-4c36-93a3-a7a967fd6532))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 6383d51c-2a4a-451b-80f6-d8ddd181fcca))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 997ebd3b-fb52-489d-905e-2a7aae5bd517))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp f0d57cc9-c4de-4eb8-97e9-9df19eea248e))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp f2ae85d9-7640-48a3-83c4-8d4b3e89cde3))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 2536e930-06a4-43c1-bb06-fbe9f6f63e41))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 26d0960c-3dad-40b7-9ad0-2a8d7207d84f))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 75b57470-3933-4be6-8842-b2898714961d))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp c030dc50-5966-4aad-8d18-d61b053ef0ce))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 151 "Net-(J14-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp a4ac0519-b7a7-4509-bdb5-35a62928ff28))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 1a2d78e0-24f8-46e2-ae75-c9d7f0a8588a)
    (at 180.34 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681579ac")
    (attr through_hole)
    (fp_text reference "DKD44" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c641ac9e-2a1a-4e58-a1b6-3187057f4439)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b0bb866-f07b-417e-be71-9ecb8f9d8b97)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53390312-51ab-451f-8a21-100f127845eb)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 54b72cbe-e485-4587-9972-a5fd09d6781b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5cba886a-9661-4668-a71e-26b275c4304d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp c5ef6875-2ca2-4de3-903c-7d74aae072dd))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 554f07fa-d397-496d-b24d-67d978b548ff))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 20693eea-11f9-43d2-9455-8c165c10ae1c))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 466a90b3-da22-4b44-a493-b04373d5b366))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b8af2efb-5cb8-41b6-af55-4223ec44e1b6))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f96adb8b-f381-4fab-a5c9-ee8ba31dbc0a))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 2d124462-7aa7-493a-ac87-a244d2a873ab))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 83243eb0-ad5c-4511-aec4-efae644dbc5f))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp ff42e85a-2cb6-4b82-9134-e1e563b2b716))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(DKD44-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 13e5ae2c-e154-4a21-bfbd-cc4cc4e2f4e4))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 1b918202-cf42-4316-9f7f-988f6edf3e52)
    (at 35.56 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/73bcbbc6-a043-409a-ab80-98753b715cbc")
    (attr through_hole)
    (fp_text reference "J46" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da0ea1c1-a5a9-456f-9369-2ce567f94fd7)
    )
    (fp_text value "GND" (at 2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 57b151cd-d89c-4ab0-a769-6fbf25582c46)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1ccb051-bd30-48f3-a274-f42c42af90ac)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 7ae91763-f0a3-4a18-9244-057e21c36da7))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 988a9d07-287a-47a6-ac01-bd1183623825))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp bfdaae07-969c-474d-a54f-6c5708462e18))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp f2f97b90-1e01-417d-8af1-5f9ccbd88198))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp fe1fe3b5-7b4a-4bf7-9e7b-c7ee2c49c6a7))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 3ac835f3-d4e4-4445-ba04-2bf1d0eb5b0a))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 3fac69f1-dea4-4f51-b564-c4698dd0f72b))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp a7191198-7722-4775-b3ba-0abe4075cbbf))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp db0b6b1e-09b5-4ca4-b3e6-08db2298b56d))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 1d2a7927-5e2c-4248-91b5-e3b3b59f7d68))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 7dc8e40d-760c-4c3c-b38c-d861f2b29eeb))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp ed18d5df-e63b-420f-bcda-7083503b3cb4))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp f15e333d-3b52-441b-a356-bb51801e8787))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 185 "/KeyMatrix wired/GND_KEY") (pinfunction "Pin_1") (pintype "passive") (tstamp 8c4a4a48-0e00-4f86-ae38-eaf2e71cf328))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 1d4761aa-9671-49ea-8557-6ea9c5e81570)
    (at 180.34 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814ccfb")
    (attr through_hole)
    (fp_text reference "DKD22" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f3ee3523-8667-4ba0-b948-2c663b200944)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92e44473-7059-4dfd-85d8-7cfd72233c53)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 099c84df-d13a-4c42-beb1-ebc61288bdee)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2dd59b27-1513-4af2-a9ad-ff5220259cd0)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6e098f6-36bd-47bd-a72c-0a07b1906dad)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp e3c6a7c6-eb14-400a-bd45-746bd33a132b))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 55bf6d07-9c10-491d-9f49-29b2951b4dc0))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0214d576-66ee-46aa-bc69-772834d2ddea))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 05a29ab3-189b-4b70-a61b-5273c2c80bb5))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 23e98799-140c-4a5e-afe3-9b624bcd1119))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5f1a56d3-ed6d-4ca6-a008-efbdac068efa))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 3bea7816-7872-46e2-8896-cd1572c6fc3f))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 9ecf1598-57c9-4029-a7b4-33bb6b495508))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp b05a5f16-d043-4ad4-ab83-b4f28809975a))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(DKD22-Pad2)") (pinfunction "A") (pintype "passive") (tstamp f510f93f-0b8f-42df-8cd8-3766c11be82d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 1defacb9-7bca-41a0-b362-3566a384c9da)
    (at 33.02 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/3e7d3ba7-4edd-4535-8c09-fa92c51dc657")
    (attr through_hole)
    (fp_text reference "J25" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c999cd9-380c-4645-8e1d-cd50e73f1aac)
    )
    (fp_text value "+5V" (at 1.905 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e686dc0d-0ddd-4a59-bb4f-909d83897018)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c325042c-ee47-47aa-a96f-84bfc4126fe3)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 5c8796ed-0e8d-4e5f-93fc-1864b7d6f7db))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 78bf525d-6cdf-4984-886a-d31a70711d20))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 89eb91c5-88d4-4e27-88ac-997a5f812226))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 9c8a7bd4-517b-4df8-b522-fb906de1e6a1))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp bd949d1e-3838-40ce-8338-e3416dbddf44))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 3749553d-b3f1-4f21-8fbf-1adb20d44f9a))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 535e3851-ef11-46ba-8e69-ed6f2448d191))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8841214d-dd0e-4d87-bdf6-f5358a0d764c))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp fdbec5e1-e74d-42d1-a15f-9870270449de))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 1053723d-f511-40f1-ae40-bf7ef45b9a90))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 26e7e72a-a079-4605-93e8-56ec5e0640a7))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 2f1ebd2b-d08b-4301-aae2-f6ef217f6430))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 4832ec94-33d2-491a-987b-7def90eed38f))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "/Rotary Encoder/+5V_ROT") (pinfunction "Pin_1") (pintype "passive") (tstamp 0abd9d53-e15b-46ed-a9e6-cb5a12201568))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 1ee5bda6-1e63-4580-bf44-1e1ac78dcc5a)
    (at 55.88 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/fe4436c3-ec9b-4d4d-9a37-5d16547a866e")
    (attr through_hole)
    (fp_text reference "J31" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c99cbbbc-39b6-4e4e-847a-487ed1ae9373)
    )
    (fp_text value "R1" (at -0.025 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa0cb989-8034-4a44-b66d-98e61fe3c111)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f24f62cf-f376-444b-928f-063a73c7f3a2)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 0c23c2d1-f7c2-49e2-834a-dcfca9f547ee))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 9d036c59-af68-4c67-9096-2592d799fbad))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp c949f750-102a-4c7b-b53e-b6cc5b3764f7))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp e2b09f57-323f-43df-916c-056852033c09))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp eaf332d5-4a73-4573-bc6a-06cddac4c0fd))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 069e5de6-1cde-4527-9f46-9f0bf11d264c))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 27c7a05d-2c40-403c-be35-4c66d5a163f9))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 71ef1232-a6f0-48e5-9f2a-77fdefaf4936))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 847be3b5-d4f9-4ba1-8294-b52cfec08f1f))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 032a366d-27c2-40c1-9dd9-fe2bc83646fd))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 4aaadb93-4e8b-47b6-9fe2-addc1ece0151))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 50c45063-68cb-4e92-ac5c-fe3d1a5bee40))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp eff2af4c-95ed-4349-acb5-6b2d58c2cdd4))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 170 "Net-(J31-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 9538bd59-c6ed-4dbf-b450-0b1418ad25a9))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5) (tstamp 1f8f0787-dbcd-4c4c-ae4e-90128558bde4)
    (at 58.42 27.94 -90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/00000000-0000-0000-0000-000061fb92a8")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bcd8a653-fe5d-4b14-ba75-93cc9e8b15ef)
    )
    (fp_text value "MCP23017_SP" (at 3.81 12.7 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 089ce730-0424-478b-b4cc-105f9b59b8c9)
    )
    (fp_text user "${REFERENCE}" (at 3.81 16.51 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b17ae402-ae49-4ceb-bf50-99a7d1dce2e2)
    )
    (fp_line (start 6.46 34.35) (end 6.46 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 0346a1b7-20d8-479d-9a2d-685e2da6923d))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 1ffa0a97-e975-4d93-aba3-7682c83b2b27))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 2e4f1eed-ee3b-4746-be02-bf45ccbc88a8))
    (fp_line (start 1.16 -1.33) (end 1.16 34.35) (layer "F.SilkS") (width 0.12) (tstamp 6f7f791c-dffa-4d1e-a6a2-9e45e850e80e))
    (fp_line (start 1.16 34.35) (end 6.46 34.35) (layer "F.SilkS") (width 0.12) (tstamp b2846506-fee6-4170-a1a0-1a30ef3bb66e))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8d34ec17-af2a-4532-94ec-9b774cb37ee4))
    (fp_line (start 8.7 34.55) (end 8.7 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp 31469f38-094e-49fd-8d31-f1f1d2def3b6))
    (fp_line (start -1.1 34.55) (end 8.7 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 36280559-4de9-47fb-843f-86081cd88eac))
    (fp_line (start -1.1 -1.55) (end -1.1 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 972396fd-0c0d-4f60-9da6-708a690c1a35))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp c22607d0-7889-41e6-8948-1b6ab2bc79f7))
    (fp_line (start 6.985 -1.27) (end 6.985 34.29) (layer "F.Fab") (width 0.1) (tstamp 134859a2-15aa-4565-b1e7-26feea15069d))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer "F.Fab") (width 0.1) (tstamp a290c21c-f63c-4ebe-ba57-a2db6d9ba53e))
    (fp_line (start 6.985 34.29) (end 0.635 34.29) (layer "F.Fab") (width 0.1) (tstamp c31cafdf-cc1c-42b0-9cff-cf31c774e86c))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp d9bec634-1b16-439c-a985-65cd482f5936))
    (fp_line (start 0.635 34.29) (end 0.635 -0.27) (layer "F.Fab") (width 0.1) (tstamp dfde2c1f-f7e6-4285-b15a-032861861e78))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J6-Pad1)") (pinfunction "GPB0") (pintype "bidirectional") (tstamp c304bd06-f71a-4015-993a-83226725abbc))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(J7-Pad1)") (pinfunction "GPB1") (pintype "bidirectional") (tstamp 190e81ff-73b6-42d6-a044-3de60c68b533))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(J8-Pad1)") (pinfunction "GPB2") (pintype "bidirectional") (tstamp db815b65-2e01-4e79-b0a4-f722f7ccdb56))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(J9-Pad1)") (pinfunction "GPB3") (pintype "bidirectional") (tstamp f9bb7c0d-144c-4477-8c1e-c4f03702b4f0))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "Net-(J10-Pad1)") (pinfunction "GPB4") (pintype "bidirectional") (tstamp 295ccbca-ec52-4627-8aa8-4f65fecc5ccc))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 "Net-(J11-Pad1)") (pinfunction "GPB5") (pintype "bidirectional") (tstamp 079e7ee5-246f-4d56-830e-c74c7f0ff0bc))
    (pad "7" thru_hole oval locked (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Net-(J12-Pad1)") (pinfunction "GPB6") (pintype "bidirectional") (tstamp 24a1cdab-c9ce-4136-88e4-ae4c940e4508))
    (pad "8" thru_hole oval locked (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(J13-Pad1)") (pinfunction "GPB7") (pintype "bidirectional") (tstamp daab4222-f234-406f-9856-d8d7ea988c8e))
    (pad "9" thru_hole oval locked (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "/Rotary Encoder/+5V_ROT") (pinfunction "VDD") (pintype "power_in") (tstamp e4688208-e370-4724-b274-e25b1b91f0ae))
    (pad "10" thru_hole oval locked (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "/Rotary Encoder/GND_ROT") (pinfunction "VSS") (pintype "power_in") (tstamp c818e01e-938e-49cd-9425-bdf6b2c272b6))
    (pad "11" thru_hole oval locked (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U3-Pad11)") (pinfunction "NC") (pintype "no_connect") (tstamp 4d5a8408-8e4c-489e-b002-657730ecf6e2))
    (pad "12" thru_hole oval locked (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "/Rotary Encoder/I2C_CLOCK_ROT") (pinfunction "SCK") (pintype "input") (tstamp b32acaea-cd47-4a73-a0c1-373d519f4021))
    (pad "13" thru_hole oval locked (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "/Rotary Encoder/I2C_DATA_ROT") (pinfunction "SDA") (pintype "bidirectional") (tstamp a9808457-1913-4e14-a8bc-bbb85854f337))
    (pad "14" thru_hole oval locked (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U3-Pad14)") (pinfunction "NC") (pintype "no_connect") (tstamp 3db1dfcb-b205-42e6-aab9-289056c3f809))
    (pad "15" thru_hole oval locked (at 7.62 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "/Rotary Encoder/+5V_ROT") (pinfunction "A0") (pintype "input") (tstamp 8becf175-9d14-4edb-bd98-0f6b8dfa7f29))
    (pad "16" thru_hole oval locked (at 7.62 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "/Rotary Encoder/GND_ROT") (pinfunction "A1") (pintype "input") (tstamp f9e43d95-038e-4c2c-993c-6421e6b482ef))
    (pad "17" thru_hole oval locked (at 7.62 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "/Rotary Encoder/GND_ROT") (pinfunction "A2") (pintype "input") (tstamp 1482851c-2e17-4260-a1eb-f2555c4a7bdd))
    (pad "18" thru_hole oval locked (at 7.62 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "/Rotary Encoder/+5V_ROT") (pinfunction "~{RESET}") (pintype "input") (tstamp 1ef3510d-b6f3-404a-aeb6-d68acdbffe02))
    (pad "19" thru_hole oval locked (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U3-Pad19)") (pinfunction "INTB") (pintype "tri_state+no_connect") (tstamp 4f137560-fd15-43b1-8f79-c87161dbfb06))
    (pad "20" thru_hole oval locked (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "/Rotary Encoder/INT_ROT") (pinfunction "INTA") (pintype "tri_state") (tstamp df4a707f-c422-45b9-846e-5f8beda1b995))
    (pad "21" thru_hole oval locked (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 151 "Net-(J14-Pad1)") (pinfunction "GPA0") (pintype "bidirectional") (tstamp b4d2c23a-7cc4-45c9-8b80-2fac4ca991f3))
    (pad "22" thru_hole oval locked (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 152 "Net-(J15-Pad1)") (pinfunction "GPA1") (pintype "bidirectional") (tstamp 7dc2d1f0-9853-41c5-82ef-3e8bfad85b15))
    (pad "23" thru_hole oval locked (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 153 "Net-(J16-Pad1)") (pinfunction "GPA2") (pintype "bidirectional") (tstamp a835fe7e-5fe3-4753-8be0-85264176b5b1))
    (pad "24" thru_hole oval locked (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(J17-Pad1)") (pinfunction "GPA3") (pintype "bidirectional") (tstamp c217cc02-b8ca-45cd-9e37-ba17e558e20b))
    (pad "25" thru_hole oval locked (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(J18-Pad1)") (pinfunction "GPA4") (pintype "bidirectional") (tstamp cfadeddf-442b-4347-ae7a-f19df8b9afb9))
    (pad "26" thru_hole oval locked (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 156 "Net-(J19-Pad1)") (pinfunction "GPA5") (pintype "bidirectional") (tstamp 45dd312a-4854-4626-ae8a-71a3ad2284b7))
    (pad "27" thru_hole oval locked (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 157 "Net-(J20-Pad1)") (pinfunction "GPA6") (pintype "bidirectional") (tstamp e4504463-45b2-469f-ba7e-89cbf4245f8e))
    (pad "28" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 158 "Net-(J23-Pad1)") (pinfunction "GPA7") (pintype "bidirectional") (tstamp 22e36685-b889-4540-8920-0f092b032b4f))
    (model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 1fbed9e5-7de0-4ce9-9c55-ad7572e12e59)
    (at 81.28 121.92 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/09a83b1d-03d4-4819-9c4b-c384e604fd5a")
    (attr through_hole)
    (fp_text reference "JK3" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 95dd0dcc-e6ba-4cb9-9a88-76b380c1434c)
    )
    (fp_text value "ROW3" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78fa9d0a-b319-40f5-af5c-9b67602adf03)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fb94971b-230a-497e-9daf-e8f08c0c2223)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 0862bd5e-0ac6-4e9b-be9a-956136c19bae))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 170eb43b-6b1e-4769-9984-466d5dbe3a9f))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 26bdfa0d-6af1-4493-9d7e-fdd5bea4bf19))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 5153ee31-0e61-404d-be1f-68a6010b3e59))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 837be359-b11e-41ab-81ab-4c967b1d7725))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp f999c9c8-a289-4c39-b155-743db33d4fe2))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 23700b0e-0a0e-4efe-b88e-8c9be5acbedf))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 95805065-0680-4549-89a3-041defe32728))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp cfeb4e89-951f-4b30-ae6c-549c9fa6bc43))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp d0f96765-6f97-490d-a77a-a9b455f17b68))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 26af7c18-0252-499f-8bec-fbee5ef37db6))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 50540584-1c8f-4619-8a66-4d8c95dd174d))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 5b89da72-879f-440b-96c6-c1f1e0879801))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp e3e0fcc8-c608-43ea-afd3-660516bd7071))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp fdd408ca-5d6d-48c9-8073-ad1770355341))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 925ce23b-0098-40fe-8ac7-c13cd1cf1f9d))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 6249050e-da8b-480e-ba89-59b6fa9cb4cb))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp b15c58f2-138f-4e2e-a1f0-f72bcc780684))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 3be5bcc6-6fde-4e00-9ca1-bdc52f967f0f))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 5681f026-6461-4b97-af09-2b771dee272e))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 4461fe1c-911c-4869-abec-1bd3f3171e7b))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 11c2657f-4884-45b1-91f9-c468486f0c77))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 0643c5fb-ba8e-486e-ab50-199940b54645))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 1fdb8584-c52e-417f-b3c7-5cc7b2e6188a)
    (at 149.86 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815ccc6")
    (attr through_hole)
    (fp_text reference "DKD55" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2b15622-29a1-4811-9286-a4e1f1acf2cb)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7672dbf5-3981-452d-bc87-6f5bcbaae722)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 132a5e0b-6c8d-4520-993e-55bde96dc44f)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f895801d-72ff-444b-9df3-0eae772199fb)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa9f7f9c-2474-4119-8838-368d75a47893)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 070c927e-bd6e-4749-a00d-6025a7cc2e54))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp d0939212-83bf-4d62-a6be-dba42efcf3ae))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 274a4d0d-7270-4848-83ba-6a7dc339298c))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5ae29462-92cb-4948-a8f8-a3872073b7ff))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 673813e3-0e66-4725-b053-81eaacb22f40))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp f55ca79f-cfa8-4c89-9123-e4fbefb89011))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 86d45766-71d1-45ea-9026-cca454fa33a9))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 76dbb9ba-2b5c-4665-ada4-bd8f948f4198))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 96d783c1-fe9f-49a5-9f95-7948960ba668))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(DKD55-Pad2)") (pinfunction "A") (pintype "passive") (tstamp cea5ff33-39fe-4ddd-bf61-e9c1030974e4))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 20a058cd-e097-4271-bef0-c49928861558)
    (at 160.02 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814c3df")
    (attr through_hole)
    (fp_text reference "DKD21" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ea8525a2-9da9-48c7-a199-6f6b1439bfbc)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp db537f6d-1c2e-4b62-b1d2-cbacf0144990)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ffdf9c5b-4744-45dd-84a8-257e2be120e9)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0161a509-bd99-41d3-b35a-042dc75a95d7)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 079b6926-c1e8-4fc6-8291-89cd99d7c292)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp f622a005-4dbc-417e-8da1-6adcd41ce47f))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 37dcd2fb-2c18-4b5d-b15f-623c9e2538f8))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5fa82c16-a59b-4825-8e88-d2064dd69f72))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 76342627-7e80-42fe-b7a3-dde7f4914ebd))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp bb01b669-aa6f-4e6c-ae73-3b067f5fccb5))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp bdef8eec-9bf2-4968-a697-7a4caf89e746))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp dea97c9a-8620-47b6-bc76-188c27ee88e6))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp ad881e84-05e1-488e-a9dd-6c40065bc6b5))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 46dceff2-f413-4959-9756-33b218a73402))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(DKD21-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 3e4f32ec-40c7-4211-a33d-d84eb33e0fd7))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 22876da4-6173-4cee-aff0-6f741c24d508)
    (at 53.34 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/4819908d-cfd1-465f-9b62-2ce7b5db795b")
    (attr through_hole)
    (fp_text reference "J32" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0d925833-dccb-4e15-be23-69beff1a5884)
    )
    (fp_text value "R2" (at -0.025 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 02a319e0-fb9d-4e3c-9b70-0723d9e4addc)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2e886aba-90d1-4427-9ed6-dfc77d460eae)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 1238fc37-b0ef-40ea-80c5-a10ab39725c3))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 1c2e0d04-0111-48cc-ac9d-8a4fa42d4d51))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 6bce3627-7853-4ba9-8ec6-b207afe8ebab))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp d8892d27-c191-402a-af96-2f58d4d323d2))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp e0d47248-ce8a-439d-b01c-7ca6af193523))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 391ac68b-dda1-4114-a497-a5a7f3466ccf))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 54329482-0ea1-436e-83f0-c843539b8b9e))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 621b96af-5459-4b8a-bdaa-ff7146d60274))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp ea3e800f-913a-4265-a41e-c2f859811fe8))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 431a68ed-cce3-4fae-9281-596d89cd2342))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 4c24fb55-aa3f-4c64-951b-43707d65d73a))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 5deb3030-34ec-4bf5-a74e-0c5896bb1476))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 7de44ea4-e660-4b7b-9f5c-00a5cc43e645))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 171 "Net-(J32-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp bc2eff40-16d3-440f-b575-2b07b4310bdf))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 234b8920-a74a-4224-ba9e-cfdb60241bb4)
    (at 81.28 109.22 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/254082e6-8a5a-4a48-b6e0-9d740cdfde71")
    (attr through_hole)
    (fp_text reference "JK8" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e38ac691-790d-4d0b-a87f-ebab35f8baa1)
    )
    (fp_text value "ROW8" (at 0 -2.54 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5775e194-b2fd-4007-8048-b771adfec218)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1242995d-428f-40a2-bd95-02f213fe78f6)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 20e4b388-06aa-4818-bf3f-59c94c93e81f))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 333a6185-20f7-487c-a80d-48872445e018))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 412824d8-a8b3-4889-96c3-1172746cf041))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 50656a60-6521-4e05-a027-b1bfa28e77f6))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 555621ca-6bbd-42fc-a371-6babe966fb6c))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 88aa5a3c-bfb2-4ae6-991c-be4c7a474d9b))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 19722fe1-1632-4fbc-967c-dcadd05e874d))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 881aa936-233c-40a6-84df-ec64fdb71b17))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp a7d379f7-5ca8-4f08-8489-a94bb142d785))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp aae98d9e-490f-4c97-a42d-e74cbaadea13))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 079b05fd-5a8d-4e8c-96a3-ed72f11dc0e6))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 310d4f19-e2ba-458e-8977-07a7c94bde30))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 9d784278-e2f6-42ae-a3c7-1bf55508c20f))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp b913eae4-beea-4246-b1aa-cbecc96a0971))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp d4d856da-3698-430f-84c4-4e691a7fb2d9))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 6d6d6b20-c742-46d7-81dd-71843426bd72))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 590bd1b0-55f7-4e1a-b85a-60a9b0243bd1))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 55c6e39b-b120-44a4-af4c-e7eb7b02a6bd))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp e5c63fa4-d1c1-4af3-b7db-1ef290d50144))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 453420d5-9d85-497c-9ec0-e19fb4314dd3))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp e30018fc-b176-4d90-a7f6-0a2c2226b2cd))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp c032e423-cdbd-40ad-92b2-0a107dd5179a))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 02ad6ba0-ce4a-4f6d-b42f-849d16084f7a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 257a43be-3849-4c05-9f72-7ad1bcea5448)
    (at 48.26 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/31c61803-b73f-4a77-8c6a-0adc05864be1")
    (attr through_hole)
    (fp_text reference "J41" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b5094eef-9f39-4eff-9d68-32771bd2a5d7)
    )
    (fp_text value "C3" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89b4cd9e-3141-400b-807d-70bde2e207c1)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7de73a63-1203-4cf6-b197-7c7ef986c70f)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 0658d96c-bfbd-425f-a8dd-b760f9811985))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 19d2e95a-dc04-407f-be81-df67b85eb5a7))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 35077b29-c5e2-4a4e-8b10-c979e46b261f))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 3c64a8a7-5b1b-4cb6-9ae0-97f2ec0bb19a))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp ae533d36-6d70-4511-85bf-22b0a2f39320))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 69264c76-9f0e-4895-af38-f93fc82bbad4))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 79d73f8e-ca17-4607-b895-8c7c2b10c5d2))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp b3b0a7cb-49cd-48e2-a918-b7d3f1c3cd2f))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp c9fcd0a1-fff3-4987-a890-6b2882deb5c2))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 03d73340-7d05-4084-979c-7691c75cb4de))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 28c3f832-75c6-472c-9ddd-8a90ab09c03d))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 2e19352a-2d06-44a4-ab94-29cd261b2fe6))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp bf74ef38-2ae8-4b93-b987-6f937b195342))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 180 "Net-(J41-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp b82e839d-feff-485f-a698-8db273695973))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 25c72e85-368b-4f4d-b62e-88af5da66328)
    (at 175.26 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068155527")
    (attr through_hole)
    (fp_text reference "DKD40" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 36b53743-b01b-4908-b071-a133577464f0)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c2dfb49-51a7-44d0-9565-3d21f801c2b3)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6326245c-f875-401d-82c3-27679d3d6d0d)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07a02a6d-b5ff-4277-9076-566612ba07d4)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5e9cc669-8841-4c63-afe5-d06769b5cf43)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 232f6d7a-0bfc-430e-b68f-4bfe6967e025))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp c3f341c1-9234-42c2-9047-85a9765091d8))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1ebaa823-baf2-4e26-897a-1985ac8be773))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp aca6919a-9f2d-4cf1-b88b-78d4d3893bb8))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp bfd6e3e4-7c19-4606-9805-31f133da3ca5))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c52c939f-477e-45cd-93a3-66cdce9f5a84))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 58c684c9-e360-4d18-b78e-55de5e9c735b))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 3c5c55c2-9ae4-49d4-9d61-305e9f5773ce))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 37fbf160-d730-4aee-a57c-dc3b5d0a8863))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(DKD40-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a93a5867-17a0-4375-ac94-d08bbad60158))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 260c918d-52b1-49dd-88ff-9b07c3e58dee)
    (at 177.8 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068151881")
    (attr through_hole)
    (fp_text reference "DKD32" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d763d653-92b1-4dde-9df4-1e447d89b8c5)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c49298df-902f-498c-b46e-e6798b8ad089)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a85b30b-1fee-4b67-986a-f779dddb51ce)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 905f1712-5236-4abb-8199-1781860dd224)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ced513f5-f98c-4829-b395-ecf4e1ccb4ef)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp bf622b91-91f1-477b-a0d5-29de8fc70679))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 9e1cfcb9-2168-4925-970d-fe91b9a199d5))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 18f73e73-af59-4538-b4ca-8477304c2200))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 751ab53f-862e-421a-bee6-1dfdcbd9c61c))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp c7af8083-8af1-4798-812c-c1cc4a19fecd))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp ce223e12-7ab1-47c6-8038-4fb856ba31ff))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 0f4ca9d4-93f4-40ff-aedf-3e049b7a0e15))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 33d7a27d-5c23-45c6-86ca-3f06c1ffed17))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 0ba2a9bf-fa99-49e6-b755-16db36cf1987))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(DKD32-Pad2)") (pinfunction "A") (pintype "passive") (tstamp e125fe00-ac5c-48c1-b30b-a28592a296df))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 260d316a-afcb-47fb-9cc4-c0ebdd6e99e0)
    (at 27.94 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/a9a75cb9-f8cf-4866-ad8c-e5c1c70caaa2")
    (attr through_hole)
    (fp_text reference "J27" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0f7394c-ceb3-4217-9ecb-df09d2215173)
    )
    (fp_text value "DATA" (at -2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c03aac8f-2c88-4d06-9566-5dae9b575cac)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 588edd11-2e50-4108-9a03-93d34c69db3f)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 13829c8a-4754-49a5-a64f-833517abd83b))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 3ae99dd6-68c6-4c0f-8029-48571177a4a4))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 4d3fbe30-8d80-40e0-b7ae-5eda5664f629))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 5a2ffe10-ce02-42f9-a474-f76d881a7163))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 5f567410-98c0-4c61-86ba-d95ac31b434f))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2b3b87fe-178d-462c-ba75-4c49c832fa94))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 719bda63-4195-4c5c-a44b-ca388f59907f))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 9eccfedf-a791-4695-b0af-985ec515edcb))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp c0358443-e9f9-4f80-a497-d7dbc807ef4d))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 05cb59fe-da5f-4695-a492-e1a7a16aeb5e))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 472fc804-d674-4867-b49d-d0b7110e09ff))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 6280022d-17f6-48ad-a197-535eafd9dff4))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 86d0ebd6-3f72-4457-9c26-bbd62913d687))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "/Rotary Encoder/I2C_DATA_ROT") (pinfunction "Pin_1") (pintype "passive") (tstamp 1cb8969e-d6f6-458f-ad19-ff8d1f94f199))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 27dc23fe-58b6-49a5-96f7-ae1c17cf5172)
    (at 147.32 68.605 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062f0b3c2")
    (attr through_hole)
    (fp_text reference "JKD11" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c1c53dea-2ca8-490f-a231-051196d69ab5)
    )
    (fp_text value "COL1" (at -2.515 8.875) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e64a102f-397b-494c-8cf6-c95b62df1847)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 22bc81d5-133b-4d1e-bb64-884c17cb825d)
    )
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 08c365b6-ac18-4c6f-ad1e-f80c54e30b16))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 130dafc5-8f4d-4bb5-9b9e-9e3702c11259))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 5c4f8d4f-e2e5-439f-b226-134c5072c34f))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 7a3aefc9-915b-41e7-b962-5450254a5034))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp bd809837-082c-4f5a-ba4b-f07fca987c94))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp ef2cb56d-0208-48fd-b900-84c0e5b48914))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 07646a8e-d5ef-49ea-b34b-d3ac28ae813c))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 7f777d93-d28c-4281-abe5-9f3ba7b885c4))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d625e1ae-ac62-453a-a4a6-84f216e698e5))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp fc1d98f4-4c7b-4319-a427-c73965a890c9))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 5ae40c09-6fe8-45c5-91d3-fc889f940b4f))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 80f9d4c6-acc5-4161-b078-5c433b7da6f4))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 8f37e9bd-65a6-4dbc-98b0-5551b75c9c02))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp cbc3a475-62ea-475d-acf9-f774bfd02592))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f5f4a85f-50e4-4c92-866c-57eac7550cee))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(DKD1-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp 92f5423a-4a7e-4615-86a1-33528092e678))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(DKD9-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 3d172ed3-d962-432a-ab36-89a3c838f827))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(DKD17-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp 859a77eb-19b7-4410-ae5a-3069c4d9580b))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(DKD25-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp 36a32b77-5c6d-41bc-bcec-fa9739f2e402))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(DKD33-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp 027b522b-4227-4e43-86ca-58baf1dc2d8c))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(DKD41-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp 2ecce095-ebeb-46f3-b95f-74cb15721f9c))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(DKD49-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp 9c47cb5c-623e-4338-8f38-a7c4a0f89793))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(DKD57-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp cbf193d5-c339-4683-99a3-d89192aa5c32))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 27ff589f-3de7-4185-b7df-d1dbb0da622f)
    (at 43.18 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/afaec224-6eb9-4aa4-acce-937066a89442")
    (attr through_hole)
    (fp_text reference "J15" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d9e49fc4-46fe-482b-8906-61af7c1472eb)
    )
    (fp_text value "B4" (at -0.025 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a3c320b8-4eef-49ac-b336-329b66e86bef)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 225fc398-2971-432f-ba6d-b4d5757d1c6e)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 156771b5-21dc-43d8-ba98-5c070b5e3b90))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 677f7fd6-fe65-4132-818c-44a0c91f5c31))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 8727dfe0-a564-4062-a385-c46672a2b168))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 8edc60cf-d5df-4697-953b-31cc055aba5f))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 915afd34-85f2-4f65-b2f6-5c607c325148))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8bf24a80-dffc-49df-8d9b-da527be5fdc9))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 9eac701a-d699-4247-93a2-af5e41c3ae6e))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp a1357a48-2956-4148-ac29-519f0e770f12))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp e0ba3ee5-78a5-4635-88aa-b5b3d5589222))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 004d701c-7e69-4a10-9c95-7de04fa2be20))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 787fdc1e-7e28-46d4-9188-bbfe7882ee50))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp abcba4f1-6f59-48a1-8ae5-91c9b3b973a4))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp eda12c9f-b24f-4458-a3cc-61f318dc57fe))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 152 "Net-(J15-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 58ed07e4-b138-4a86-827e-36284fa14c0b))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 2928ea20-8541-4021-a606-452f78a20d19)
    (at 162.56 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815ab1a")
    (attr through_hole)
    (fp_text reference "DKD49" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba3774ba-3fc5-4d36-9165-e45ae0120ea8)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 324da8f2-b0a2-4713-84ab-f6edf29268bb)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ace8864a-e1b6-4356-ab82-97191299e8d0)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3adc5ae3-536c-407b-a9d5-012565de6587)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bba4381d-efd3-4ba0-a706-a407f1feba1b)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp d83fa470-c252-48ce-b8cf-8a8e325fe8b2))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 05e96eca-9cd4-4523-a01c-9bd94b282f45))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2801d196-175f-4646-8f7b-69ed030c39e2))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5909c8c9-9ea1-46c5-928f-3f8cbb43b7ff))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5b0bb349-3d3e-4f67-9f25-3b485e608a8f))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b7ef66ef-f9ad-4552-bdfa-42cadbae2be6))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 29a82a38-138c-49c9-9929-1e78c98b37c7))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 2d0a103d-9868-4e44-b588-66f64693352b))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 9531f785-594a-48e3-959e-3345ab9837e3))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(DKD49-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 35c51e5c-433a-40ab-8945-4a198f312769))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 29df3f6f-748c-4874-adac-147e5b573cc0)
    (at 40.64 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/ad826993-8060-4ac8-b31b-fb9ea3e66c9e")
    (attr through_hole)
    (fp_text reference "J38" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad033d3f-7515-4bd5-8071-19514401ff9c)
    )
    (fp_text value "C0" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 386e0141-bfec-4df2-994c-6e60070752a4)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07c35ce4-407e-46bd-9fd6-02e59a1a39c0)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 5448dfbe-f8c5-4321-83be-b8da4a6f7008))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 7ccba34f-4bcd-4aaf-a5ff-8608b3ef7a07))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 82d18c53-ae61-47b8-8220-d0c0f67879dc))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp d793383b-7c58-4e0c-8e2d-5ddb26c377e3))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp f7c68938-c19e-48f9-88bf-5a1a6ebe7506))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 50d363e5-01c1-4695-965f-b8325a3fe035))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 5b17eec4-07a7-4eb8-a2a5-5eafc122f204))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 64430570-0a8e-4d39-a725-9ce9c1f0532e))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 6d66f42e-0f95-4b42-b02b-c52ef54a5f8b))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 3880c54a-722f-4831-82c4-cb9c60b240ac))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 4f92886e-1254-41f5-bdfb-f991f8f5e60d))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 5a455553-33d6-41a4-9d5c-5fc0d0702eda))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp c5a6c2f2-238c-4e0b-8412-a2399875cc4a))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 177 "Net-(J38-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp e5340b9c-b4e5-423d-ab82-ef3bd8f3bf9e))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 29f9e224-de0c-40d3-8828-3dbebcd4cdb9)
    (at 81.28 111.76 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/1fad7c0e-1222-4e2c-b60d-86033f546938")
    (attr through_hole)
    (fp_text reference "JK7" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e2ea8e0-e55b-4eb5-b5df-25dd678a2bf7)
    )
    (fp_text value "ROW7" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7a93b4f7-bbee-42bc-bb48-05087cffe2dc)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c5578e4-2f01-4b64-b5d0-7d34e23c6a97)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 06f9acfe-a8c5-49e7-a23f-47a118a3f9c0))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 0ebf878b-d139-4cd7-8806-47aa7b55a260))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 73a38cf8-037e-4a4f-a07d-0cd8e9bdba5b))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 7aef7f4a-2611-49b0-be4d-7c63c3228874))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 8f818c50-4c03-46d3-83be-470e63acb0fe))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 93b3a714-de18-45fc-97aa-8ba096dddae4))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 19153702-f26a-4b62-abcf-e93bb87b3382))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 212d2e58-01b2-47fd-956e-a8b9d1a47ecc))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 62a46037-1ff6-4b86-9b2f-e1846ee4fded))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp a1be18f7-f59f-4ac6-81ed-5e99ea541d72))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 3105fc4a-2d45-4d31-bdad-cd55420eaa74))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 4e308f3e-e2b4-4841-940e-c77b370c8dff))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 58e0d859-6778-48c4-84de-c1fd4abdc723))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 83b29e81-6fad-4977-aca1-5d9c3a19eb33))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp adb74a00-dc7b-4987-9e42-24debc8606b9))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 75bb3744-a91c-4e8d-8460-cfe5b4546c2d))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 2a7bbcab-fc15-4f5b-b8f6-a7cdaacb84c4))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp abc66a50-6214-42a1-b1c4-c5e3527744b6))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 31626a48-065a-445f-8bde-b4a32ed2c7b1))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 9e377702-74b2-4c5f-965a-a13cac8dd9b8))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 5fa44da3-fe2c-43e9-9e1a-30cb987e5331))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp bdbed806-9dae-4b96-adec-b1df8ed6ba43))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 645574fc-37aa-4582-aec8-2cf6be3dabc5))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 2df97280-a7fd-4d41-8dbd-6b6c7b25d23b)
    (at 50.8 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/308a8331-62e8-47c8-97d7-77c125dbca58")
    (attr through_hole)
    (fp_text reference "J42" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1cc0cee9-b5cd-46f1-be4e-672b3110c552)
    )
    (fp_text value "C4" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 39fe0ad2-879e-4613-80db-b6597ddd715f)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 42f95bdf-2bbf-4138-91d4-3465ff587469)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 08bd36f6-27d6-4196-8311-2f9fbef01a8b))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 1fb16541-bc7d-4847-83a0-0c4eec111ac0))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 6e2999e0-6117-41cf-9fad-01e6edef9c84))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp bbdb96ac-b023-404c-b291-c0956d537adf))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp bc67eb24-176e-4903-8ea6-c24e90adad44))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 1ba9cee0-3351-421a-92fd-2a4dfa088328))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 31347198-46c5-4ca3-aab0-0fb2ecbe1887))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 48809651-568a-44d7-9220-81ecac8c4776))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp f3f15c00-e138-45fe-b851-d56b93c71c4a))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 816d0585-8f64-4c5c-9e96-e44a5078155d))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 8e6d0d3e-22d3-41e2-9846-097b0e7f84d4))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp b39c647d-5f7c-4dd0-b7f3-04178b86815a))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp c9de39da-e912-42ff-a2b7-7995c2f44381))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 181 "Net-(J42-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp ffb655a1-f3da-42de-aec2-c9d423064714))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 2e919ef1-aef7-4093-8e65-23f808c67039)
    (at 180.34 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814dae9")
    (attr through_hole)
    (fp_text reference "DKD24" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47be3af9-453c-4d2f-b8ac-391e561638a3)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5c8b1bf6-f8c0-4f71-9ea0-e0ee5b44cf21)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bbddaa25-618a-4dd5-a258-5aeafcadbeff)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5574a4d5-d803-44fc-b2e3-ddd2854e15b8)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cded39b0-4d0d-458b-8188-edef25e77bf4)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp f5373a35-073d-4d7f-b8cc-d2dba3d3138b))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0a7803e0-8b34-4b13-8051-47403c2b9c14))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 20f3e462-5dbb-4f9c-8342-7f47fca6c583))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6b8c1fec-f8a0-41a3-b20a-41b391367135))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 89ac63e6-6cea-494d-ae7e-7dab26f1f8ff))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 90820e86-dc3e-484a-9b48-92ff7e113e9d))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 219159c0-31df-46a2-bce4-2ca3492ac58f))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp e31a3ac1-d228-4a33-9f8f-fa8c9b488ad5))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 6648e275-d72e-434c-8813-5fe002de0a13))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(DKD24-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 1e10c0ce-6399-459a-9541-60dec691887c))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 2ec28f2f-a015-4bdf-827f-b360c0fce7e9)
    (at 154.94 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068153f99")
    (attr through_hole)
    (fp_text reference "DKD37" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4285067b-a4c5-4407-859d-4189a2f1ebf4)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b51f17f-1e0c-404c-9821-ff86cb93d4b2)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp edcbc407-88c5-449d-a995-eadf003fbd5d)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53723086-6779-41f5-b214-ee15d1c82538)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ba001ad-d3db-4285-843d-228f3f67508a)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 7b87c91f-b3af-464a-82d7-80a0efb475c2))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 44382511-e499-4c6a-9c24-cb1a9818f3bd))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 53707df5-9a46-46d0-ac51-34bdb4c24446))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 650bf3ce-8e8e-4b15-8637-54cb9b7d608d))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 90f6e54f-8e86-4885-a5e0-960086fd80b7))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp fcf37293-f178-4396-8fee-82c7d5b494ed))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 7c45bc2b-7033-41de-862a-4885e918afe2))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 6df7fde3-e833-4138-8b66-d98eee476786))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 3c2aa11e-fc8e-415e-bd1a-a8a33d458486))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(DKD37-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 3c617998-16b6-4be9-9522-6cee4305fccd))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 2fdbee4c-6893-466e-aa98-3ca01e92f5fb)
    (at 149.86 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681482c8")
    (attr through_hole)
    (fp_text reference "DKD11" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 860fb94b-670b-4dde-933c-edd7bdf41ac3)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f1ec7da-9239-4fd4-b510-70d15f721d13)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 62307f40-ee28-453d-b4da-7c2e08d97af4)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6965d4d7-a611-44cb-b184-28c6fa35e440)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp abd10654-8788-483a-a927-57c91b5ac4b1)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 1acb15ba-369c-4e4a-b3da-7fd82d09d8d3))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0ec321b1-24b9-4d01-8fe0-61ed6baf81e3))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 008125e8-6427-400a-8bc5-145955e4037a))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 17deca54-18ec-4581-bc43-43a4702aebc0))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3f53e4ab-1c07-4775-83c8-d0bdaa64de60))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4536d474-d6f3-4c79-8a29-57eef91fa233))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 0abd50a3-5ef5-4e09-8899-8c61cf2b4e6f))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 2a8fa52f-463e-4b55-b7f8-3688b88490ea))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 06481be9-17d5-4348-8cf3-2ac380ada025))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(DKD11-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 79060d7f-785c-4e21-9e2e-9cfdabad60eb))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 303a2368-91e3-4143-b405-e6238492df42)
    (at 165.1 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815e9d0")
    (attr through_hole)
    (fp_text reference "DKD57" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a5b9bd8c-68d4-4297-9ebc-b08c763c0096)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7107537-9e87-4486-9353-c0630d84a349)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1eb64b80-b738-448d-b183-b6641e66228c)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2e8d5ee0-68ce-4937-933a-849702e2c738)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c7e105af-b4c1-43d1-af30-74551ba5599d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 59d2d24a-ec57-4fbd-86a0-ef9319c24c95))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 5c1e128f-7853-4ca6-a876-24b2cbe748fe))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 07a47422-194b-4174-9e39-172d9929e5db))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 27af4110-25e2-42b9-8806-9a065bfe9cee))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5a33a38d-035f-4db0-bb64-95cc16189f85))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 8408dd20-5d23-4f82-9d95-c907bb718d6c))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp f25274ad-69e1-44e9-ba1c-55b5275fe3ce))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp ae683a80-510e-4b09-8ce6-e4d6abf69a8b))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 498f17d0-0619-4922-a0e2-49d0beae0659))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(DKD57-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 55888fbd-a7ef-48a2-b735-102a73004be1))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 32a605ab-62ce-48b9-af40-d9f3119e89b9)
    (at 177.8 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068152d8a")
    (attr through_hole)
    (fp_text reference "DKD34" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa8902a2-1062-418c-80ae-0b1bd8ceb2e9)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1428f3a2-257e-43d3-b776-cadec0f10d1c)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3cc16dd6-3be9-4936-bfc1-efcd6a1315ea)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 17f04ce7-5610-43e6-b74d-5846e57d20e7)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81f7c4ec-a1ba-4df2-9d04-990fde4df218)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 9c94a715-94f9-4cff-83af-56a961002c85))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 62315f20-e38b-4b9a-8faa-ba4c2569f33b))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 465bf43b-7a2a-496e-8dc4-575f7042160b))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 57f888c9-37f9-4284-986e-1b2e1e114ff0))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 71f1d60b-385f-4b2a-8c0f-92a6f8634db3))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 894ae735-1f6b-4f3c-8e47-123bc510fdde))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 3933fd0e-b61c-43e3-bba3-9a3732eced7a))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a5be969b-8d67-4187-89f6-307ad3e3bcc3))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp f484e7f7-498e-49d5-bdf2-6735b858d914))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(DKD34-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 87bd4820-c17e-4e82-bb76-5a5c9c08183f))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 33dc1d17-3c43-484e-a994-57309880e165)
    (at 182.88 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815ae00")
    (attr through_hole)
    (fp_text reference "DKD50" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7559ce4c-aece-4358-8ef5-0f5081f5553c)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 449c367a-d901-4db1-8270-742c3ccdd03f)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9d66e8e4-d1a8-4585-9c03-6c256490ee69)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84ac7706-2d6b-4639-b249-f0c474b17ad8)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9f7eb7c-e2da-4511-8740-b2d1d2ae9532)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 1be2ee13-3f69-423b-b8ea-798e85c6cc6a))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 7ed91da6-3a6f-4520-ab74-e297ff794255))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 06d72d7f-a993-46d9-aa59-e05517035829))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0bb2005d-8374-4d0b-ab50-e295016a137d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3e38d6e6-f89c-40b0-9d5a-7d087a7893b6))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 91d95bdf-3286-4afb-a0f9-2486f740ef6d))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 178937db-8ae9-42ad-bfc5-1bea39c38b61))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 494e6177-b6ee-40a6-80a0-705ae1ec1e38))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp a1b20006-1a00-4a0a-9fdf-f49c33172d75))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 "Net-(DKD50-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 76be8b00-7a84-442f-9f31-22c5f5a7d20a))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 342ab4a3-9b4a-405c-9e22-ea88b62e54c9)
    (at 167.64 58.42 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000063313f69")
    (attr through_hole)
    (fp_text reference "JKD14" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 68791939-ff46-429b-a973-6ecbfd7d787c)
    )
    (fp_text value "COL4" (at -2.54 8.89 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 666363af-61ea-46d8-89bc-310c5615f444)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2960cac4-1460-4a75-91ff-46eb496637f7)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 37290fc0-bf19-4a52-9ea2-d369ee78f52c))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 8761abae-16b9-4d5c-822c-3ff66110f2a5))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp c0e2e3da-4f63-4738-b80a-67622b6c4b38))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c6f70770-85cc-4f65-86f0-7eafbf22eb72))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp e36794d1-e796-488e-809c-b25c9c765f43))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp ec75bce1-7dd9-4a11-a981-ef9d15e0c988))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 4c6b350c-1dbc-44ab-a3da-3889309824a1))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 545f7426-527a-47f4-8e5c-ab8e232af387))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 62ad5b48-2225-484c-9dad-4cad583f801e))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 8a2cc9db-b569-4a1c-8d20-6d810f5018fb))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3da39d12-258b-43e7-8d98-463f52d77355))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 7366abd4-debc-456b-9c08-526324ee0172))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 7e6d7218-93b1-4719-848c-e4d80f4c333d))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp b185fb7d-92cd-4d8a-84f1-56df004c28bc))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp db95491d-4dba-4063-8fe3-0a2fd6b507b4))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(DKD4-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp f8e7d2dd-2d13-4b8f-8890-06aaeb7ed96f))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(DKD12-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 842d48ad-8b90-46f9-8160-46c5ec76f179))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(DKD20-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp 6ffa9b53-531a-4f55-8667-f5f55cba2a1a))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(DKD28-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp 82b07cca-5861-4a31-afe1-9dfc1c6c38a3))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(DKD36-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp e9e35f6d-190f-4548-a69d-13c472e38db2))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(DKD44-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp bb74fa89-5571-4ff5-9ee4-e40568fd09c4))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(DKD52-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp 8f518a9e-2d7e-467d-ac54-d055cf3e9a8a))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(DKD60-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp e480dfd4-47de-4bbd-ba09-6cbbf6954ada))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 3a933794-312a-4c4d-96e1-014bc4bde59c)
    (at 157.48 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068151268")
    (attr through_hole)
    (fp_text reference "DKD31" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16e730c5-1e07-4f07-b6bf-8c1416ee66f5)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 72cd1155-6032-4285-889e-59f6033415f6)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61319212-8050-4da7-9e7d-4cef355923c1)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a87649c-bbdf-45a5-b250-aee0aaff10ea)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c215c629-aa87-4d8c-a7af-6baaa01aeb07)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp f0f55563-26cc-48e2-bedc-4bfd8b1ae3a4))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 7995874c-0529-4f7b-89dc-df9b6fc6fc83))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 037f40fa-dd12-444d-aa2c-52f52f843809))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 26e2c478-de82-4665-a0ff-22e160598029))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp b0add160-1327-4ad0-8aa0-bc539a4d64f3))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp edcd8abe-a2da-4682-b538-1c11470f8141))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 5275c1ad-3518-418c-ab0a-0b08cee88da0))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 8bf56856-0428-435b-9a35-8b1ded1977e2))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 1b8cc23a-b82f-4894-b752-71e499dbeb74))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(DKD31-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 013b3169-07bb-4bba-ada1-390766df98dd))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 3a933db5-3569-41ee-b97a-515b8fce0241)
    (at 165.1 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815f3c3")
    (attr through_hole)
    (fp_text reference "DKD59" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dc1519d5-0b4c-44dd-80cd-3ee015a02102)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0f396173-755f-4622-a9e8-ce78ad470352)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ee36e36d-b1cc-4f97-8639-9b6b1817c753)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d0c792f-d26d-4f56-8cfe-ace648f6906b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9511b9bf-3523-47d2-bf6d-be7507328f51)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp f9be50ba-f79c-45f8-a492-46f677582b02))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp c9df5675-4af4-46fb-aea4-77773b58599c))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0d47d7fa-baf9-4b6c-920a-e1c3f6d1f707))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 617e2366-edbb-4d57-a47d-19624f8469a9))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp a12c6a75-ca6b-4049-87e3-46ae5de4b7e3))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ba7180e9-d33a-4ae9-af2a-504d7be100c2))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp c76f6f7c-228e-4091-8a67-a333f74aa2d5))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 6e172697-d2bf-469e-a83e-86b88043e40e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 9344b755-2d82-4a47-a8f7-02b5fa888319))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 145 "Net-(DKD59-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 66354a91-7981-4c3e-8fe5-faa5b7b49d87))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 3b0bbe34-c31b-4e8f-858d-5fb9f9a1f254)
    (at 50.8 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/4971e12a-d07a-4b0a-8cfd-ea8bd16efa5a")
    (attr through_hole)
    (fp_text reference "J33" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da172ae5-842d-42c7-a49c-20bae12c4b8f)
    )
    (fp_text value "R3" (at -0.025 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 99d49147-09e0-409a-bef7-5e2145406ba2)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7fd485bf-fcb4-41a1-8c5b-087505f61e04)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 150da4b1-6451-44a7-8ae6-faa342460210))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 19916063-f7e3-4504-a5bc-a60c8c71bb86))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 47140528-c4e2-44b3-bc20-53f7a46f493e))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 813c7e94-7e04-4a47-9c64-d2fbfca8a5db))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp de58e641-9ad5-4173-bead-6e926668f202))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 1082cfe9-dbb3-462a-ba9c-3da280275e6a))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2369cff2-508c-4f84-ac99-d8ce6e3bcf34))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 847da94c-120c-49e7-86b7-a77a20365a6a))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp cdc85718-888c-4146-8050-4d029e3bad37))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 31d2eed2-98cc-4e09-aa60-e9a00cc8af36))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 43605d53-3ca7-4ed3-be10-db6af8d179c5))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 4861ac2f-8d8c-4811-9567-2a97a88d31e0))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 7063db2b-e9ac-4a3e-b28b-aaa87a857d14))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 172 "Net-(J33-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 515ef9a9-6c73-4ab9-abec-a02cc2abcc02))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 3ba82779-31bf-4934-9ae9-ede599803b0b)
    (at 55.88 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/b93d027f-21f6-4fc9-ad3f-317eded6973b")
    (attr through_hole)
    (fp_text reference "J7" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b481b075-9fdf-42c9-9f4f-1820179a57db)
    )
    (fp_text value "B0" (at -0.025 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c1d61362-65a2-49c7-92c4-42116f69f186)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 06bea721-6e44-443f-a10b-fdb382354c72)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 2bf57d54-6508-4cde-9868-7d1a1f902503))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 39dd4899-db7b-4f42-9636-f6aaf1c5eb3e))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 468f1465-a526-429e-822b-774275d0ce38))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 5606c2c9-8d20-49a7-a220-882fb12b6de9))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp fe34a838-864c-4aee-999e-a4d9d2a53aa1))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 21ae025c-519f-452f-85f8-6c4a5765c910))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp b2a6473b-dbac-4141-9e30-38f28870da3c))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp f7929113-ed56-486c-8bcb-866485096b1d))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp fbcf8f18-273b-4de6-a7fa-1aa52b6a30eb))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp c594017f-aa60-467a-ab4f-3544e1ac6b56))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp c9519dbb-7fda-4b2d-904a-05f32731be38))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp ce049c30-6629-4827-b32b-d3c8b0d57289))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp eb5539f7-1c4d-429b-928b-15d4b3d0598a))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 "Net-(J7-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp c63dc724-2c12-428d-a6d9-e73eaba68b2c))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 3c2eb42f-9013-4478-a977-42449c129146)
    (at 185.42 38.1 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006331405e")
    (attr through_hole)
    (fp_text reference "JKD18" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b00981c9-8bf6-4b78-80c1-933fcbd51a89)
    )
    (fp_text value "COL8" (at 2.54 8.946371 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2327360-867d-4991-8419-6cb934a9cf56)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf609d9f-a23f-493e-b93e-9d03f9c0c792)
    )
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 05ef0e00-29ca-4d4d-9642-2600927db091))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 0d5de438-23ae-412e-88dd-fe50beeca185))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1c39129f-84a8-4c89-85ba-4d05dab9654d))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 326b9baa-5003-484b-9521-a250e3f3528b))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 5f50af92-3291-4cbc-8333-d444b031428a))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp e6630dad-2a15-455b-8921-0132cd1df109))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 5d7ba097-47df-4fc9-8e57-8705c2930f96))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 774eb6f6-f7a6-4bbd-afa6-91eaa6394f8a))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 8b5cbae1-9434-449a-a703-cfda9a0822df))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c35fd526-ced0-4dd7-af3c-fec07192a0c7))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 26a8f6cb-4b07-40f7-b88f-b66f634bdfdf))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp b0d3edd5-bf1b-4ae6-bbbc-7da31b7f37c5))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp b7fe458c-e50b-4b49-98ad-1f6101385c43))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp b86fafce-607a-4bac-9e0d-ee620f1cb55f))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp c756f7d4-1f46-489d-9315-1fb92d306863))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(DKD8-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp e29c3067-0ead-49ad-bad5-c2b1ba1d17a9))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(DKD16-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 47986d26-c836-4c2e-8a0e-8cb25c8470e8))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(DKD24-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp fde298f3-2b6b-4a93-ac7d-3b4d3d2858bd))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(DKD32-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp a296636f-f326-4157-bfb4-9225abe53b66))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(DKD40-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp 3489d450-28dd-4397-a0a9-ed2cc8a68453))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(DKD48-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7e794796-dff8-4cf5-8963-4eb5dec38ca9))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(DKD56-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp 6a84f3ed-4bf7-4725-835c-924cae858800))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(DKD64-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp 4cda26ce-7ee7-49d6-84ab-e4f93412ffd0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 3e0e88aa-3e9b-488b-8ac1-df465c4da286)
    (at 172.72 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068158993")
    (attr through_hole)
    (fp_text reference "DKD46" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1748ce0-72c7-4271-a77b-6d8a1a1fecaa)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 76479ac3-ae09-4b1f-982e-ca0d4fa40790)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96e6e9eb-30e0-49b1-9dfe-bf205bb0676a)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4dc56d86-ee8e-4946-ae4b-ae226eca705d)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5bcaa730-7e90-46d8-8c93-175716d61312)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp cda91e73-6bda-4a39-966d-8648f7579d54))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp dc90718a-d67d-4a65-ba2a-3970d5a0bf76))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 48fd0c80-51fd-43ed-bb78-554f10776331))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c264dac1-6060-4fa2-b51b-b12d0d8730af))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp eefc4b4e-6cf4-4f60-b055-58aea2b0bc24))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f3599601-bfc7-400e-b061-68efc239c5ec))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 557e50d1-1aa2-4927-b2a3-525c4a05d767))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 5308bb10-13c2-421f-a4e0-b5daf6856432))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 454f0ff5-2e36-4384-9127-b2d36b0e9b4f))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(DKD46-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 7f69bcc6-c5cd-44fe-8680-a6173311a32d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 3f1dd0ef-da65-41ae-b280-6236bbcfcc3c)
    (at 121.92 30.48 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062d3c8a4")
    (attr through_hole)
    (fp_text reference "JKD2" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2d5a51a-22e1-417a-9408-288163dc6dc3)
    )
    (fp_text value "ROW2" (at 0 22.86 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a462ee1-3c40-4947-b6a8-88984a3c3437)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cdb2a6dd-f46f-4baf-bd34-e44eba1ef929)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 2094e9fa-1d71-4e64-ad2d-48bd3e69388b))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 3233b95b-f686-4b83-a858-8125567043d5))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 548b7d8b-a92b-45c6-af0a-7c2dc1100fce))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp c7fd69e5-4044-47fe-a7e7-2b3fe755e4a2))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp df3ce281-4ab4-4f96-b0aa-bbb921f672f2))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp ed31e92a-404a-4406-8b6e-38b515b0aaf8))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 01eea81d-981b-4a2c-bad3-3242e669598c))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 3626ed38-81b8-4b4a-8e1e-5ae20a8c0bfa))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp daaddc3a-521f-4fb6-85ee-85f00a930de7))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp f7399592-4c81-4c92-af0c-c43e5164cae9))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 0700a721-e632-401e-ac76-476d2a737ce8))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 19e4d4cc-9bde-4051-88b5-44b9978de6b4))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 4816b946-dfad-490b-b7c4-49c09b29fdbe))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp a8b7b39a-273f-41e9-a8e6-8032da655c3f))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp fea5533d-abef-41be-a549-2822bf2ac716))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp ade2cb95-8122-4d54-a630-98e49a0ad1f9))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 6f117f6f-ff32-44da-a11c-21438911514e))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp fff899fe-76bd-4963-a395-59335a68579c))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp a16fd816-4a42-48bf-afd2-57521dcf297e))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 60c3edeb-7634-4dd9-85e0-f880966fbcb4))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7ce6a47b-d831-45b8-b06e-9c4c65cd8e78))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 98e815be-a0c1-43d6-8493-98fda86a6941))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(JKD2-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 34cabc97-60ac-474d-9fff-4c7829415391))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 40b20146-03e0-4b43-a71c-eccef9a00c98)
    (at 81.265 119.405 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/7b075ef6-34f5-497d-b2c4-d126c3850d1c")
    (attr through_hole)
    (fp_text reference "JK4" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3325de8c-f2c2-4c6c-8acb-8c6d57fbb840)
    )
    (fp_text value "ROW4" (at 0 -2.555 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c5964992-9cbc-4489-9e7f-e31e383b5123)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af01c317-7284-4268-a701-f371c29f155c)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 0575b032-30db-4c9d-9c64-6e88583e71f7))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 3f5adcc4-feaf-411d-a5b4-0cefc6c115f1))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 47fdbbd7-ce41-4e74-8173-282db6a2b5f6))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 60031a4a-1c45-4b8a-8428-66343d3551b6))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 89aee3e2-346a-4849-8364-4f7b1fde8c85))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 995bea88-2561-42db-9a75-78d9c74f48eb))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 0917c52a-b018-484f-872b-565c28a10aab))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 0ae36fba-7a37-4b2e-933d-9172ab05a66e))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 964fdbdd-d817-46f7-bb5a-b19937f82ab9))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp d740f583-b66a-4a0b-99db-915a7d058bbf))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 42f46636-9c84-4e87-8dfb-72c05e13d743))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp ab895532-8ca9-41d5-91f8-06d737eec62b))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp d6c6da7f-994d-4778-8657-e8dbe44cf50f))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp dfdae403-bb08-48d4-b042-b5f0fa182e90))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp f813ffe1-fc01-4d76-adc2-b56acdf35680))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp bd8bc864-1cb8-4ad9-9e6d-35e1bc437948))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp b4d8bb6a-4f72-4b99-b3a6-eeb2b1a0c6f3))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 8fc3a5f6-af60-48d9-951e-21c0bd122a69))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 41d4f8af-1867-4d58-b12b-9bef3ec5f44b))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp acd231c3-d87a-41aa-a37a-d99be4caff1b))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp eb0d05e7-5fd4-4ff4-b2a1-56d0078fba45))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 326f8b6a-9cc1-48ad-9792-3e4c8fde7153))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 9d8807e3-f82b-4f8a-8f8e-86296401e24c))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 43b2885c-bd72-4099-9f8f-2099fa3e98fb)
    (at 180.34 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068156da2")
    (attr through_hole)
    (fp_text reference "DKD42" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4126ac92-9c98-4c7f-89cc-c7ff51c8e54a)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8d275705-9286-48e7-a3f3-e9c0e04980c2)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5973b297-5c9e-42b1-b43b-91699dc9bd68)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 70ee1530-f53f-44d5-9f1e-ba8b270851e0)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e4d2fece-1b12-4aea-a750-28747ef73f3d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp bf5e4a76-0c05-4cc9-8778-2f3daa0d3f4b))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0e080afe-9b82-4b61-ae86-ec8cc124007d))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 32f15c15-c278-4d22-85d0-598f46263eb0))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 85b2298f-3486-4843-ad67-e06b484cc8a8))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b5f268d6-388a-4834-a981-1906838711ac))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp bd30b38a-3125-4ef0-8fc0-30c121a42354))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 43b10474-0a07-4754-85e8-fccc93fc9b1c))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 8a9b58c7-3db4-45b3-bbba-c1bf7aa59e53))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp bd2a7031-921c-46cc-9c16-9d13db33bbfc))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(DKD42-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 686e5427-1453-46e1-88a2-83332d06c7e4))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 44712abb-8e5b-4dc5-87c1-d135cfe6af79)
    (at 162.56 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068148ddd")
    (attr through_hole)
    (fp_text reference "DKD13" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7db56d91-91f6-466a-bb94-d46be6a937df)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c30873a8-10e3-4933-bfc7-9129164dd7df)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3cceefda-4442-4b19-a320-dadeabbc5917)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 713e8728-938d-4a6c-81a1-bf9c9c8dc077)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca92107f-b589-476f-8df1-41a59e194516)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp e4ac3532-2938-4b58-acc6-16af1c25509f))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 662958f8-8abb-4494-9b58-ca4df663b432))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 59b1af1f-69b2-46c0-a4f7-3ee941d390d1))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp f0432be7-140a-4a76-a41c-f9e875122bb7))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f72fcb0a-0e5a-4f8b-aa52-34a4a1b680c0))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp fb19be03-f801-4ad4-adfb-bf5c6ccf7979))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 243de128-482c-4c17-8ebf-c82ebd886767))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 175e72cf-9851-4c0f-8e1b-8064fcd292ec))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp c43cfe77-ecdd-44d5-a44d-e58f8e33a58c))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(DKD13-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a3dd7b33-079f-4a03-a0a8-7ee34da5a11e))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 49f451f3-8725-4518-8619-93498068637a)
    (at 45.72 121.945 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/a9ec2a0e-723d-4586-bb29-c7e7adc2beea")
    (attr through_hole)
    (fp_text reference "JK16" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bccb0510-9df1-4c15-8035-daedfc13ae5e)
    )
    (fp_text value "COL6" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 304a6dd7-a837-4272-b1c0-56a40dc6b4ac)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 987c85c3-5203-4907-b9ed-589791ecde2e)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 083f32c3-f1b9-47a3-ab83-63fed9648c92))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1f0a8375-ee31-4829-802f-2f66c7e80095))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 241932b5-3590-4619-bdd4-6de9ce6dc426))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 4b8be3ff-4f25-49f4-9eee-d26026895d38))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 908c7b6a-0cdc-40f3-b71d-cc6e61fa3ee4))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp cfe354f3-a152-4130-8cf8-3db201a85cc6))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 6520a531-76e6-425d-8997-a1a2279f9dc8))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 8a29e9ac-167c-450e-836d-840c410eb487))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp b8a2def1-1d18-4f23-9342-2810b6cd2735))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp ba80640d-142d-4e72-95d5-70d0866c1e8a))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 184880fa-efc0-47e3-bc28-fcd09a24113a))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3cbe6e28-cf7c-4cc9-a887-f6050e1a9eb5))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 79ea7338-2596-41cf-bdd1-428363143cd9))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp a4ed682d-b072-4d7b-a158-66bdda88358b))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp fbe50840-3f2b-4c2e-a821-ca8b29aada40))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 680d9c2f-9684-4229-bc57-145857e7aae3))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 01ccc412-83ac-4f51-aa4c-3b661b9cc31f))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 39ebc0e7-8a31-458e-ac32-21184b87aa70))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 1861bb60-f0af-409f-8bfc-bd57508b6e72))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp e3cac474-8192-49b4-9c24-8dfdabd42c61))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 5c31cc22-ef91-4cb2-806e-a0afc8e57c9f))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 5548e0bb-9382-4e2a-83fe-f8f4f5c613e3))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 677bc118-6808-4a49-b3f1-068f10ecee31))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 516ab4a4-a8fc-46f7-bb63-fa55d12d120f)
    (at 182.88 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068149591")
    (attr through_hole)
    (fp_text reference "DKD14" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f18c7a02-fca6-4161-8cc0-907b96fc11f6)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 48bb1e6e-fb71-46f6-8965-78dd94b820f7)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41a5225e-7368-46f8-94b1-5f0db3b93a7c)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8126b9eb-29a0-44c2-8b1d-57c291be4876)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d994df65-2aec-4ce0-a0e9-a928c1a212b0)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 55ab279c-0dd1-4283-8cde-27cfa920972b))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 8998cb6f-0a15-4ef1-8f4e-3ee7e94b2ab3))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0fd40c73-f4b1-491f-9215-e6632db4bdd7))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp b18d7170-7e65-4653-b9f4-ee2e69881775))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp cf88092c-7bce-4684-b2d2-b431b9685586))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e9efd602-6fcc-4bcb-8d95-14d17a9c0757))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 237ae8ef-8b14-493e-8c17-03c9748db117))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp d964cfed-b4ef-4e68-92d4-8c61a0859467))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 1f30cc00-272d-47a5-a58c-433de6f990ca))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(DKD14-Pad2)") (pinfunction "A") (pintype "passive") (tstamp c116d476-29ce-4a25-992a-a6d67401be43))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 5299b0fb-f74d-4e79-b7d7-40687e8d5bd3)
    (at 45.705 116.865 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/ab4f2aaf-c08d-4b11-a37d-319ce4b9b7d7")
    (attr through_hole)
    (fp_text reference "JK14" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e30a1e0-3916-490f-a7d0-169d613b5bda)
    )
    (fp_text value "COL4" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c2eaf71b-2d04-43b1-a52f-d59a7a480dea)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61263771-a8e1-487c-9d7e-34afacb6d74d)
    )
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 33510bdc-9a8a-459b-a53b-229d3c7e48a0))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 66569666-594f-4046-aefd-dc898a9ec9da))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 68c754ab-66cf-4170-934d-8f56f71792e9))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 7488179b-fabc-4964-915a-5cad2181a652))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 8d7fa8bf-f617-47c9-9946-7d6216f7e8c8))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp a4afacbe-258c-4089-a9a2-cfd535e98560))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 1cd00423-271f-4170-9408-812e5f49ae31))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 52b32cdf-33d3-4a71-94ab-55af40e7c7c7))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 85ddd4cd-b041-4214-ba37-21af2e95080c))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 92c9c7cb-7904-4332-a7d7-65c9606b0b8a))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 41fd0096-953d-49a5-b7b1-c986c610c29b))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 85d0cc72-2416-4741-b8a1-212da7024682))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 9b6994e6-c40e-498d-ac9f-887afe9ad4a8))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp b082c83c-dc3b-4bb7-84b5-c1603d0912fc))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp b792fe2a-3fd6-4054-ac4a-abb07d4b4c33))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 19c3ae37-c6c9-4b6e-8922-ff1148aa181d))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 81386521-8f9b-411f-9833-1dd6b271ccd8))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp e9e5e01c-f4d6-4a09-9021-86688a24622f))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 8468016d-0a6a-4ce2-beef-67673f688aec))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 52281a8d-9e32-4a02-9b76-7747c697e85b))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7342b642-c7fc-4002-bfd0-19b422093d13))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp da67059f-e8a1-4b43-a3d9-1ddaf6e948a0))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 2835bcca-4b5b-4404-b3d7-cfbd434919c9))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5) (tstamp 570d66d5-2854-404a-b3ef-8a618d8c3fa9)
    (at 58.42 48.26 -90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/b22185af-1de2-40b6-9e80-0da54f88759e")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f491419a-4a73-49a0-84d6-676e320ae74a)
    )
    (fp_text value "MCP23017_SP" (at 3.81 12.7 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 018ac0ca-e905-4956-882d-cd184ed826bb)
    )
    (fp_text user "${REFERENCE}" (at 3.81 16.51 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50e960c4-6d6f-4449-aef5-2fc7d5426fc8)
    )
    (fp_line (start 1.16 34.35) (end 6.46 34.35) (layer "F.SilkS") (width 0.12) (tstamp 28e4cea2-bc58-45f6-a2a9-a4645c15862a))
    (fp_line (start 6.46 34.35) (end 6.46 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 75852742-e7c0-4ae3-bf5f-3e6d27110e7e))
    (fp_line (start 1.16 -1.33) (end 1.16 34.35) (layer "F.SilkS") (width 0.12) (tstamp 803e9b4f-7806-41fd-a8f4-c2cb3da5bebe))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 97e5dcfd-c8a0-4d08-9ec7-297c86da9ce3))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp d66f75eb-2912-46cd-b5af-0a315fed9bc9))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 81fe1463-89d2-4343-ba25-2acdf78bd5d6))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp 287ac47b-db32-4a94-8cdc-fc4964081b5e))
    (fp_line (start 8.7 34.55) (end 8.7 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp 2ad00b42-9555-4c5b-99df-e36d4e59d274))
    (fp_line (start -1.1 -1.55) (end -1.1 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 680c9338-b49d-4168-adf1-7ca0efc08cc2))
    (fp_line (start -1.1 34.55) (end 8.7 34.55) (layer "F.CrtYd") (width 0.05) (tstamp b189398d-80b1-44ab-9f2d-2bb02a73b131))
    (fp_line (start 0.635 34.29) (end 0.635 -0.27) (layer "F.Fab") (width 0.1) (tstamp 243be0f9-9dd8-4d43-a34e-0746d6525c73))
    (fp_line (start 6.985 -1.27) (end 6.985 34.29) (layer "F.Fab") (width 0.1) (tstamp 4386aa39-bb1f-46b5-9dd6-efabb8746d63))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer "F.Fab") (width 0.1) (tstamp ab978915-8c30-40ee-9c70-59f4e5a53c03))
    (fp_line (start 6.985 34.29) (end 0.635 34.29) (layer "F.Fab") (width 0.1) (tstamp b6463d1a-58cc-4e86-980d-5696f73b9bc3))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ee87a575-4c85-467a-9e60-819334432063))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 "Net-(J30-Pad1)") (pinfunction "GPB0") (pintype "bidirectional") (tstamp ac54e68f-3856-48b9-84ae-658930835ca6))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 "Net-(J31-Pad1)") (pinfunction "GPB1") (pintype "bidirectional") (tstamp 30ccc610-1103-4304-bc72-c447e671abfb))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 171 "Net-(J32-Pad1)") (pinfunction "GPB2") (pintype "bidirectional") (tstamp 0d97d0a7-1cd1-4f9c-8f0d-80354719c46f))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 172 "Net-(J33-Pad1)") (pinfunction "GPB3") (pintype "bidirectional") (tstamp f52cbf36-51d1-4d33-8de4-637622a2b888))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 173 "Net-(J34-Pad1)") (pinfunction "GPB4") (pintype "bidirectional") (tstamp a4fa321b-bf67-4550-84af-1aa6b788cd86))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 174 "Net-(J35-Pad1)") (pinfunction "GPB5") (pintype "bidirectional") (tstamp 7e3514c1-07c0-4b04-84b0-e42ae820b405))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 175 "Net-(J36-Pad1)") (pinfunction "GPB6") (pintype "bidirectional") (tstamp be38b6b4-07fe-46cb-9636-991ca80eb1da))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 176 "Net-(J37-Pad1)") (pinfunction "GPB7") (pintype "bidirectional") (tstamp a0a8a96b-b779-4daf-97dd-7e5cf44be371))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 "/KeyMatrix wired/+5V_KEY") (pinfunction "VDD") (pintype "power_in") (tstamp 8e314bfd-d550-4b68-95bf-ec0edf94e0d3))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 "/KeyMatrix wired/GND_KEY") (pinfunction "VSS") (pintype "power_in") (tstamp 731fc123-f9ee-497e-a05b-dc66b3aa4158))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 188 "unconnected-(U1-Pad11)") (pinfunction "NC") (pintype "no_connect") (tstamp 494911de-32e7-413f-9b51-ac71676da46d))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 187 "/KeyMatrix wired/I2C_CLOCK_KEY") (pinfunction "SCK") (pintype "input") (tstamp fcf420d5-9724-420f-9a5b-8b335cf3fa2b))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 186 "/KeyMatrix wired/I2C_DATA_KEY") (pinfunction "SDA") (pintype "bidirectional") (tstamp b16f6f24-33ec-43ab-b619-2c22c2efba22))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 189 "unconnected-(U1-Pad14)") (pinfunction "NC") (pintype "no_connect") (tstamp 20327333-565e-476a-93c8-6bb2da5b4ea1))
    (pad "15" thru_hole oval (at 7.62 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 "/KeyMatrix wired/GND_KEY") (pinfunction "A0") (pintype "input") (tstamp 909cbb47-9e5f-42cf-83f3-656d7d25af3f))
    (pad "16" thru_hole oval (at 7.62 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 "/KeyMatrix wired/GND_KEY") (pinfunction "A1") (pintype "input") (tstamp 82c81cb3-3539-4e2d-8028-99156bdf1daa))
    (pad "17" thru_hole oval (at 7.62 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 "/KeyMatrix wired/GND_KEY") (pinfunction "A2") (pintype "input") (tstamp 52b10da1-d858-4a3b-b810-cb4019703dd8))
    (pad "18" thru_hole oval (at 7.62 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 "/KeyMatrix wired/+5V_KEY") (pinfunction "~{RESET}") (pintype "input") (tstamp ff6a6c0d-8c42-4206-ba80-8b05040ccf1c))
    (pad "19" thru_hole oval (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 190 "unconnected-(U1-Pad19)") (pinfunction "INTB") (pintype "tri_state+no_connect") (tstamp a8d53190-e910-498f-bd45-4346f0f093d2))
    (pad "20" thru_hole oval (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 191 "unconnected-(U1-Pad20)") (pinfunction "INTA") (pintype "tri_state+no_connect") (tstamp da77077a-dbc7-47dc-bc2a-414d2f31f8db))
    (pad "21" thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 177 "Net-(J38-Pad1)") (pinfunction "GPA0") (pintype "bidirectional") (tstamp 7d59b625-3ba8-4d2a-ac26-706eb0829f73))
    (pad "22" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 178 "Net-(J39-Pad1)") (pinfunction "GPA1") (pintype "bidirectional") (tstamp bf202eeb-8cde-478a-9c54-f57622ca78b3))
    (pad "23" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 179 "Net-(J40-Pad1)") (pinfunction "GPA2") (pintype "bidirectional") (tstamp 2fca7c4e-45f9-4507-93b1-6de47f287731))
    (pad "24" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 180 "Net-(J41-Pad1)") (pinfunction "GPA3") (pintype "bidirectional") (tstamp bd52a347-67a1-48c0-9fa0-cd31697e7a79))
    (pad "25" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 181 "Net-(J42-Pad1)") (pinfunction "GPA4") (pintype "bidirectional") (tstamp d2b07926-2d1a-40e9-8d4d-cd832f289460))
    (pad "26" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 182 "Net-(J43-Pad1)") (pinfunction "GPA5") (pintype "bidirectional") (tstamp 9bb96b4b-f248-446f-baa7-ba0d3b1fd45d))
    (pad "27" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 "Net-(J44-Pad1)") (pinfunction "GPA6") (pintype "bidirectional") (tstamp 84a84d60-fdc7-474d-ba62-a738cac994bf))
    (pad "28" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 "Net-(J45-Pad1)") (pinfunction "GPA7") (pintype "bidirectional") (tstamp a4114195-75a4-47fb-9546-0cd2ee584a1c))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 593b6382-e8d0-4286-af7e-c963ce1047fa)
    (at 58.42 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/0acb7b97-c6e6-44df-ad0d-230a70aa8726")
    (attr through_hole)
    (fp_text reference "J6" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33dd8803-71f2-44bd-b4cc-8dfca4a89608)
    )
    (fp_text value "A0" (at 0 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e7073ff3-5477-4e8e-8eac-c6c839211d13)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4118ca42-cbf5-4007-8f00-3c853caebfae)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 2db73e12-8d55-4c9f-9111-06321ff1bf3b))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 5e131de0-59dd-4487-8337-de0dce828791))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp a944a0a0-302a-485c-ac01-78d811b92b30))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp eec9adee-0ca3-4f4a-bc2a-d385e11c22f3))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp eef0b708-d745-482f-aca0-70f6e8b031a8))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 0dd8a88a-3c85-402b-a2dd-d98bc5ddbd5e))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2c9e77bc-a78b-4385-bbfd-f567e0df96c3))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 4d24f783-afb0-42a0-9683-e8b59325e024))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 7df80943-5e57-4498-aea6-993562316ae9))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 11fed0fd-e478-4d70-a2a4-ec27e972ebf4))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 397c7179-11c5-4ba2-8026-b27a0edfc173))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 3aa9856c-47e9-4ecc-b55c-c27c5da2092b))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 611b89fe-c54b-4f54-9b17-d4142ae633a4))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 75 "Net-(J6-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp f744641e-4674-436f-97f8-bda7558362c2))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 5ada835d-561a-4dce-a1cc-333025507ece)
    (at 33.02 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/8c90d3b7-ed32-4c78-b2d9-31baec8389d6")
    (attr through_hole)
    (fp_text reference "J29" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c4139120-c7c9-4616-a0ae-9a851adb1f9c)
    )
    (fp_text value "+5V" (at 1.905 0.635 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81d2a3d7-9e78-42be-94e9-00bae4f7e7f6)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ec35fb6-fbea-4c53-bc7c-52d581e3adb1)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 196f058e-8f27-44e0-b0fd-f8cc62686315))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 43cfb8fd-8455-45c8-8b72-d7070ac63b03))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 7b95a7c4-cda8-4bcd-807a-99b5ef03fe1e))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 923cb571-19be-4be6-8532-02c9d244b0d5))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp a6a29a4c-0a52-437b-8da0-296025dac4fb))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 970993a2-1f28-4914-a470-29d59376f99a))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp c7ed31dc-b1b6-4ead-abad-3a055196871a))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp ca4af12e-71cb-4b12-bbb3-009474823ee5))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp d66161e6-ec5e-4c68-8f75-63f16b295d6b))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 33106bd2-3e98-41f6-988c-7158791c3c4a))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 812a9bf5-0cb0-4a5f-bce8-2a3cdb8d7062))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp c47df8d6-d01b-4f21-8eaa-4777f8956be5))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp d9fa1bba-ba87-4376-952a-41bb8392f957))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 168 "/KeyMatrix wired/+5V_KEY") (pinfunction "Pin_1") (pintype "passive") (tstamp 818e6ca1-9b10-4d24-a98f-05f907ff65f3))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 5b361c12-85e7-4d7a-ad0c-5635dd503d9e)
    (at 167.64 68.58 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000063313546")
    (attr through_hole)
    (fp_text reference "JKD12" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 91335775-654f-4a24-80bb-f1921595dc99)
    )
    (fp_text value "COL2" (at -2.54 8.89 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5079bc00-a690-488b-ae36-39dd6d1246a2)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ecf0af1e-3208-449c-a9f1-93dd437e23e6)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 0641728c-5460-43d2-950c-4da1df9f243e))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 0adcbe70-ee0b-4b15-bb49-68bd4d51c5a4))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 45466bc8-0ddc-4ace-b70c-83e30724e674))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 5a6e5175-3c50-4f06-b6ff-8bf6e821d890))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 80826803-6f46-4861-bf58-63b21487b0a0))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp f47af63a-d50f-4ae3-8e5d-b9d1c0de7f16))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2d219123-23a6-45ad-bfb5-f918de396d51))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 4948feaf-6ece-4a7e-9757-1dea7199d34d))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 7bc77701-f83b-4986-a2a5-565679d6c0eb))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp d07a514b-b2fa-4622-942f-e91a8f74fa57))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 13c9024a-b42e-4d33-8db3-ce7611045d05))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3d02ff62-2d1f-4fe1-86cc-5f35b1f013e3))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 554f564d-ac66-409a-9408-3ceee3e12298))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 5a179d07-ef25-4e96-a2df-319f3d452547))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 9f50a10d-0898-41c5-9035-2c47919e1628))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(DKD2-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp 8b530ecd-2836-45a5-b9eb-0e58d78a4dc9))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(DKD10-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 6737138e-48e6-4aac-a609-07583d685222))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(DKD18-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp 289842ce-8fd5-453e-94f9-7b17a98f0b7e))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(DKD26-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp fa7ccf3e-34d5-4832-880c-d9f6bbe3b2f7))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(DKD34-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp 5d93334f-62b6-49c8-bd2e-abcf5a900aac))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(DKD42-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp 0641abdd-2de1-4450-a4b0-af8d9cc4d65d))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(DKD50-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp d95d77ba-3385-4516-b362-0978ef9b3cce))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(DKD58-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp 0664dda2-2d29-42aa-a693-1b46ce3c9bf0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 5bcf28f7-2e42-42f4-95b4-8abf2df3e733)
    (at 121.92 27.94 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062e51d23")
    (attr through_hole)
    (fp_text reference "JKD3" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5692755a-8bdc-4149-a594-175ee80c5c65)
    )
    (fp_text value "ROW3" (at 0 22.86 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp be0fcfdc-8670-47bd-ae5d-be0f71cb9093)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 87081929-5755-498f-aaa3-ab03281362ef)
    )
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 44c798d8-a538-4cf1-aed3-fdd41a578787))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 587d7c85-91b2-4ac6-a655-9bc2a3e19c97))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 773a93b5-2a04-4837-8b56-e3d660537919))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 791db7b1-f826-48e7-bcc1-8b10d49bf61e))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 91bc792b-bbdf-4d49-a9ff-5e1605e42f15))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c05452a2-29f6-4d40-a1e2-c9e8b0d64b0e))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 1bdfe29b-822d-4f5d-bb46-980e52168096))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 3d568e00-069c-4b67-8454-535c4f92774d))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 415e6d92-6497-4cd1-8bd0-2cdd76fe3de3))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp f2b709d6-1e13-4603-9cdd-dc34d7a04714))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 01c2245a-c887-492b-aec6-90c24e6d5e4a))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 2fd9b8f2-6ad9-4634-84d3-e17933375fca))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp be015a33-def2-4a3c-be86-6c139ac011fe))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp becffa58-0edd-44a1-a585-7772c6344fcb))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp e0725e4a-e2a2-4dd7-90a8-ef7e1380bd67))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 3885fae2-b15b-4250-a4c0-8f039447b7fb))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 73a6c348-8a6a-4260-a559-a881b81c3a76))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 2989db1f-eff3-4697-afee-57e3f9ec2a62))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 6192db96-7630-4aa3-bdbf-5ff3389f2bc4))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp e46a0d8c-3fe7-4832-b808-cb3a7f8ade84))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp c7057315-071e-4f63-9a9a-b6f8017f46ed))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 1520b925-71d3-439f-b59a-a1e9460d37c0))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(JKD3-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp b6ae6891-5b19-42c9-af74-245668011306))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 5d44cc4e-a8eb-4036-9770-8d574c03b5a0)
    (at 48.26 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/0bdb6175-8701-43d4-9212-8e88185a01b9")
    (attr through_hole)
    (fp_text reference "J34" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5526f846-fded-45e1-ab8f-3e77f29baa8b)
    )
    (fp_text value "R4" (at -0.025 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50edec12-f2d7-486c-a238-cf600b34e1b5)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2e8c4c72-0a75-464e-9b42-9d31d1c354c9)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 31e0c95a-78ca-44bb-9184-1c4d48ccbf3e))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 603ffe71-d502-43f7-9155-6e6da6e380c8))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 8dd2ebd0-beab-4a6a-a970-4109d2d0d2a4))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp c01a1ce6-aea6-4b9e-95ac-caf2bdbfe10e))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp d9c0241a-6ebb-41a4-87f6-309aab930fa4))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2e89248a-15d7-4656-a7ee-18b697173f47))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 53e09637-2981-4ef0-9061-5a44f519a23c))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp abf99505-1c46-46f4-816f-6fedb93ce4af))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp ee8a6fd8-1e7f-4e43-ab8e-8f82128f2170))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 06587bee-b192-4516-ae60-9e51f83ce577))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 1f7f935c-1486-4d74-a7be-35320430f56f))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 4ff116fb-9ea8-487d-8c52-fdafb2a9e05c))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp baa55708-ee83-445f-90d3-122f514b8a19))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 173 "Net-(J34-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 968e9c9f-cd24-4a12-bbe3-5cd4499e2633))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 5d685473-9730-4a87-a74f-ac0c7d9ae88e)
    (at 165.085 48.285 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000632d6459")
    (attr through_hole)
    (fp_text reference "JKD15" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ae3a16c4-f80a-46de-80f3-8e6d41f4594d)
    )
    (fp_text value "COL5" (at 2.515 8.875 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2934ec74-eeb9-436d-bfeb-5d23eb7af938)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f93cbe4-3e62-44e4-b339-d68f1337a52a)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 02fedba6-ad2b-4be1-9de9-b82a9662b3ce))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1435a85d-b2ab-40ff-8820-5523bfed863d))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 173be1f4-4ec8-47ce-9b8b-d69b25e91b1a))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 3a151cd4-e26f-4bf4-b848-47de440c2a9b))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 3c6424b1-cd56-4e4a-8821-cdd88b109e53))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp a309dd88-6707-4c6a-a563-891eb9b9c9b6))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 15a80f8c-a2c8-446e-82d3-b221fa079703))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2de4196e-66d6-47a7-95ab-a25722d2f514))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 6c94dc78-3c03-49d3-94ca-0fdbb5150694))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp a4da397a-f913-4b61-902f-65e1034be114))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 15cce064-74da-4a3f-abf7-e0eba22e3cc6))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 31bf6108-7e6f-4bdc-bead-2206dccf2814))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 870ff586-8467-4da2-80e0-58d061686a4b))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 96766025-b62c-403f-8194-b45ef1c2de17))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ff03ab9c-1d66-4621-a0df-d83942206346))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(DKD5-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp cfe8ca95-8ec7-4cf2-802e-8d0c2e3e9472))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(DKD13-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 695320a5-7541-4782-b0ed-d5730bc68ebe))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(DKD21-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp 58e5f2bd-5a23-4a58-bfb7-00fbb51223bb))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(DKD29-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp b4d37e34-2f66-4ac6-bdad-be886abe28dc))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(DKD37-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp f0be6bed-0866-41ac-a480-30670794abaa))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(DKD45-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp c686a11e-75f9-48b1-9102-a14995e94dff))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(DKD53-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp 7ea2ecbf-74ff-43b2-8f48-a7972e09fb12))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(DKD61-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp 947b429d-460a-4da6-bc18-524fbaf63389))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 5e87af77-cab8-4eda-9b71-08f260f853d2)
    (at 157.48 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815018b")
    (attr through_hole)
    (fp_text reference "DKD29" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07626c52-cd53-4de9-9de5-b4da0887b4d9)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b317b792-b369-46cb-8ebe-d9d242ff6d99)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 591a3067-adde-4a9a-a10a-2e59ec902eac)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7149c19c-4c89-4bac-8f0b-5b7970415adb)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d914f5fb-0045-4f53-9ed7-8dc8344c55ca)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 632a477e-4826-4a16-bcd7-83061378effe))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp cad83d04-c4a4-4b81-b801-4f80335fc410))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 763bc84b-f623-447d-9fda-4e45c5120ce4))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 7c7b1a3b-2665-4afa-b492-908ee227ba26))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9dc8beb0-5f0c-4fe8-abee-bc790559704d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp a4588bbe-5a65-44df-b724-b4dba9ad9308))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp a153907d-50d3-4706-8bbc-02ff726cf909))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a86c7c1d-48ed-4fa2-a431-51eed0e3263c))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 5470c000-ba58-481b-861b-3f77527476f9))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(DKD29-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 0a1a168b-1911-4efe-b2ed-1a1b3833a3ee))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 5ee5dba6-bc2c-408f-88e2-269ae0e3ec9f)
    (at 45.72 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/9bac6bac-7f2a-4129-b344-f43fb7c2d498")
    (attr through_hole)
    (fp_text reference "J40" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca747592-63b8-4c46-a923-52775f5763ce)
    )
    (fp_text value "C2" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a7af943-e293-4d91-9bd4-7440e6fd2953)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4fa23a0a-7519-4aba-8b1e-f626b601ba0d)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 4fe4f960-cdd9-4a2c-be2c-494e2da47eb6))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 8848cedc-b195-4cec-85af-5d99a2c3ce72))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp b6aef2d5-a3e7-4ab4-9b63-77387460522d))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp d3a0b23d-9d89-48e9-b40c-114194336960))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp dacd3f78-200b-44e4-a99f-02807b16a25f))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 242bf942-1d00-40e0-8e33-9df3436484ba))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8557376b-c91c-4f76-bbd0-b9ce3e5ca7e9))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp ae798f09-b18f-4364-9a21-29af6407b872))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp b57a84cb-d025-4c68-a211-a81a285de21d))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 18026e32-7d3a-4d8d-be21-54d45d069462))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 671da2e0-3045-4f39-bfa9-3c6d34ad540b))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 860f3769-08bd-431f-a7f0-67e3f35b257e))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp e04ac0c2-721f-4c45-8e11-a01a38fe375d))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 179 "Net-(J40-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 62a833ac-3d86-4c63-9e37-db24bb2ba350))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 65a1cb00-f323-48cf-b952-ca130a65e4fe)
    (at 185.405 48.285 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000063313fe4")
    (attr through_hole)
    (fp_text reference "JKD16" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 95865d09-62d6-4cd4-965c-4cc09a110768)
    )
    (fp_text value "COL6" (at 2.515 8.875 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3e64cb4-cc9f-44dc-974e-d304da305852)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec4603ac-fab2-4fd3-9313-456d38f2d931)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 4401399e-2514-4494-8982-665deedb2a7f))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 6284eab6-2965-4ea8-8253-b09bce590321))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 6a02e844-9f26-4224-a787-cb73f2ca1b0c))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 7ddc0c3b-77a9-4525-a561-c8ed92a3a155))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp b280ba9f-4270-4601-8837-e11e77893dbb))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c772763e-498e-4b7d-a236-afc0716dcaff))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 57a602b1-53ea-4357-89c3-979c908ed87d))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 79515287-579e-44a5-98e8-4fdc26133802))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c91965b6-21be-4ce3-aad1-1274bee02645))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp dce5fd67-205c-4ac1-a971-93d647952e04))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 94ae5b69-85a9-4020-915d-52b69babab29))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp b7a3535b-75fe-42ea-80a6-628dd6590cb2))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp bfe00b6d-a358-4943-ac00-1bf8765b4191))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp ec1eae32-73e7-4834-90c3-d2f1fe9952c9))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp f709b7d9-00eb-4d51-942c-51ff5b545dfe))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(DKD6-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp 52a28c38-1109-43b8-a136-78de79e3de97))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(DKD14-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp fd8fd08b-9217-49a7-9cc1-55942d840806))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(DKD22-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp 1c493b21-7b28-4f27-be93-be15736339f7))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(DKD30-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp 782e7ab6-d607-4e67-a926-392d32564367))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(DKD38-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp 2df706da-e9e2-47da-8371-0aea21dcf8e6))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(DKD46-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp 264a8864-0cb6-4647-a3ad-7688b9a24b1a))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(DKD54-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp 16ef902a-5d62-468f-9010-9e86c99a1a98))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(DKD62-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp f93914ae-dcf0-4825-b645-a8290d031d5e))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 66b19a0b-d07c-43ff-9bd5-abe61a163306)
    (at 40.64 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/3074fade-b34d-479b-8200-fadd967b837d")
    (attr through_hole)
    (fp_text reference "J13" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 22ba7011-af16-481a-be60-4832e2fa49b7)
    )
    (fp_text value "B3" (at -0.025 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3147e880-51e1-4334-9901-8c646d0f1c58)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 674dfd9c-2241-44b5-bfb4-f6d11b1ff583)
    )
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 02fad080-98cd-46ab-9ee4-13a74595ac68))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 3e2733b2-429a-48e0-a5f6-9bc75cea3fb3))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 3ec4c6d4-d672-41bf-9275-f96679fe932f))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 5ed867d6-e24b-4827-bb08-f4f5e703c946))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp c0d36b8c-6b63-418d-9fae-b9063f7e525a))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 785e7afb-5347-4e11-b292-701c649113fb))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 7e75e4cc-e0cb-4b98-b80b-d3c04ae9a412))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8c6484b7-f099-4c5c-b5fd-abaa05b4ab18))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp a72be1e0-9af1-4c8b-a80a-e23a2ce6ded3))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 36ddd131-24a1-406c-a011-522c67b17ac1))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 6613902d-850f-4102-9d7b-cc5a5ef20ea0))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 9d68ca63-4f76-4c15-8edd-c79507b64ea4))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp b3c4f9ea-9465-428d-a878-c35a35b4a0ec))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 "Net-(J13-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 05d71641-765e-42e9-b112-428ee2e771ec))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 690958fd-853d-4e62-928f-0f0ab7da9e49)
    (at 152.4 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068159000")
    (attr through_hole)
    (fp_text reference "DKD47" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13cf84f6-489c-47de-993c-72a831e22fb9)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 209130f0-dabe-4d79-98d9-d25f97a50854)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 35df2f13-c4ea-4169-9451-7b8e2f2a2b1a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11857262-6963-4d50-895c-ed444b2fc51e)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c6889ab-882e-4bbf-9d88-65236ec52ece)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 7227f1b6-b085-4f1c-a982-beb29ab551de))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp a4b8b3e3-ae56-4593-89a5-9b674f662c71))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 28fbbd11-2162-45a2-8d69-1516a2bb611b))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 529096d1-16b7-482f-8b1d-450af91fdcae))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 65e0f591-b4ad-4a41-99b1-8a5e42503746))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp e2f7efe6-d7b3-43bf-84fc-8215a70bd6e3))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 390c6c5e-72f4-4a56-a8fc-411b3470a286))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 45e4e106-6e2a-4966-9fc7-d85f1b4a924a))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 0a684576-9cc5-4b11-ab10-b30706fd3ba7))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(DKD47-Pad2)") (pinfunction "A") (pintype "passive") (tstamp fe82d0ae-3685-42e9-bff6-efdfb53a4052))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 69b60f37-8cf1-441e-a118-ac3ed62047ca)
    (at 147.32 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068160f36")
    (attr through_hole)
    (fp_text reference "DKD63" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e965750-a634-4900-aedc-7f4ea033448a)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9337f4a7-a64a-4b94-8ad0-212b4bad337e)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4605a823-9f56-410e-9580-9f88b6af6a6e)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07d0ff0a-ab1e-476d-8071-bbe6603b0c45)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f5f88aa-a430-4ee3-9d98-f253b8dc3d76)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp e788b498-a0e1-40ca-accd-a881895938fe))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0bf3964b-56c8-4f9d-a746-205b336fa881))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1f0337fa-bcce-4ee7-a9c6-c44981574782))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2edb39dc-d189-46c2-9674-a21aaeb5d76a))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 738207bf-0b15-483c-bc1c-5f4b93aa64cf))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp c9ae631d-b80a-4958-bdfc-dadc7d2be346))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 302e5853-d4bd-4adf-8617-ade3fe742fe2))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp b30b56fb-f21b-494c-9bc3-4f39592609bf))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 537d1958-886d-41d2-aed4-5396020dd8de))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 149 "Net-(DKD63-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 271f2b55-6a3b-461c-a3e1-833beb3aa10a))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A41D) (tstamp 69c7190c-e105-4931-afc6-fe0b07e0d673)
    (at 71.12 25.4)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/1908c35d-2c55-4083-bbc5-a3c968285595")
    (attr through_hole)
    (fp_text reference "J100" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 473ba493-9122-4fbd-989d-1dd98309adb2)
    )
    (fp_text value "PROMICRO 1..12" (at 2.54 13.97 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 68b680b1-ea6d-40b7-a888-061877726e4a)
    )
    (fp_text user "${REFERENCE}" (at 0 13.97 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4657a7e9-9250-4605-8b1c-b2b08464af15)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 5421db4c-f988-4bd2-a432-a34be768415f))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 80496762-da74-47a0-9390-292d32f889c5))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp b0bda077-107f-4ba5-a3b6-1007dc3bcc23))
    (fp_line (start 1.33 1.27) (end 1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp bcf8af10-8e0b-429b-8cd0-ecfe4f1ff800))
    (fp_line (start -1.33 29.27) (end 1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp d310e7e3-4c34-4b15-9065-b32d914e8664))
    (fp_line (start -1.33 1.27) (end -1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp f8cec250-0049-4065-a941-66eb188d7ca2))
    (fp_line (start 1.75 -1.8) (end 1.75 29.7) (layer "F.CrtYd") (width 0.05) (tstamp 27f18e28-32e8-4cf4-8060-aaf39482a150))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2f6cf638-e103-433c-89fd-e607bc38dd2a))
    (fp_line (start 1.75 29.7) (end -1.8 29.7) (layer "F.CrtYd") (width 0.05) (tstamp dedb12c7-a39d-4e45-8f6b-d1704f88e3d7))
    (fp_line (start -1.8 29.7) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp e027cdaf-a300-42c1-9d52-b948ecc18e64))
    (fp_line (start 1.27 -0.635) (end 1.27 29.21) (layer "F.Fab") (width 0.1) (tstamp 01be90fe-fa2e-49d5-9c99-68a92e4490c7))
    (fp_line (start -1.27 29.21) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 4280af1a-1f95-439c-a6cb-a69b2a83af53))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 6122ffb5-49ef-404f-a6f5-3f2edfc016d9))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6c0cfc7b-d440-4b2d-8a5d-e6466140a64d))
    (fp_line (start 1.27 29.21) (end -1.27 29.21) (layer "F.Fab") (width 0.1) (tstamp ad7f400e-1357-4687-9263-a247d39f284e))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 "unconnected-(J100-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect") (tstamp 082b8108-ea87-48dc-9e16-7ef7886b1c84))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 160 "unconnected-(J100-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect") (tstamp a412af91-3c29-4add-ba9c-e11bd600a304))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 161 "unconnected-(J100-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect") (tstamp ce1b7a1a-a491-4210-ab07-70f6b2f2c2b6))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 76495eb5-33dd-4c61-87aa-71a348e9583d))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/I2C_DATA") (pinfunction "Pin_5") (pintype "passive") (tstamp a58dcd01-ff6b-4c53-aa12-e522be198a4c))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/I2C_CLOCK") (pinfunction "Pin_6") (pintype "passive") (tstamp b1064901-460d-49fa-b82a-8513a6dbf1bf))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 162 "unconnected-(J100-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect") (tstamp ade31591-cefc-4edd-8789-3be009288b5a))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 163 "unconnected-(J100-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect") (tstamp 7a565fb7-a97b-4a1b-9ceb-659df93c7353))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/ANALOG_MUX0") (pinfunction "Pin_9") (pintype "passive") (tstamp 18e07c4d-b9ad-4355-8ce3-56cca0a4dd91))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/INT") (pinfunction "Pin_10") (pintype "passive") (tstamp 3d9fa7ef-d37f-4d6b-bfd4-3577e12471ca))
    (pad "11" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/ANALOG_MUX1") (pinfunction "Pin_11") (pintype "passive") (tstamp 13308fc1-8d5c-4922-b92b-da9ba8f2e3ee))
    (pad "12" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/ANALOG_MUX2") (pinfunction "Pin_12") (pintype "passive") (tstamp 056e1d72-139a-4fba-99f6-0d2098a96fb0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 6c346650-092b-4155-a2d5-433c85250b59)
    (at 38.1 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/41415bac-1126-4467-b765-03fce423d075")
    (attr through_hole)
    (fp_text reference "J24" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ff6e72d-92d2-4ff9-bb22-8c5267b456dd)
    )
    (fp_text value "INT" (at -1.905 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8462fe3c-6fb2-4a5b-b8b1-e3ff86e3ad06)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c04375d1-586e-4875-bcd1-7762af6c20ad)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 3b871e0c-ab38-4719-a2d5-ed90930aedba))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 42116bfd-457d-4593-ac30-a7ae4508e2ee))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp d5ca8fc8-81f8-4a87-b951-6a5fa74306bd))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp e606296b-e2ca-468d-ac38-71b5344b6e85))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp e666a0db-591f-48b6-8a0d-7c7a6373c0a3))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 03088ce0-e686-48cc-8f83-98dc3013c127))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 29121967-985e-4629-9206-85806f8f2a9c))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 9875cb24-9ea3-45b2-a974-1b8edc7b9af5))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp a354a73b-54b0-4dc8-a419-fbc76de5e799))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 010c43a2-732c-48b0-bbc7-9b5dac471893))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 53a6249a-2895-4514-93d3-6e61542c69fb))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 6c879b85-62f9-4a6e-a7ee-23bdecc74acf))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp e4bc409f-c38c-4340-be74-f1985233ba4d))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "/Rotary Encoder/INT_ROT") (pinfunction "Pin_1") (pintype "passive") (tstamp 8cdb0859-c152-438f-a411-753aa02c1177))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 6f2bf9e7-3704-4d74-9e50-61609e297d3b)
    (at 175.26 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814ee70")
    (attr through_hole)
    (fp_text reference "DKD26" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 00db1892-2b7c-47d8-ba6b-d4783b781a4f)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9726c65e-8a21-4bb9-9b4a-8ff5219ea804)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ffdd6e4c-cd0e-48fe-a4d5-20ff4060071d)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ccbfd78-2420-42e4-b344-6bdba202fe57)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9ad44cfe-2e99-4f85-a09d-c1e0de86f116)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 3ba20d79-511f-495e-95e8-db41a1710c12))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0223cd7a-3958-4654-9da3-98e5c5783fed))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1c515c31-ce83-40db-9430-5d2d6a070e32))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 7112cbb6-5c26-4857-b7df-f13e2fe62fa8))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 73d94fd1-12eb-4bd4-9621-663ab032197b))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp fc8f5fd9-ea38-4ecc-9647-df5fbcf0e9aa))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp a75badb6-c5f1-44d6-ada3-f5de86b2b617))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 4b85da15-5ae0-42fb-bf12-5062647fa87f))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 9e309529-28d3-45a8-8e81-e87f8edf3c44))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(DKD26-Pad2)") (pinfunction "A") (pintype "passive") (tstamp bcda027e-8fd0-4b3f-b477-6c5c9133c6bb))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 718dba53-7a9f-4c42-aaa5-07406806c2ac)
    (at 157.48 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068152a31")
    (attr through_hole)
    (fp_text reference "DKD33" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ebc29cc-23cf-4870-92bf-dd3f571383d7)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b7811113-3bf4-48f1-9e20-df98a06b163a)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba25bd0f-a53d-4b9c-b093-e4a4769a07db)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5dde0fbf-d24d-49c8-8b4e-987ab2dbfd40)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfc566b1-a532-4daa-980f-05ce56d8ad5d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 1d0b6142-5c8e-46e3-9be0-e270ee12e02e))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 9224b4d8-d66c-4f8b-8028-443fb64427cd))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1af47d07-bdc4-451b-bb96-22c25c8c161b))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 50e9787e-f60b-4ef4-944b-f85f7b78cf54))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 85026ed5-f997-4763-afe1-086c5af267d0))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ffc45d11-f787-4ef8-83ce-9e1eaf910b30))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 5cfcb642-8a00-41e6-9389-971585b42337))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp fd6f67b5-cd0a-449a-9776-fa6180f4ef2a))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 09424eee-009a-41b6-8c3c-2f7e089cd8e7))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(DKD33-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 610011f3-481d-46d4-994a-c97df18f73f8))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 72409533-989c-4762-99b7-6b85e4e4754b)
    (at 185.42 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068147533")
    (attr through_hole)
    (fp_text reference "DKD8" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 11d6ceaa-21ab-4f20-93b3-1a2fa6c138fd)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d9eee5d-9075-4e73-a97c-51fd3a27f922)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b9ff39b-2b23-4a51-bac1-81f65afa8a80)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 454a371f-30c6-4b26-aaa1-c6c89241518e)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bd2829e1-6629-4f43-a84a-0dc3238f4bb3)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp cbdcd399-aa87-48ad-ab7d-f8277b14c6fe))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp da26f08a-1757-4be7-90fe-bd21c741b478))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2e3bce2e-5eb2-43bd-a5e6-4f40bc97c51e))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6bc1565a-a91e-47f1-a734-080c3b476ae4))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 851f89e9-919a-4f61-ac5e-f2e54e9fd784))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 95dec77d-c16c-4c94-8d30-3f6e315e7e42))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp dbab9d53-b5e8-4d29-96ba-be682e73d441))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a72cfec4-0c7f-4bd6-8014-29cf97b84f21))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp f36b5811-d485-4726-b28b-d623772692a5))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "Net-(DKD8-Pad2)") (pinfunction "A") (pintype "passive") (tstamp ca79e436-43ee-46eb-9d8c-9c8ff8c5a96a))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 72e50459-a757-45a3-83d2-f1b95d716122)
    (at 149.86 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062aaa113")
    (attr through_hole)
    (fp_text reference "DKD9" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dce2f061-ef39-4174-ab23-0384c9a4cee0)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bf9a1cde-5b0e-433f-b5bf-ec2b4db5eb7d)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ab12f6c9-a5cc-4288-ab62-bcc6153931af)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3a30cdfe-02b6-434c-a6ca-1c4cff7fea2f)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f049dc57-ba18-47f0-8e32-39ade4e59e9d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 49ba4409-2b74-4b49-86d4-04ad56d2090e))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp b6d1981e-4ef1-4772-afa5-08cc245f7270))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 8aad0c9e-2d90-44ae-b95a-05f28de9dcf4))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 90e5e2a5-f10b-4b72-a764-ded15d6d07dd))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 96918165-e1b4-4ccf-bce6-4e20b2130821))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f53257b7-dabc-429f-9037-1059e1cf0e1c))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 1b9361c0-eb49-4fdb-99c8-743af09d5f26))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp f6089932-7e38-4fc4-91e5-8099d63e7ccf))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp a309a3bc-1d50-4c06-94bc-5d7e9ee7e497))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(DKD9-Pad2)") (pinfunction "A") (pintype "passive") (tstamp ca770001-2d07-4547-bad0-915b7d0f1707))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 7569f1fa-35c6-40e3-bd01-f4020fe89084)
    (at 167.64 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068143d6b")
    (attr through_hole)
    (fp_text reference "DKD4" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84a8486e-95b1-480c-ac3d-fd81fd661d48)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fbf19dd6-932d-4517-a052-5a1acdb0c960)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 271271c2-50ec-4046-b30a-d0db5ffe2114)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9de07c63-8f11-4124-a1e1-57aed5992cee)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8e80286-201e-442b-ac9f-2e6a7d14b019)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp c4821cff-7291-4cdc-ade4-a9e26dd7b9f2))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2b982708-9392-40de-98e4-2393d2a05f62))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5f069c92-c668-4587-a6bc-acadf2dbd796))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 849f49a3-de9f-4855-b42f-1023f27adeed))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b4465328-d6ae-4d90-8a71-6cd4d0911a55))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp cac75460-ed52-4bab-af27-bd97e40d86eb))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 198d8740-3d70-40bb-81c0-47993a89ff98))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a79e034d-f8e1-44f2-a9fe-3219eadfe854))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7e2abef1-cc76-4d0c-aebc-918b2b05d09d))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(DKD4-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 47e2c9fb-258f-4043-af79-d89e8df7c29d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 76522f9d-4fd9-4874-9f2a-64e2a4ced811)
    (at 154.94 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068155058")
    (attr through_hole)
    (fp_text reference "DKD39" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp acf009fa-40ad-4d3d-a888-a597bb09664a)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3142959b-26cf-42a1-8bf5-ea7169ca0d2b)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1901b609-095f-4fe3-a8b2-a0e566052490)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 36aae5cd-7838-4210-8248-20122af15d1d)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9fc2a208-4609-455e-a5f9-5f16c0df934d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 1515e87a-84d7-4cbb-979b-ed34e71c4b3d))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 8d4eacb9-0103-4822-b279-9c6c88128c0f))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 7f2e3b1a-c201-4aaf-bf3e-fb36a57b53b2))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 819f0f77-f282-4f4c-a8ed-2263daabe01d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 87cb682c-0b4c-4a53-a407-87b2f1b4412f))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp dc93dc8e-9f12-4461-9737-5b0900440c44))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 9731e751-7765-4819-8ef9-31e4e3e0bade))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 4027d384-a788-4f94-82b9-10bb8ce52b6b))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 878be31c-e95c-4065-a0f9-a00b7337818e))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(DKD39-Pad2)") (pinfunction "A") (pintype "passive") (tstamp bcc20c1b-8a06-4080-966d-fe1840edda46))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 78bd3887-fdc4-4e9a-acd1-e467b76bd693)
    (at 81.28 116.84 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/067ca1f6-1bce-44a5-aa4d-1b7dc1cce057")
    (attr through_hole)
    (fp_text reference "JK5" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 67ea16e1-0c55-4397-8a77-4000de8a246f)
    )
    (fp_text value "ROW5" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 32345de2-9ba8-4bb7-9953-31ce8feaf06c)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61d905c6-3a9e-4103-b419-c7340a7ca7b0)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 416b4b4a-68d1-4dac-8de3-2d72b95dc977))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 647ad568-fbc4-4997-9789-b45f722be644))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp c2a43f3c-2d3d-4631-889e-37b8ef93080f))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c7c5c2f1-8395-4f8b-a94c-ac95484918df))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp eb935fbc-c792-429e-bd07-71e23daad5de))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp f7afb02b-0187-4c38-82cf-3673ebe27769))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 98192b3a-7189-486e-a221-1568d87516d2))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp aa5798e9-bed7-4b6f-aaf2-1a03df2c250d))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c7d784c6-ec8d-4c87-ba91-478875b50851))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp ff6bbfb6-5344-489d-8b99-88b7f3480183))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 40d9530b-9313-4d5c-b8bc-51d30daeb0c1))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 586e3c91-a343-4d50-b017-0ae0da71af9d))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 5aeaf742-32cd-4108-9f64-a97de6c418f4))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp c56e6725-eec3-4d3a-b89d-8f584d36f831))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp d81d1402-c429-4283-bfcd-5c29562dcb4e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 30e68e7a-0af9-44dc-a2d9-0c080e913c30))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp b9292852-4810-400f-be14-76e0b93df842))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 7dc40a91-5f48-48f8-b713-3a14049bfe71))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 3c7661d0-ecd4-4d8c-8608-9da0708e25b1))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 17ff9da3-4a0b-4e6f-b8c9-d48e3f5a7f9e))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 578ae6c0-5141-4fb3-a151-91926dd02aab))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 2b5c2297-5758-457d-a7db-0cb44470c725))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp a3c33b4d-11fe-4008-a759-b013130f2c29))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 7a782070-3833-4958-b2b6-05cbb20bd722)
    (at 81.28 114.3 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/03ac933a-a006-4d8b-ac97-af6cd6e29abb")
    (attr through_hole)
    (fp_text reference "JK6" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7496c309-1d2c-4f04-b676-68aeee5ba04d)
    )
    (fp_text value "ROW6" (at 0 -2.54 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af81f7a4-5c1e-4ea3-827c-38acfeb82fa6)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp faf7580c-b600-4480-9328-0c0284b85aa9)
    )
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 39029047-fb48-4bbe-93f9-3afe7d1720eb))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 64fe45d6-ce53-4601-943c-f54c68838871))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 66a78d06-64b3-4fd0-8c1d-dfff7fc6907f))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 6b918332-58d7-4cf8-9a93-e947dadb2bdb))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 9235847c-80f2-43df-a9f3-360c9c780ce2))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 9f059602-7b5f-4d19-9293-7991f24ac557))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 049babfc-7643-4fb4-8ccb-19423c604046))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 3bfc5a9e-9c2d-442f-b6ee-eb7d222cdc76))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp e6032fbe-8545-4012-85f1-35431e12ebaa))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp f125338e-b4ed-4f70-ae23-d38233e86020))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 35d2343f-b7d6-4cb1-9737-ed8a9d1e189c))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 5db85d67-8c8f-40b5-88a8-d7702157031c))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 63bb0e26-a3ab-45a1-8dea-c453b08ba504))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 6bc8db1a-19fd-4ebb-b0d6-d7d2cc4f39f2))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp ba125761-3316-4f13-a904-c7c4d34cf79c))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 0f52deab-fbd1-4237-bd48-b364b82c9220))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 94d4ea18-12a7-4775-bea8-c4aa302596a7))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 04f5e42b-efae-444c-96df-a2809cf5206c))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 3af99b0f-b64b-4839-a145-eff04622e95f))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp c90e05f1-845b-49ff-a5ff-632b6e493572))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 642dcd58-9cbb-4cff-bce4-a61e9d1b3912))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 690f7826-e55a-47e7-9149-776663bb4722))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 3d169365-9f6f-4736-90ac-3f71c34555f5))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 7e56c17a-e250-4674-a335-a07c1d26d709)
    (at 45.705 124.485 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/b8d83914-0438-4fa3-8570-97a47796af50")
    (attr through_hole)
    (fp_text reference "JK17" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec7ba6e9-706f-48bc-9bf3-0aa8a7296a91)
    )
    (fp_text value "COL7" (at 0 -2.555 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7b0b9e9f-b7db-4e23-b6f7-a478520df1d4)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a2abe392-0890-4e93-8b86-e15362369e61)
    )
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1e1742d3-82fe-4be4-895b-261fae1f3c9c))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 307cb7f7-f927-4c76-933e-59bcd7fc3a22))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 4e530985-c9c1-4b15-ada0-b1234d152643))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 76f68b18-fc7d-4be2-b12c-66e2770ae749))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 98c0f8b3-1901-414b-af86-869b2ab40387))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp cab2066d-c003-4e69-bc39-2f4edddcefac))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2fbe68e2-68ec-462c-aa3d-e1abd554e668))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 89ff669a-4b1d-4d57-a72e-a521b472f0d5))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp ea26e7e7-9f6b-451c-9f50-03110e076d97))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp febe3154-0db4-49fd-ac9f-d9a888436a0b))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 273c0b90-148e-45a8-8f6f-2c2ab53b725e))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3e9f35a7-a9e9-468a-a04e-12591f3bf20f))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 49819e4d-f38b-46dc-aba9-2278b7c30508))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 7187af9d-ab36-44a7-9fbb-00293559c62d))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp baf6cf17-83a4-4f18-bd63-a4cdb7bc82dc))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 031eb1d7-d1d9-4f4b-983d-0672a0b9b149))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 9a5723fc-0029-4ffa-b6ca-7b53296397a2))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp f98d8754-c464-42b5-8242-4019ec32e431))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp ed3b56a3-e420-4cd5-87ba-a5e6119f12c7))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp f0caadda-19c4-4109-8f5b-0e8e82d3002e))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 595897e4-690e-438c-9e16-b8968e11750e))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp c1c07011-9684-4a86-baa3-f2da39be2f0f))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp b4cd7ba5-2e9c-4b48-9a8b-a603d392d4b3))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 82f33847-5620-4941-b353-3868994451d0)
    (at 147.32 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006201039d")
    (attr through_hole)
    (fp_text reference "DKD1" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16791da8-26ff-4587-a8fd-865bdd7e318d)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ac1247c-3cdb-49fc-9243-8937645c77bf)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ffc1326-aec6-4ccd-957e-22afb40b67aa)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 884e032c-0971-4946-8284-21580768b471)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 91f0d3df-815c-4649-9c9a-d7078977a8da)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 82e551bb-2487-41e2-9775-7ac06072aae6))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 47717b47-93cd-4717-badd-07358d38f284))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 196f778f-21c7-43a6-9246-9ceae30519d0))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 49e55b7d-0030-415d-ae07-7742a8a31aa1))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 75ce9ecb-ce57-45aa-8b15-1f8179522961))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f97ce341-5c3e-4047-8cec-4609f1e49bcf))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp a49d19ec-efba-4070-b3df-50d646c82fc0))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp e53f76ec-84c1-41d1-9a71-60ef9bee1457))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 066ca134-f26f-4795-a23f-526d6e62a933))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(DKD1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 641ea8da-dd84-4788-8b8c-bc0acdc6af6c))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 87aff286-2e69-481c-9559-5aab153e1d8b)
    (at 172.72 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681596b5")
    (attr through_hole)
    (fp_text reference "DKD48" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c102341-2f81-4226-af10-89fed58378d2)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 131bc8d3-e8ca-456d-84a7-0385748e1b9c)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0d1f45d5-e0ce-4696-a9b1-ef34a84371ee)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 126c8462-51bb-497c-ba08-14a803d0a674)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19a81270-043d-4c41-9cd4-8029dbcf653e)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 5806cb81-88ef-495c-9bfe-aac8af85c6ad))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp ee20cff8-9076-4d71-9010-6d3a4a592e6c))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 11d689b4-5907-49c8-8ad1-961d87f3733a))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 60f119d9-cf4d-4412-a477-2078a4c3f1da))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6797bb26-ec48-4254-afd6-950b15eb89eb))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e6df77f8-8c8e-4fdd-8d6d-7beb92f86a10))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp e6dd9a45-b6d5-4c57-8f6e-c2a523e3ea8d))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 54861bb6-f020-4421-9648-b76324a687a2))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp c1261327-f154-4d54-adf6-8c3c2808f779))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(DKD48-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2fb2e70a-6f42-4f80-95dd-a3656e07e317))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp 8a1736e6-6862-4e8e-8e5a-db85366269d8)
    (at 45.72 109.22 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/05daa335-54bd-4d79-af6c-b601f9f5818b")
    (attr through_hole)
    (fp_text reference "JK11" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa5b8c91-5987-42d2-aee2-e6e34fe61b11)
    )
    (fp_text value "COL1" (at 0 -2.54 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04b6e096-a911-44ae-9e10-ae475098768f)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3007a75c-c42d-49f0-9ee8-607587317630)
    )
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 0250ad16-fd32-4326-9cf0-08164a20aeb5))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1c454584-c019-4ea3-a3a7-55015d01b782))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 23fae061-e9e0-4f20-bc16-9d7094b709e4))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 4b1eb16b-02c6-4cff-b4a4-c2cbe5885442))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 519f64c4-36a6-4f65-8e4b-e39a95fcad7f))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 5d5d903b-9080-4ea0-bbb9-3a14aa388097))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 4942a16c-350c-4cc3-b6d6-034e51735bcb))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 4c18b21c-df55-4b1c-b514-ab1015f3c674))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 9c352ce5-8dcd-4676-8f85-0d97597fd098))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp f142eda0-0816-4e1e-90cf-3664d7d377c7))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 2f01a09f-3b40-4211-8f44-414b31f601a3))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 6f866dfc-46da-42f0-b96d-1fc7f081b832))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp a198bda7-be5c-4500-a7af-192f2bf9c4be))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp e9bf2310-d776-4451-ba9b-11c6767ed223))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp f27d5be4-66ac-49bd-b481-775213af8981))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 2543cd22-a280-40ad-8a48-6f245d4f3128))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 91abda88-a077-44a4-be08-64ddde98a781))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp f7edba16-03fb-48d4-9ada-50a21353a670))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 83b50757-cd58-41c0-bec9-21d155cfd7b1))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 9ee8beb8-098b-4f7a-b56e-7834b8c10924))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 4194b4a0-f335-4ad3-8095-b9ef0e2282f2))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp ce779216-9b0f-4bbe-9db4-258749d7fe63))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp fb379631-96dc-4030-bba3-a9f12c023051))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 925145ea-5336-49aa-a6b3-5e45101c9006)
    (at 157.48 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068153234")
    (attr through_hole)
    (fp_text reference "DKD35" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 06ef91a0-bf30-4751-a8ac-5bee1fe1260c)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c37261d-d6f4-49f4-8f43-f15a3c8fb7bd)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 759c546b-c0b8-4a8d-a3bb-e487d2114970)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2afbc569-6ecb-4c25-9a76-3ebcdcb03ab6)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba2900f4-331f-4c0f-a55b-65da04d4f1b0)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp dc174ff2-66c8-433d-a01a-35688cd69e3d))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp ed0856e7-f85e-4982-84b2-b4c386a99d39))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 079a1d16-7ef7-4795-ac36-33c7038dfe67))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 35ce001f-336b-46ec-83e0-7e551fdfc10f))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3e3bd1ba-472f-4699-a47a-e5cc27e49b74))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp c12686dc-96a3-4e76-ad68-768f524367a0))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp a4bc7ac7-fd41-4007-8ff1-d35c18085f3c))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a23ce614-3dfd-4906-b174-a8150dc0dc37))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp fdb09952-63c7-4906-963f-f3fbe4fa66ed))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(DKD35-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 7dc59c13-d669-4228-a9aa-25c20e0a7c65))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 951a2e06-c37f-4a26-bf5b-40c91f1ef735)
    (at 147.32 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681428ca")
    (attr through_hole)
    (fp_text reference "DKD3" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 45695b2f-766e-4063-b6e5-15deb791d27f)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp edcfaaa3-3b3e-423d-a56d-4cef558b58fc)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4163eca4-fb42-4c24-a9ed-844ee273630c)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19b664b8-b715-44aa-84f8-ca5c96ac1a6d)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf35d99c-a8b4-4400-91d4-0d338fb1c0cc)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 093f5789-7a3c-45a0-97b5-c12d836a868d))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp dbc797ee-5c33-4aae-b8e0-4ffddcec9594))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2af7e455-0c97-49ab-a9e9-0ff2ebcd666a))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3f6f45cf-b97c-4c47-b6a3-bca533dccfc8))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6696f3bb-5718-4e18-8e4c-ee3b65432b3e))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e35e6077-74f7-45d8-8dfb-ff5bd7de790a))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 03eea94c-f208-44d5-b7a8-4939ed604e02))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 88db3832-8cf5-48e1-b5b1-5260c3666ac4))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 3597c40b-b20a-49da-acd7-9e749a9dcca1))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(DKD3-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 21c4670b-5350-4467-8b6e-a603aafed2c5))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 96ea7aa6-700e-42b4-bef6-e684a17d5aa9)
    (at 35.56 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/8fbaf924-d871-450e-a1f0-30fbf0262d25")
    (attr through_hole)
    (fp_text reference "J26" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bd66e6de-b853-4de2-bf42-06831b49fe08)
    )
    (fp_text value "GND" (at 2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61446f17-835b-4791-9188-67c3e22457bd)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 23b1c6b7-24b8-452a-afee-8dc8caa001c5)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 232c2654-a24e-4679-a9c5-8a14111d3a59))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 330aa160-0dcf-4d86-b12c-6facdce00691))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp a067e2a9-2168-4a75-b1ae-07175f3097e7))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp d00d473b-dbf2-4046-9ca4-13245b851c7d))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp e35f74da-1ad9-4cb8-ac48-b4ba064240a7))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 0f015f70-b9be-4792-8502-9235baab7ad3))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 58bcb7be-d6fc-44fe-98cc-4ab651432282))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 7ef98de2-0407-484c-b75f-d3f0938f17b0))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp cf9b593f-7152-4b36-a501-419aa3f30746))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 0b8acda2-e6d4-4de7-b591-ea0c9b51fcec))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 7af2ff61-aa57-437e-b3e4-6de63a8458e0))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp ba7195ae-a1f4-4965-82ea-89d705092be4))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp c3c02496-b038-43f1-99b8-409718a4222c))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "/Rotary Encoder/GND_ROT") (pinfunction "Pin_1") (pintype "passive") (tstamp ec3e67b0-4243-4656-a7ba-dca7a98ee1e2))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 99a7cfc8-5cbf-4d9c-aad3-f866de8a288d)
    (at 55.88 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/54238fb1-8778-4633-862d-fd76f64f1725")
    (attr through_hole)
    (fp_text reference "J20" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 86fb7087-6ba8-4b85-b696-07c14f0a9fb5)
    )
    (fp_text value "A7" (at -0.025 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cd7002a5-dbf1-4947-bf07-b7ae28be3b4a)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b1bdb303-cb9b-4bc2-a172-da9546d29135)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 51e52e2d-6785-4c86-9dd7-8aebf7924453))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 6fecb7b3-ef3d-4da6-9d91-57f091c44310))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 82b4e16b-220e-4644-bf1c-0c096f491472))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp f239c5a8-dbfe-4237-89fc-56c709be30b1))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp f80c9353-1371-4ac2-a3fe-3c48b88b02f5))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2a1e126f-a9a5-414b-9647-9870ac9981f9))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp b6456347-a8b0-4beb-be5d-c94cb7d030d6))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp cbfed367-b5ba-46b2-9266-1ffd7189ad3b))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp fcd784d4-f3bc-4084-8a2a-7b74ccc9478b))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 18dcb17a-d81c-4b8b-8db2-863005a99fab))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 26a15f37-7ac7-4448-bfb4-f78a37fce015))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 28717230-cde2-4374-9345-a50192a67a85))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp f054547f-18bb-49fc-9aff-91e047769f87))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 157 "Net-(J20-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp b78043a5-7a02-4945-aa76-579ca8313cb9))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A41D) (tstamp 99da0a1e-0e84-4a04-92fe-5e54b8d4b54a)
    (at 86.36 53.34 180)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/bab30c98-c3b3-4ca0-9d1a-b0d48653d0d6")
    (attr through_hole)
    (fp_text reference "J101" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dda8e3dd-fc80-4d77-bcc1-06f659359b79)
    )
    (fp_text value "PROMICRO_13..24" (at 2.54 13.97 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 103946ef-af65-4091-9578-f66107223270)
    )
    (fp_text user "${REFERENCE}" (at 0 13.97 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4fd6e862-1863-41b5-b1d9-a2a116ad20f8)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 254e8c87-910a-4feb-9f38-804ef4baa30f))
    (fp_line (start -1.33 1.27) (end -1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp 51cded6a-441a-4c31-8dd3-290886b14e37))
    (fp_line (start 1.33 1.27) (end 1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp 85e5e533-fab6-43d3-b676-c013a2e7c8f1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp b2880886-3163-4bbc-90ce-28f264cb3452))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp c046b272-7b5d-495d-a49d-1978d8023238))
    (fp_line (start -1.33 29.27) (end 1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp f50afc37-29ff-4cf0-8193-a2f633fb33cb))
    (fp_line (start 1.75 -1.8) (end 1.75 29.7) (layer "F.CrtYd") (width 0.05) (tstamp 47effaa2-8ca2-4524-8e1c-504f7ab363c0))
    (fp_line (start 1.75 29.7) (end -1.8 29.7) (layer "F.CrtYd") (width 0.05) (tstamp a21670e4-69bd-41d5-8d7b-b757e83ae086))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp cde19217-d20b-4ae2-aa87-cc7435946b2a))
    (fp_line (start -1.8 29.7) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp f52c67fd-75b3-4a43-b37c-7bb928d7d776))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 25cf6790-6002-4f51-b267-fe556bb7b7d3))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 51fe1480-9615-4473-8228-167720ee011d))
    (fp_line (start 1.27 -0.635) (end 1.27 29.21) (layer "F.Fab") (width 0.1) (tstamp b3c6f4a0-5616-4f4b-932a-a5b210dba5e5))
    (fp_line (start 1.27 29.21) (end -1.27 29.21) (layer "F.Fab") (width 0.1) (tstamp cedb473e-d741-4b3b-808c-68af5a994df6))
    (fp_line (start -1.27 29.21) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f252c2b8-f699-49cb-b9bc-50cb2b4dc531))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/ANALOG_MUX3") (pinfunction "Pin_1") (pintype "passive") (tstamp b6a0e2cc-6470-42e6-8fc7-7d13008aab27))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/MOSI") (pinfunction "Pin_2") (pintype "passive") (tstamp c9579104-4fae-4c02-bec0-4cee67f5eb30))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/MISO") (pinfunction "Pin_3") (pintype "passive") (tstamp d40b6bb2-2a99-432f-8863-c2eb8b4a7574))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/SCLK") (pinfunction "Pin_4") (pintype "passive") (tstamp d2975d44-6d67-4b97-bf23-c7bbde3a37ad))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/EINK_SEL") (pinfunction "Pin_5") (pintype "passive") (tstamp 0ee5baae-4e7b-4931-a754-859b41caeeea))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/ANALOG_IN") (pinfunction "Pin_6") (pintype "passive") (tstamp 696d07ba-1dd4-4ad6-9158-3708596bab26))
    (pad "7" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 164 "unconnected-(J101-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect") (tstamp 3fbafa68-5f51-43ec-a208-fdcbb1459461))
    (pad "8" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "unconnected-(J101-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect") (tstamp 3e4d4dc3-33d3-49bb-821a-0af699e5324b))
    (pad "9" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "Pin_9") (pintype "passive") (tstamp 3fab6383-99f4-44e8-8559-bf502a3a3a5a))
    (pad "10" thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 "unconnected-(J101-Pad10)") (pinfunction "Pin_10") (pintype "passive+no_connect") (tstamp fe0b7838-4162-40c1-add0-633fd96edbf8))
    (pad "11" thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive") (tstamp 9e4c940a-92c8-4190-8df4-bbac20c26440))
    (pad "12" thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 167 "unconnected-(J101-Pad12)") (pinfunction "Pin_12") (pintype "passive+no_connect") (tstamp 04f0473b-2ebf-410c-a50d-a457aa35ee6f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 9a9a9126-af36-4978-8831-60bd27caeff5)
    (at 147.32 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006816009d")
    (attr through_hole)
    (fp_text reference "DKD61" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 140cf9c8-0981-4fc7-bdca-12efd18defe7)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e64e461c-7746-444c-864c-1461e1fc36e6)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30321038-7c9e-458b-806e-4cd15b590f79)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f2f3ff1-a451-4f53-86a2-b2f85c378993)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ffc3f34-79d7-4659-b92b-72ca5c57db2c)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 4664263d-8684-443c-8942-67d3d2a8a601))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp ef0a1d4f-2862-4595-ad45-6e142e95bb7a))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 326c24f0-8a4b-498d-ad55-1bd64e295841))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6f10aa5a-83f3-444d-87f8-603ad7d62493))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp dad725b1-ca8b-4ef3-9412-c059bfbfa20a))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp e2283fe3-101d-4361-b181-a6b0a9b9348b))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 1d0932c5-589d-4904-95b3-285d1c0cdfc0))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a92a43c1-e404-4deb-96f0-6762773e35d4))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7ebe66bf-81f1-48e2-a41f-b6b2d3ac5cb1))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 147 "Net-(DKD61-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2bd811fb-3e2f-4c44-baf1-5d8aad0740b5))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp 9b547084-c7e0-40c4-9e5b-1b70bd77fc6f)
    (at 40.64 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/2c4dff0e-97cb-430c-b06b-cd8446c042f5")
    (attr through_hole)
    (fp_text reference "J37" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12d85746-843a-4457-8a10-3788392e76c7)
    )
    (fp_text value "R7" (at 0 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d2c92adf-1fe1-47c3-8ff6-f267b017628c)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0685f3a-590d-4608-9d26-146a166a084e)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 09c82046-ec4f-4d8b-a599-623eb4c90e55))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 23319b93-8872-4015-ae92-a25e2d30ff15))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 6b2547cf-2adf-41c4-a4a8-d1cd26b63aaa))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 75db9b73-547b-44b5-91e6-0aadeadd89fe))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp e6d29fdc-66fa-405e-a61e-768cff1fe41e))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 9f4d031b-bcae-4d2b-b4fe-e555a7a445f4))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp b161d14f-f972-4c9e-bb89-30daef53ccb3))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp cd0b1421-5548-41b7-bf57-1c2cff9a030f))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp f78d2c25-640a-4548-a027-472fc3511f21))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 9a266aed-18b6-4ff8-a7be-7791928bc708))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp cd3fa90f-5708-44b0-ac6a-8f9c3f18de22))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp edf90760-7f2c-4758-b79e-4873fba75358))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp f323c458-bf9f-4d9f-8f08-814ab4ceef0e))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 176 "Net-(J37-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp f356780b-7769-4a78-85e6-e1375ee9b7a4))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp a020398e-a550-480f-a3f6-334f08c54d17)
    (at 175.26 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814fa64")
    (attr through_hole)
    (fp_text reference "DKD28" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b7fe77cc-e089-47dc-94e1-e996d8e680a7)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7dc2f3d6-5033-4b4d-829a-a52cede6143e)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 296c06ad-4adf-4afb-bc6b-1f9f84a65ef6)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 377fe22a-1b4e-483c-afa7-1e20aa663909)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6616844-0115-4ac1-8b5e-5f2d3925e36a)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp b3bbb060-2dab-411a-b9bc-a8fe9195e809))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp f92ee491-0b14-4f52-bf57-1ae4bf7a406c))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 83eff285-d016-4256-92d6-54fcc8dc4a64))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 8787ef8b-f2cf-4bb9-8cf8-cd9fff165d92))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9fb6868c-d1fe-461c-af70-f516ee84379e))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp df816362-2c24-48cf-bcd4-e6b314b250f6))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp bc080d7a-d040-4c72-bfff-4d2ce65e8cd7))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp f4fae871-28e6-44e3-80f9-ff97dd0dbb35))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 295dc4df-72c5-49c3-8858-fa4ce446c815))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(DKD28-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 7f2c923a-5ed1-4707-b050-9aa1614f67c9))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp a3c1a97d-5474-41fc-9bcb-837360527251)
    (at 55.88 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/cddd98ec-06b3-4b4b-bd3e-77cb1b75197e")
    (attr through_hole)
    (fp_text reference "J44" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56c9de1f-b590-406d-9440-c897fe15152c)
    )
    (fp_text value "C6" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e9543f3c-cd46-4dbe-9725-9e4f6abbbc7a)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f0b52b7-1cb4-424d-af8a-799a42f4f1c1)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 8d4e2929-4411-4597-8c87-8dcb1df47ea0))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 8e943e4d-bb7a-4187-9536-b7c28ba62816))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp edb6c311-a95a-484f-aafd-726b7f62accb))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp f7fc9e09-f875-4f17-a255-8cec9b248a05))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp fd5dace0-f317-41a1-b7d4-73f491b500e4))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 12dac358-e34f-4cdd-a0b9-24c9a009f82b))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 46755be3-b815-4af6-a3d6-85e2c83d2780))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp e5dd8363-7d79-4f98-8f67-10ab4e3bfb29))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp fd19f347-1055-40d5-b762-4b48fc48e586))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 054e2bd1-40be-432f-b01e-7eb877390200))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 21e40f47-68f1-4e6b-b41b-96c38b453398))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 7bc878bc-9fbf-4d8d-a5f1-fe6c257b39d9))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp b5b57aaa-3fb4-417d-a10e-9199d42e1eb1))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 183 "Net-(J44-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp ebaca5cf-ad9e-4eb6-a6f0-8116d87b1f63))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp a4257c70-fa6d-495c-99eb-48dc07d98831)
    (at 81.265 124.485 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/9d8821d5-4a46-42af-bc96-ab0db55e6097")
    (attr through_hole)
    (fp_text reference "JK2" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c201b801-be57-43f1-9ad1-189ee6e7bc11)
    )
    (fp_text value "ROW2" (at -0.025 -2.555 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cd687d4b-472a-4b2d-85ce-917f03a73835)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 200427ad-2832-4dbb-9227-2f456bd31af2)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 064d2ceb-ed0a-4fc8-8669-798ae2c1911a))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 15818e07-2620-497d-920e-c0f3fa45c878))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 635d3d46-da80-4ae0-a469-28a4a14fe2cd))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 69ed7c81-a952-4378-8357-76c9747c83f3))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp aec4a5f8-dea7-422c-a852-5566f47c7f4d))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp e0d78f56-637c-46d4-adb7-54ec9ed9a717))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 25ced3de-676b-4ac0-9053-fc67b3d03691))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 301bb7bb-5f67-4a12-9750-89181d549b6f))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 667a6064-da95-4136-b19f-3d95581483e8))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 73c6a740-f6f1-4f8a-b454-3005d2b89391))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 116dfe6d-587c-4dd5-a481-7afc3b428ec0))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 12ffd6aa-0f30-4629-a970-b081b41f4267))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 82867bf4-f706-48dc-ab65-fa19c1c7efd9))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp cffb2abb-c1d3-43d1-a481-0af242966521))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp d336bb33-8551-45e1-9a37-39a5964e22ad))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 43706053-4f4e-461f-b054-7f5de6dc0258))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp bd08beb9-5319-4ea5-bcca-5d8f756c28f7))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 3e36d46d-8471-4871-8ec9-6da665345d8a))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 9bf6eaf0-8b37-4e51-b5e7-a2be99b52b96))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp b3179e89-cad8-48ce-93ab-34954f0b69ac))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp ca2dd9ba-0ecd-4f8d-808e-d875ef4c56c9))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 9907ec5f-30b6-4f70-8109-7a4eb7e28e38))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp a3919a37-6c0b-458e-808f-5709bfa0fd57))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp a57f6de9-743d-4ea3-b8e2-8c4602f7a501)
    (at 165.085 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814449f")
    (attr through_hole)
    (fp_text reference "DKD5" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5776b2ca-7c7c-4c8e-8501-5ab62022c76d)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0cc6721-d0a2-4328-8749-2137fe533d3b)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b624ddb5-5af8-43cb-a5f2-0319c9312004)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 082f0b3e-128f-45f7-a29d-0862269a686a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14a7e9b1-064c-43d9-8beb-d8ad17feca11)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 58d8d163-4406-4eac-8f10-4c2bd893084e))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 4c138c33-a47b-4828-ac69-8f6266c97dda))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 673e6a52-45a9-4a6b-a74c-d3217773284f))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 8d03fb71-5ea2-4daa-9dcc-86b162aaead7))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b8a30f0f-19f4-4d4f-85b8-7af0b4aada4a))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp d24ccd92-829b-418b-b2e2-3780d3fef4d5))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 84274e7d-bb6d-4080-aac1-80fdfd8e41c3))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 6ef3ac1c-3572-4c02-8291-b3ec77bba728))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7f611165-6a21-48b1-b8ed-eccacbdd06bd))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(DKD5-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 7244a769-5e3a-4d57-b1f4-47af8df7cae9))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp a65de6f7-a57d-4433-8d00-2faaf28702a5)
    (at 53.34 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/92529218-3086-4e38-a5d7-361f20edc13a")
    (attr through_hole)
    (fp_text reference "J8" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 34123646-538f-4d29-99e3-ef929983a259)
    )
    (fp_text value "A1" (at 0 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 792df31f-d7c8-4ab7-9004-848451dfcc4f)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c3d52d09-a3df-4a1f-b4d9-6c9229ec3718)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 403f035e-89c7-4267-bc39-540407f9432f))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 5112e7ff-94f4-4953-9b3b-e89ab066bf44))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 633ef1d6-5811-4caa-b46b-b2c44b20f0ff))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 8a26463c-6132-4640-81bb-e4ad34aa7d3c))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp a682d36d-28f3-4c0f-8f71-912aa876dffd))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 291d9785-819b-4ab3-8871-6887bb427f84))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2e74c5cf-df21-4ecb-90c2-e2781152c95b))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 5f30f18a-2eb5-4274-9d3d-af9601238118))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 91d720eb-a86c-46fd-9f6a-0dddf20bde1e))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 72596630-6f62-446b-a788-e57836f8a3c1))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 744bf9ad-3201-4631-b4df-82ae02271ec9))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp bac0882a-cd95-40e5-bcae-36dd00c1e400))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp dfcdf09d-9f20-4402-b580-09edd237e4fb))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 77 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 08def91c-96a1-4452-a029-3015fe0a2365))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp a7fe22b6-b84d-4572-88e2-d53a39988d8e)
    (at 177.8 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068150a01")
    (attr through_hole)
    (fp_text reference "DKD30" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9eedc8f7-9afc-49e7-8979-1bbdc40da357)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa97c6aa-4a29-45c2-a54c-e9082697af78)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 564c12e1-207b-44cf-ac13-5c637ab497bd)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d355dea6-fa8d-410d-b8b5-0a9a351f0246)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9096fe7-a504-4634-afce-f3c31e0300b7)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp dba17e5a-514a-4dfa-9594-6e27a43c26ea))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 7b251fe4-fd26-47d2-a7fb-7dd45aead396))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0b60267a-30d3-4059-a071-7684b08efa2b))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 28629766-01ab-43b9-9a60-80195f99c100))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9601acf2-3d42-48ef-92c7-a5a43be4a695))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp fd379091-f1d6-46c6-b404-7a9d1a5b7385))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 22c6e7c3-1f3a-4a12-8ec3-00e728aeb8e1))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp e31c92f8-7cba-40ba-91d0-030c8fe6c8e9))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7b2697b3-96c6-44a3-954a-9d19e7c775e4))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(DKD30-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 83a3af19-7776-4e24-8de3-5533f96e55c0))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp acdc19ad-2d03-410d-b428-0229e9757c86)
    (at 58.42 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/7ce8fcd7-ee6c-4af5-92da-5d397d1d555e")
    (attr through_hole)
    (fp_text reference "J30" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8714ff81-a855-4fd8-9732-ddd502df00a1)
    )
    (fp_text value "R0" (at 0 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6d55896f-2f3d-4bd7-8b5b-85ea2c518d49)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9da609b7-fe60-47f0-9e40-40a42c3997d4)
    )
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 0ad3949b-21ee-431d-8d86-3c3c8edfbc61))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 1f7abaaf-d23f-440b-adc3-25bac38bb936))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 20268fb3-13d6-4179-98d2-70291583fa2c))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp b351138f-c54d-4626-955e-d86ccb154148))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp ba49fd39-28cc-4fca-88f1-a37cc4f98a46))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 0f08e558-7e5e-4c1e-8503-d96b836058a3))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 3e6b8f5c-7f12-4d82-8011-dc1fd9fd0356))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 625bf30b-b634-48aa-91f7-ca803f4966c9))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 64704956-2983-4ef9-bd08-b61b254129f5))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 6103885a-aac0-4142-a439-da65bb88a09b))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 718c6bc9-54fb-4902-b091-b75900fbec5d))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 71de7f86-b4ed-4815-8f13-085ef513c926))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp aed21c63-9316-45e5-b341-4d36629d2fb2))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 169 "Net-(J30-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 37f9345c-43b6-4e31-8280-acb94755535c))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp ae0fff6a-54a1-4c88-a6a0-552ae2b18136)
    (at 119.38 55.88)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062e52366")
    (attr through_hole)
    (fp_text reference "JKD7" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca20c5c1-29f0-409d-bad9-37dcf0fa9ef3)
    )
    (fp_text value "ROW7" (at 0 -5.08 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba0090d3-a7a1-49e2-a590-906ddd61ff9f)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e875cb46-6950-4eed-801b-a157344ce867)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 089ae691-dbe1-42f9-9b31-bdc55bb4b595))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 2b0b632d-d56f-4a16-976f-8d00021b3991))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 6a063219-484b-4436-b72b-d432daf66d0e))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp af670862-df57-4be0-9dfc-d82ec0c8a1c5))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp bf4af012-4f5a-4de5-bbcf-c7cc6c0daf78))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp f10a25e1-4c3e-45f3-808d-b580e4dc8e9b))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 42ae335f-b709-4546-a2e1-a54b154efab0))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp a38802e2-988c-4024-b848-df9268f6b39f))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp d8bd1f46-f49c-48ea-8f23-af08fa4429c1))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp e24b9d15-43fc-44b4-9d98-3c2417407b4a))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 10f0f962-fb7a-4a69-8263-217fd21b0a75))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 5310a858-61e1-4b29-b2dc-acef324eee04))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 88961251-ffd3-4d93-b9f9-6d97e92ce245))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 8d344cb4-b973-44ec-84df-d5885de46933))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp b1e864a4-8bb2-4ddf-9752-dcae0eea7f90))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 5949d15c-454e-4973-ad53-7637d691c575))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp aceb672b-2dc9-4a62-8afa-639a7712a31a))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 5c1c6608-7251-4e13-b32d-bc3a0ab8f2da))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp cdbb78d9-a18e-456f-a84a-2678a8a54ff6))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp a25e9992-f4e5-4b4e-a91a-0cc827b063f8))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 519c18b4-ec92-4dce-bb96-cfe57cbf5d17))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 3a23b806-c20c-4504-b6b5-6d7ffd433f46))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(JKD7-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 43ee2970-62a9-45da-8ad5-93c0e2a572b5))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp aeac112d-337e-41cb-9c53-71307713cf77)
    (at 170.18 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815c5d8")
    (attr through_hole)
    (fp_text reference "DKD54" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e76d7b86-9e83-4454-b4c8-213e6f7e816a)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0c566a0-77cf-4af2-9966-bd4d4fe30ddd)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3367483a-6bc9-4c36-adc8-7463eb43c425)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1aa04eba-76e5-4f9b-a7ae-4563a38e7b07)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 59f07814-32d4-436e-aa41-2c8764444c8a)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 6cc72c89-b49d-4422-b991-62fad8863454))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 08ef0b28-bd0c-42f1-ac0d-81b417611f02))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 597592b8-da38-43a1-92a5-65c1669049b9))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 81455f9a-94e6-4671-aa8c-06efac3e188d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 90449114-054f-41bd-82de-d9b346041ad1))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp cd723210-2d10-45ae-825a-bd5c3d886654))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp c7cc8a27-c7b3-4c3e-9d7a-afabe62ad290))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp f39d6152-3b51-41c9-a787-9868acd9e83e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7d9408d8-8ed6-4f7c-b509-97ffc2da581d))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(DKD54-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 5585520a-1aec-43e0-8cd5-a3feb8e0c4eb))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp afaa94e1-65c3-4b6f-9c68-5ac59bc472d1)
    (at 170.18 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681487fd")
    (attr through_hole)
    (fp_text reference "DKD12" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f3230268-1aed-4b00-a493-d153e3ff0827)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d09e516-5380-468c-bc06-247967e42a14)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7a024c1d-7d04-4892-919c-7130e771bc02)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d206aff-6fd9-4bbe-a6e6-2b006f63b7e1)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c54f2b88-6876-4157-b720-3f2686820092)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp ba4d84c5-7efb-46fc-9949-eae1d09c5308))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0a0032d9-6e5c-4480-90f9-0dcb5afdc86f))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 60711925-33c6-4d4e-88f1-05072edf3f9d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6ba4c624-cb5c-46db-9104-96b9b43d31c9))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b3159aba-444a-4e87-bcb0-a783b954a9e6))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp d64f152e-d8fc-4064-a5d7-53d32cde16b2))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp acf41fca-e289-4843-8917-96dd8630e43b))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 17546b63-a656-4e51-aca8-b92b92131d44))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp bfc9e505-58c1-4c7c-884c-7553b191d3fe))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(DKD12-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 175924a7-69f1-44f6-9144-78e34b9a371a))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp aff73507-4f3a-4fb5-a966-c2bc3ad0d300)
    (at 165.1 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068144fb6")
    (attr through_hole)
    (fp_text reference "DKD7" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c623e9cc-f90b-4fe4-912f-ef8305c4db20)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78a1f4c8-86a4-4a49-b709-c945e95ec6e0)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3ad910d9-e991-42f6-a40d-ba55015c61db)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d39502ac-9c2f-455b-935b-6c908072e0fe)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp debab658-2a37-4a70-ac55-c704f10a0ef4)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 975c79ca-0646-4c44-a9b9-a4fff59f6994))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2a15fe61-2256-44f7-8b98-e52d21928fdc))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 217bfe9c-cddb-4ff7-b9a3-dbfde59e657b))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4eca3929-f3e4-4f8c-9817-1423b3d63370))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 7bab4640-d653-49f3-8eb7-4b4566874d1c))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c6b1aab8-f288-460d-b479-e26cb83b4fc1))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 3281e759-45a1-47c2-92ca-6b2b58c66601))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 7f45c2b6-8de7-4371-be6f-6ecb7f9fb618))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 74d3ac9c-6ed5-4cd0-993f-71eb855dc22e))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(DKD7-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 02dcb8e3-f451-4f24-a3f3-f266079c76ab))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp b00b3f89-5c5d-46b5-afa2-7a55e245664f)
    (at 167.64 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814222b")
    (attr through_hole)
    (fp_text reference "DKD2" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e75e582e-01ef-4b14-b0c5-66f381043f61)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 25d40d69-6800-4c53-9fa9-c091deabe046)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ab93736-0a20-4c0d-bb92-79c6b2f6de3d)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a6dce6f-7bd4-42cf-b0d1-534d59cfd2c4)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c9d99ed1-bd1c-49dd-a522-9221961156a4)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 0f948b6a-1741-4240-ad7b-29377405f2c3))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 7d240446-854a-4c36-a53c-6ac4a11ee32b))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 236b6e46-a264-495e-b625-e0e7865f028d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4c348dfd-59c2-44bb-a25b-5bd07025c373))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp a39819ad-c3fc-4f7f-bccc-7cb70fa2c87b))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b7b6156e-1468-455e-b8dc-dc10b8d799ba))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 46d89aba-d23b-4eef-b626-f77d61617c5d))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 3b2de860-7bff-4d14-ba3c-a367c07b8499))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp df3ce918-12b6-4a76-80df-c3d0e87ce079))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(DKD2-Pad2)") (pinfunction "A") (pintype "passive") (tstamp c96ae41b-52ca-4741-afeb-1785e674f144))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp b10e55e0-16f5-41f3-8599-86a4305b27b4)
    (at 185.42 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815edc3")
    (attr through_hole)
    (fp_text reference "DKD58" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 42f494a0-47c8-45e5-8a63-e37ff542165c)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0826d1d1-b618-45c5-a646-c0cdc1c4c5c6)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9f695e5d-e696-4aec-a6ce-74a0ccb54bc4)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 23d76785-0af1-4d2a-83f6-9e6efce3b336)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3dfd7fcd-5c10-44d8-91db-3057b1f086a8)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 98043ef8-a951-4755-8580-a3d952a02a78))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp f5d7765a-6532-40f1-8f3a-b6fa19a55e3b))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 35807b19-6e0a-4ee4-afdc-1a4db2f3ec29))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 58057263-17ad-4ee6-b85f-6a4af8f40dd6))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp ba21db68-662d-4d89-8919-0c8a01e04c57))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp cc93644d-ac07-4385-bb9c-f3e082f8c543))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 7c791c15-efe2-4a63-9b5c-a971f7cb16df))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp bb9a0d15-95ab-4530-9c76-9e54445335d9))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 9423c896-00d8-4fcb-ad20-391995e30040))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 144 "Net-(DKD58-Pad2)") (pinfunction "A") (pintype "passive") (tstamp abe6968e-6a42-4605-aafb-6962fdcc88ed))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp b2cee2f5-c93b-431e-b6f8-b5af11d8cc19)
    (at 152.4 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814b941")
    (attr through_hole)
    (fp_text reference "DKD19" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca6c0ea8-c358-4eef-ae21-dc7ead95bbff)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e38b010c-0860-457d-91d8-f2ae5caaf61c)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa122f5f-0cb3-400d-bb47-33fd1f4c8534)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a743d17-5a81-491e-8632-b512db7ce533)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1ff0b72-2bea-4044-ab21-5375a4ceaa91)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 72233dde-e432-4cd0-bb30-5ff245709c4a))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 08c02e85-5fb0-4d46-8f99-02611a0909f8))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0dcbdba0-5ce0-4c3c-a08f-ee9c2fe3f575))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 62d6d193-bf87-489e-816e-a472033d391c))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp dbf36f47-adb3-4264-b413-55aabc40e540))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp deee72e4-b1fe-447c-a732-65e5f929845b))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 3115dfa4-c507-4654-bb62-2a981ffb43d8))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 6569c4f7-bae5-450a-a302-5c73f9351a17))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp f40a02d6-746e-4cfb-afcb-e20fdc44b9c4))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(DKD19-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 13773ab6-f60f-49e1-bb0f-a94407a1d0d1))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp b31ecb97-70a2-4071-a8f6-07e3d12d9031)
    (at 172.72 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814b1f7")
    (attr through_hole)
    (fp_text reference "DKD18" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cd0012cd-c31a-4d11-8037-22e462456f0c)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f57f4d7-00f0-4316-9c2b-eecf9fee8d94)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8779ff29-6c0e-4d78-8d31-1b171c487091)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16c6bc31-6148-4f52-a599-8d7d9c4a1beb)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8ee9a9b-066c-40e0-8794-21c37df11d80)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 3017eacb-4698-4878-b189-1d2d567ed994))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 3fc84e92-3620-4d72-b6d3-d86990989327))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3ae70b89-493e-4ddb-aa93-89b3656744af))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9d872b21-4aa7-472a-8993-61f2cf522e96))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b8075a25-cca3-4ce7-aed0-3f2ecd641088))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp fe368c96-8518-46dd-92f8-947078ac9f52))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 7fcae10b-b779-4479-99ea-cd556454773c))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp d3be0fe6-d2f9-454b-8ed8-c569dd48d59e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 8bb7350d-67b5-477f-b968-1abcfd0b9a92))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(DKD18-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 330e69eb-c1cd-495d-9a75-0ea0b0d8ead8))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5) (tstamp b75a61b3-7249-411c-9b84-f29450ac12cf)
    (at 58.42 127 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/d04feb71-13a2-42f3-bf5c-5a872bc136db")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8a40e66-9193-4ea0-bb90-6adefac55e31)
    )
    (fp_text value "MCP23017_SP" (at 3.81 7.645 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92dd96ae-7a33-4a80-a3d9-203c50aae3b9)
    )
    (fp_text user "${REFERENCE}" (at 3.81 16.51) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4b8359d2-b152-4e40-b073-6f21c63eb6ff)
    )
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 37f5f4ac-be45-488c-a2e2-ce9453b7dc8a))
    (fp_line (start 1.16 34.35) (end 6.46 34.35) (layer "F.SilkS") (width 0.12) (tstamp 74f59410-d7c9-4f10-af8e-1d8a709f9180))
    (fp_line (start 6.46 34.35) (end 6.46 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 9da5b309-0e3e-40e0-8c33-c80743624e07))
    (fp_line (start 1.16 -1.33) (end 1.16 34.35) (layer "F.SilkS") (width 0.12) (tstamp f38dd2f6-ec36-4a35-91a3-25818d4dcbb9))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp f4b5a2c3-da51-4603-b28c-bc7691f10604))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp f9e90746-5f38-482b-a4b2-8421aa7fc6d6))
    (fp_line (start -1.1 -1.55) (end -1.1 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 1eaf6dba-fafa-40a0-a924-bbfb4d5e4e86))
    (fp_line (start -1.1 34.55) (end 8.7 34.55) (layer "F.CrtYd") (width 0.05) (tstamp 96f86a62-3538-4884-bda5-db2302814bbf))
    (fp_line (start 8.7 34.55) (end 8.7 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp b537769f-c280-4736-a055-e1e2564923f8))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp e0256226-13c0-4882-87e6-9df29af48266))
    (fp_line (start 6.985 -1.27) (end 6.985 34.29) (layer "F.Fab") (width 0.1) (tstamp 43957a13-d531-4097-8cd9-3226b3753ad7))
    (fp_line (start 6.985 34.29) (end 0.635 34.29) (layer "F.Fab") (width 0.1) (tstamp 50fd0d9e-f456-471d-8144-f18ffd98e314))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp a6893bd5-f260-4563-9033-51242ba5bd1b))
    (fp_line (start 0.635 34.29) (end 0.635 -0.27) (layer "F.Fab") (width 0.1) (tstamp d9969fbf-35d2-4e51-8af9-4be7ea6a102a))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer "F.Fab") (width 0.1) (tstamp fa266a27-6870-4915-bf82-970b050bd2ef))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "GPB0") (pintype "bidirectional") (tstamp 28013d4f-c155-43b4-bfea-cd85955803c8))
    (pad "2" thru_hole oval locked (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(JK2-Pad1)") (pinfunction "GPB1") (pintype "bidirectional") (tstamp 73775b96-1be6-4d48-95c7-2a6112393261))
    (pad "3" thru_hole oval locked (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(JK3-Pad1)") (pinfunction "GPB2") (pintype "bidirectional") (tstamp a55657b2-79e0-47d9-9d82-ba503ed330c4))
    (pad "4" thru_hole oval locked (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(JK4-Pad1)") (pinfunction "GPB3") (pintype "bidirectional") (tstamp cf051e12-3a7b-4739-8f13-f30f9d9ffbd8))
    (pad "5" thru_hole oval locked (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(JK5-Pad1)") (pinfunction "GPB4") (pintype "bidirectional") (tstamp da042666-6cf8-4b6a-8882-f343de9fedb5))
    (pad "6" thru_hole oval locked (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(JK6-Pad1)") (pinfunction "GPB5") (pintype "bidirectional") (tstamp 1f4ffa1c-74bb-40f1-9a87-c8c7ae01469e))
    (pad "7" thru_hole oval locked (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(JK7-Pad1)") (pinfunction "GPB6") (pintype "bidirectional") (tstamp 5b13342c-44b1-4a1d-8e55-0aa2ed400a1d))
    (pad "8" thru_hole oval locked (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(JK8-Pad1)") (pinfunction "GPB7") (pintype "bidirectional") (tstamp a46f5c0e-7b98-4810-ae01-a80772aa65ba))
    (pad "9" thru_hole oval locked (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/KeyMatrix Ext Diodes/+5V_KEY") (pinfunction "VDD") (pintype "power_in") (tstamp fa7d4586-0faf-4e76-974e-6a593c27cc46))
    (pad "10" thru_hole oval locked (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "/KeyMatrix Ext Diodes/GND_KEY") (pinfunction "VSS") (pintype "power_in") (tstamp 2677bd75-5f41-458c-be5e-32eeeb3e769b))
    (pad "11" thru_hole oval locked (at 0 25.4 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "unconnected-(U4-Pad11)") (pinfunction "NC") (pintype "no_connect") (tstamp 5b04d356-9b80-4bad-a02d-af8f683851d9))
    (pad "12" thru_hole oval locked (at 0 27.94 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "/KeyMatrix Ext Diodes/I2C_CLOCK_KEY") (pinfunction "SCK") (pintype "input") (tstamp 2582ad59-0b6d-4f54-b398-b0193b524c3c))
    (pad "13" thru_hole oval locked (at 0 30.48 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "/KeyMatrix Ext Diodes/I2C_DATA_KEY") (pinfunction "SDA") (pintype "bidirectional") (tstamp e4474014-c7b4-4d3c-9f74-52b067ffda1f))
    (pad "14" thru_hole oval locked (at 0 33.02 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "unconnected-(U4-Pad14)") (pinfunction "NC") (pintype "no_connect") (tstamp 6916e120-a3af-4ae6-a7ea-158859b18d6e))
    (pad "15" thru_hole oval locked (at 7.62 33.02 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "/KeyMatrix Ext Diodes/GND_KEY") (pinfunction "A0") (pintype "input") (tstamp 8c14b2f8-b6d9-4cbe-b982-9af24c5eeb24))
    (pad "16" thru_hole oval locked (at 7.62 30.48 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "/KeyMatrix Ext Diodes/GND_KEY") (pinfunction "A1") (pintype "input") (tstamp 5c35c5d9-9cb0-4a1d-a782-ab700176fae5))
    (pad "17" thru_hole oval locked (at 7.62 27.94 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "/KeyMatrix Ext Diodes/GND_KEY") (pinfunction "A2") (pintype "input") (tstamp 084f8335-f8d4-4612-8998-a301079d7751))
    (pad "18" thru_hole oval locked (at 7.62 25.4 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/KeyMatrix Ext Diodes/+5V_KEY") (pinfunction "~{RESET}") (pintype "input") (tstamp 65f0ddab-df14-4e1a-a1d0-cecef7caf555))
    (pad "19" thru_hole oval locked (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "unconnected-(U4-Pad19)") (pinfunction "INTB") (pintype "tri_state+no_connect") (tstamp 58d16e18-ae63-40bc-9399-d753b84af8f5))
    (pad "20" thru_hole oval locked (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "unconnected-(U4-Pad20)") (pinfunction "INTA") (pintype "tri_state+no_connect") (tstamp ad45a499-27cc-48fd-8f9d-237e4fc9c3d8))
    (pad "21" thru_hole oval locked (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(JK11-Pad1)") (pinfunction "GPA0") (pintype "bidirectional") (tstamp 5bddf81b-04a7-43e1-8857-2461efbac6ab))
    (pad "22" thru_hole oval locked (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "GPA1") (pintype "bidirectional") (tstamp 6bfb23de-870c-417a-a5b3-52a99a51d307))
    (pad "23" thru_hole oval locked (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "GPA2") (pintype "bidirectional") (tstamp e1db2773-2d65-44bd-9002-d861be2d2cff))
    (pad "24" thru_hole oval locked (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(JK14-Pad1)") (pinfunction "GPA3") (pintype "bidirectional") (tstamp 44195891-8326-460e-9817-79cd37f6691c))
    (pad "25" thru_hole oval locked (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "GPA4") (pintype "bidirectional") (tstamp 36bbb615-9c3b-43c5-817a-da89d3b6dbfc))
    (pad "26" thru_hole oval locked (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(JK16-Pad1)") (pinfunction "GPA5") (pintype "bidirectional") (tstamp b9cf6d8e-3ab7-4d68-9e32-fe2997d8bf79))
    (pad "27" thru_hole oval locked (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(JK17-Pad1)") (pinfunction "GPA6") (pintype "bidirectional") (tstamp 56d73c68-6a39-4dbc-a29f-e0b2252c96ff))
    (pad "28" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(JK18-Pad1)") (pinfunction "GPA7") (pintype "bidirectional") (tstamp 2c53a12e-2752-45f7-86f7-dd5d3e1cefcf))
    (model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp be24ae03-b884-491c-bd4d-04bc48a1877a)
    (at 160.02 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068156a8c")
    (attr through_hole)
    (fp_text reference "DKD41" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bca57493-4665-4bd2-a1eb-5062dcce8524)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d5b46ff-372a-473c-a17d-a173443d7539)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 90ebe019-1e3d-47a6-9ae3-d599ab79f004)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 42600f3b-4507-42a8-9977-bebcdeb76d91)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 683954e5-f75b-48e5-9ae3-3558d67ef102)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp dd3bf008-a4ef-44be-a327-35e4e851ed16))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp fca4dcc9-2b2c-476e-aa78-1dce7e980f3b))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 233d9cb3-d3a7-4382-af77-393d1dc2aa60))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2d99fb6e-8252-4390-a466-e6b7639197bb))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 374c88c6-1f0f-40fe-b7ed-e7023749ae82))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp ce767a80-e412-4a26-8a47-9fdf01f29e88))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 6d6100cb-68a9-4eb1-bacb-a15fc1bf38ae))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 65bd2809-5a0e-42cd-90b7-252f4dd9662e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7dd6f054-6239-43fd-889b-e2bdf905305d))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(DKD41-Pad2)") (pinfunction "A") (pintype "passive") (tstamp d4995d88-0ae7-4f6c-bdf5-9635e58034df))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp c0a116d5-22f0-4495-8a59-52d46300ecd5)
    (at 167.64 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000681608d0")
    (attr through_hole)
    (fp_text reference "DKD62" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b5e69b3-869c-433f-a2c0-463917330315)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4b772cf1-840d-4892-9ef9-ade37df203a2)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad516bb8-70fb-4883-b96d-17d084879857)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 368244c4-b9f5-4a4f-838a-d29d7a1b0f2f)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4bd6124e-620d-428f-97bc-495b176d7af9)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 52811732-6ffc-4904-bac1-0522877f7eb4))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0ff431ec-530f-4b7e-80f1-67998497d8bb))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 05ca249c-3f24-4c04-ad4d-61148e1cba15))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 212dbb8e-dfa8-431a-abcc-d5bea220b0fa))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 956fcdc5-1b2e-4df3-bc45-9e389a99112a))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ad66a112-77b3-420c-90e9-34b6925502a0))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 957f0bf7-3ebb-4117-b25b-fefcf31c0682))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp c2960c67-2d67-42ac-89ef-a8c7d5e526e5))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 324fe22e-e464-40f3-84d3-4b399de311a8))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 148 "Net-(DKD62-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 6bbd7eda-d00a-489e-a7df-87bc0317add5))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp c1ae0bc4-d493-4918-b4f9-f3161bf2fd78)
    (at 43.18 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/55bb1663-5f30-46ba-abeb-15eb836bc9d5")
    (attr through_hole)
    (fp_text reference "J36" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a852190-2f18-41f0-b357-4a1bd13f2f4b)
    )
    (fp_text value "R6" (at -0.025 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0f936359-83b0-437e-a930-cfd4e3e8c3dd)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 218ed193-86e9-4590-88cf-584091e454fa)
    )
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 533bc9b3-57fc-4b39-b09f-f0226bda591b))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 85bc4398-c4d5-46dc-a31f-fd7a41f10264))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 9b1102b7-0351-47e7-b73e-5bb515b1d50e))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp b610759c-a6aa-4963-9928-31539aae5108))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp e96def04-8e6d-44cd-ae43-dd53cec285ed))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 1eb949be-49f6-4e5b-a675-6b403636048f))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp ab0e6089-78d7-4500-b3b8-bc8c92102ccb))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp b8be7d38-a474-420b-97f3-f713b524e263))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp c38b477b-8356-4d22-81c6-e2b90d44c035))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp c4b40da8-c4c5-4a3e-bde6-11adc0b1330f))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp f8b3a069-edb0-4ae2-9f6e-520a504023be))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp fb2dc1bb-16c3-429b-86ab-10dfc4a18e6e))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp ff72b64a-8dc3-4b06-9bdf-8a29a3f3b4ef))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 175 "Net-(J36-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 881e030b-be4a-43b9-9e22-22aaa56cfb36))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp c3919767-e4bc-4aa4-89a3-77d8f27a2291)
    (at 30.48 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/2203e43f-03d3-4724-9dd2-784030ce3703")
    (attr through_hole)
    (fp_text reference "J48" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 40ff2bb7-182d-493e-bf2b-36ba83038f3a)
    )
    (fp_text value "CLK" (at 2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0f0704a5-b8cf-441d-a46f-0c3d5d22a609)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp feb26b97-9192-43a0-b47f-cc408e65afeb)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 15beb506-5c01-450d-8e1b-8afa781797ec))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 5753cc55-77e8-4925-88dd-45639691fd28))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 66c5b128-7624-4c04-bc6b-b3d355c93056))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 6789f180-42c2-4e39-ae51-abd90535b39b))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp fde1bb0a-28d2-49a9-8bf3-58062ea36ddc))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 01d3944a-eec0-447a-8dfe-662b847ce924))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 01dbdea3-b29c-4291-9e33-6eead9b4b21c))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 99a754a7-1566-4a13-af0d-a9dbcdd914ed))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 9d6500e2-6a96-44b8-9ed7-06f1e8ff443f))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 466ce0c8-9050-45c1-ac73-0ddc2d8e3981))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 611d605a-e0ad-45b5-9dd3-7e0e4b27f9b2))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 742c4d3b-0f03-4162-8195-5fd6cdd95254))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp a5bd7528-7513-4f94-bd14-41aca476124e))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 187 "/KeyMatrix wired/I2C_CLOCK_KEY") (pinfunction "Pin_1") (pintype "passive") (tstamp f6de6dc9-f6ae-46c3-b8f8-13f01d985f52))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp c504d8af-5a1f-489d-b53e-05734e316e49)
    (at 185.42 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068144973")
    (attr through_hole)
    (fp_text reference "DKD6" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9e44f32e-46f1-4582-87df-cf7792d42e5e)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fa9b1b2a-5099-47ba-99de-cca19598b247)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9d8c2732-4267-4cce-91a5-31ade65ac147)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aabfe3ca-da31-4664-940b-e302b181ce3b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b33daf0b-a1a3-4160-be65-9b5947fe406b)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp c8cfb1a2-ae8b-4522-88e1-897252749871))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp c589775c-0a39-4d73-8993-b344d366a227))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2eaed717-0671-412c-ba5b-c679ad3661cc))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3d3d9119-ad2c-4559-b2b1-12ed3d4fc7b8))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4fcde239-ce13-458e-ba77-64e46beec488))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 84d53a31-60b9-45b0-810f-f584c3df8e91))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp b1664d61-973d-4df4-a80d-5b00f4b9cb91))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp fbed568d-01ce-4110-bbd8-9128bc6552be))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 5929e2bf-9570-42d9-b2fb-b9c49448ba00))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(DKD6-Pad2)") (pinfunction "A") (pintype "passive") (tstamp d420b2d7-0c14-450f-9c90-fe6feb9a160f))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp c51c1592-db99-4658-8c52-c05011ba6649)
    (at 165.085 38.125 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-0000632f47fe")
    (attr through_hole)
    (fp_text reference "JKD17" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 91b01c88-6812-4d37-9977-aa8e3c9ea609)
    )
    (fp_text value "COL7" (at 2.515 8.875 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10ae79e9-5c36-4de5-8fbf-38c0a52b96d8)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6ef79059-720b-495c-8960-372cd7d9b5ce)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 03f3230e-765e-4e04-9a6c-d0cea092b4b9))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 05847f7b-3abe-48f1-9df7-860b9a1ef30f))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 98ec2fb7-fb3e-4124-b219-af19f99b8bec))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp ec328770-82c1-45b3-acc6-5245e9ae133d))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp f3e05ea3-8623-45f9-8ef0-8c2556cd7dc5))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp fa58281a-3800-4e40-8cc4-da5753497ea7))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 3c8de7cf-b531-4c9f-aa25-608a515d6acd))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b5c8b2b7-b288-4072-9260-6b9995dadf72))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp bddea9b7-00b9-4c99-b84b-449430b7ecac))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp f367159b-e862-49ab-a610-11212c7454a9))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 039a5921-0fb7-4dda-9e27-fc329fe1f26d))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 368830b5-e466-42a9-9d1b-72fc5aae88af))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 4f23c274-46ab-4b58-8257-c73fcb32c044))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp ddb3d7db-03e7-4c15-b109-5bf90832fd0e))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ebe890b4-fbb0-4061-a3cc-6c80aacc10c7))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(DKD7-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp 7e8932c9-1575-45e3-a67b-557002264c0f))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(DKD15-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 5fd2d534-3c06-40f1-bc41-a722ff6e36a4))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(DKD23-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp 8bfbc1f4-f343-4eac-9288-06bdf9ee0914))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(DKD31-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp f786eab2-6b7e-4ae1-9a1d-acb83d0b90fb))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(DKD39-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp 0c2d8eea-42e2-4fa2-a673-2e32ccbded97))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(DKD47-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp 174899f0-ae03-484b-8b1f-5de8fee705b0))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(DKD55-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp 0083f166-7d82-480f-a516-bc3e5d0aaae5))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(DKD63-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp d1e84ad9-dabe-4b81-83b8-ac80638bb58b))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp c8509056-f9cf-40fb-abc2-83d5a808d266)
    (at 154.94 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814f5ce")
    (attr through_hole)
    (fp_text reference "DKD27" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c47cf990-ce35-4327-a32a-cd351212c551)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c989cf9-7290-41e2-9c0f-2acbe72f3378)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 017ee991-2dcc-4ade-ad29-1b1ca8a0a6f1)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a858de35-23ba-4284-ad07-963d7f839610)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b5bb0daf-2486-420f-bbb6-9b927ffa1d2a)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 69482ff4-2b6c-45e8-806e-ea90d62e9e13))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp a26a9ae2-53b6-4796-9be2-fdcba110cf68))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 23f6c6e9-5e8e-4b47-bdaf-adcdd8b5966e))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 41f9f420-3a5c-4e4a-b8dd-6661255f6571))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp f44fa48c-aede-4d02-aec4-02b76a3e8d9f))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp faa8be90-a156-4552-b3a2-ade94a8eef1e))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 6bda0299-e1f1-4acd-9efb-1a3194d60734))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp fe879c0c-d210-41e9-96d8-e5c366cb2211))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 78cb5cca-7c4d-4b26-a709-03b63d560203))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(DKD27-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 6523d37d-5c0e-418b-b32d-c2ae27e1d23a))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp c8f213cd-0099-42f8-9510-87508d4732cc)
    (at 45.72 114.3 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/f681b41a-8750-4d97-b200-70bbad5e12d2")
    (attr through_hole)
    (fp_text reference "JK13" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3d7d791-05a2-400b-b575-898d97367905)
    )
    (fp_text value "COL3" (at 0 -2.54 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41789951-05ce-4881-81bc-960a13406cf5)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9f6db306-132f-49a0-b46f-e061c931c23d)
    )
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 5022df45-c596-4c23-b54c-9a82d47fe6c6))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 50727438-4695-41a1-a09c-f998c01cfab0))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 7db8baa9-0a9b-4144-b996-953dd283de35))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp e3d5be8a-29ca-4e6d-b3d4-4ee84d49f97d))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp e4932d61-dff9-4ccc-906b-9a2819ee76d4))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp e932aac1-95e3-4db1-9dab-a0f4a8c0b63a))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 75f8aa27-91bf-4981-998f-efefe35a5859))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 88593c4b-83aa-4f28-9bc3-4c5889404f09))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp c2210897-4862-41d2-8cb0-86cfc82de427))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp f4abf6d8-7dd2-48de-9895-f50f9ea14a52))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 1b6c0c4a-6f17-4493-91bc-8a413f6d7fc2))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 3117168d-20dc-4945-bec3-6e4c1438d258))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 5c93ba4b-aba6-48e7-8232-e3279a27f58d))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 831079af-e11d-48e2-89a0-71c69fc96be5))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp af7a51bf-1bc7-4511-bad5-3969001dce96))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 5b14f90e-8d95-4991-b8ff-c460b36ba3a8))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp b978a9d2-1f4b-441d-8043-d71668310fa1))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 1e186f38-d505-47f0-9817-6daf97ef59e1))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 7197cb6a-60cd-43a7-8154-b8fd99c5fc33))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp d030a329-df24-47e1-9c5a-9b61fa11dcd5))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 068fe57f-7ff7-4be4-be72-11fafb931d99))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 29d4af86-63e5-4cec-b024-45e55ea68ee8))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JK13-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp e953b70e-1a7d-4e1b-a2fc-15fa3e9fb900))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp c9abd8e7-9bac-4f32-b61e-7ee03ea544b5)
    (at 58.42 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/cc823f72-f0e4-4202-8e7e-d5cbcbc3c9fe")
    (attr through_hole)
    (fp_text reference "J23" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2e1fa008-357a-4aac-8cf5-970493fa664d)
    )
    (fp_text value "B7" (at -0.025 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 80e302b7-97a6-4d5e-8db8-a2ecb63bf436)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 79467a30-f83f-4a69-bc32-033df608d42c)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 014fd689-fe01-4a73-ac80-3c226a12a5bc))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 031a6158-41bb-434c-9952-f633292a0643))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 2ce4fb29-0ccb-4d7f-a490-6e4518b7173f))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 8b764051-f191-46fd-bc3d-0b22f8af5e5b))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp b5c4303a-4bc2-4089-a1eb-ab41ec53cfbe))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 2a47e126-8855-40dd-9e4e-56cb5c33cec1))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 9f1245f2-9177-4975-bfa0-f75992444b8a))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp fdb3150f-7b5c-4b67-b101-e0eba3c66191))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp fe294f12-b7ae-46d2-886f-9cdff5563bdf))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 18af1d88-91db-4163-9359-d7124e411ab6))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 1c0d02da-5b5c-42ee-b683-56c0e59ebf5f))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp d768292d-7ad8-48cb-973b-82d3c96ed0e4))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp f6a0f3c6-29f4-4236-9faf-ca3f64f72dcc))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 158 "Net-(J23-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 89658244-8e23-45d4-89fa-a2eb92c896cb))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp c9c252ce-b0f7-42e1-9dff-3e0e7b3b29ef)
    (at 162.56 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815b321")
    (attr through_hole)
    (fp_text reference "DKD51" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b882e4e0-bbdd-49c1-938e-4d7a5d9b5f1c)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b01e988b-54aa-46bf-a11f-b7b63d301a2d)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c7ae3fb-6fd0-4251-b74e-359208672383)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 02f0b4e5-6ceb-492f-b747-962c1f195936)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9cf537c8-e426-40f8-8057-509050a35627)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp b2f74bc6-1fa4-473e-959c-8aec92865a07))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 33f95e64-fb9d-4833-9ae6-300fd8638776))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5a752037-c3c3-4fd7-bf61-e56297424900))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9ac61070-e05e-4881-9304-1c4478741071))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp d1942295-51dc-499f-9571-f30b4e3b69b5))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e9b53bf7-f999-4331-a187-88c742ec297f))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp a81b8b7b-bf4b-427a-a0d9-d3f4e142d077))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp c4163c77-b8bc-4125-937a-677be9781037))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(DKD11-Pad1)") (pinfunction "K") (pintype "passive") (tstamp e9989e79-6583-4630-af60-98f025e39e8f))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "Net-(DKD51-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 4be25a76-c142-442f-9e9a-f32392c84d48))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp cad62a3c-a286-40db-a3b2-ee6282a0e0a0)
    (at 162.56 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068149b87")
    (attr through_hole)
    (fp_text reference "DKD15" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b7078d54-064c-41b4-9f27-13b2f6f84950)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 25cfc39f-3542-4981-a5e8-7bd23e658bb5)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f600e68d-fffa-444f-a552-0883caaf3e17)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 172a603b-ad00-4751-88b4-96252293ce59)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp be1443db-4ee8-4523-8e60-5bf415d1c6cf)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp d7872099-9ddc-43a2-a6c7-3cd9e4c6523f))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp f634debf-fcf8-4a3d-9563-4690c1ba9078))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0b037d9f-8f5b-4c8b-9edb-46417ecbee57))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 30238d44-291c-494d-92ca-c55760ff4d97))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 7fb5a003-ba95-4c94-844c-909849ecb707))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp fed5ff06-ea80-4f72-abb3-78ad0ed267f5))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 38728e66-e7f4-402f-911d-e4ec525ba585))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp ad7237f5-7c6d-46aa-b6ed-58c9b612c3b9))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp c4906877-f34e-41ea-9593-c886178643dc))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(DKD15-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2a8bd4e2-1dfa-4acb-b6d1-1167c8a75d3b))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp cce66d06-ed54-4eae-867a-a3f52946556d)
    (at 50.8 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/ab8c7386-0042-433f-b83d-d0d190b2c608")
    (attr through_hole)
    (fp_text reference "J18" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed4be033-e859-4855-b148-62dd9430802f)
    )
    (fp_text value "A6" (at -0.025 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6face538-98d0-40ae-a653-e8999ce4e018)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp eb0915de-c86a-4d8e-a0f1-84dcf28d1327)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 05a60061-f69f-4cf0-982b-3b600d194cef))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 4eae949d-97a9-49f3-9fbc-cba93e4e519c))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 895c2a55-d35b-4bc4-9770-a708d43f72ca))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp bc94524b-c378-44e8-acce-7c1ac0292375))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp d7d96405-8ab4-4875-86e3-09261d23b5fe))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 0d525ad4-3f7e-4e8e-b572-5aed774da48c))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 5e1594bb-0ff8-4379-a06e-7271e78563fe))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 64c39fd2-36c7-4cd2-b0b8-1a1e70b12069))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp cd568267-8fa9-414e-ae44-a717296573c5))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 53c3dfa0-4629-47d5-b909-4a3f4eb869c5))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 602a1461-f2fc-4f38-9213-73e41c428934))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp b64d922b-f1cc-4940-96f6-60cbefb80766))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp dafa8fd1-c18d-4c85-9433-2b8c8008bb67))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 155 "Net-(J18-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 550e0f79-ef9f-4d36-adf7-81e26d574c59))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp cd456294-dca4-4c26-9abc-c7a07f86c1c8)
    (at 45.72 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/e92cc26d-27f8-43e9-a58e-4cbff1061bf5")
    (attr through_hole)
    (fp_text reference "J11" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5c9e5a1-eb3c-47d6-be9a-b6b058a3d5d9)
    )
    (fp_text value "B2" (at -0.025 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2db578cd-b125-49d3-b68b-3360b8f58d41)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c67d947-286e-4eeb-ad61-68de893b3f2c)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 3be93bf9-8c44-4bd5-ab0f-f48691dd7c5d))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 3de5b137-b7ed-4a67-a65d-5332350a142e))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 4a7a8704-b751-4f8c-aedf-2558a0174a72))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp dc4ad6d5-b7e2-4098-b974-50466b3890e2))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp ea0658cd-816e-408e-924b-067dc4ea75f8))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 872056a8-3317-408d-800b-762b71027ed5))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 973720a6-f461-4d46-b2fe-59915df69d25))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp a2da6c4b-cf98-4d3d-b54c-e05e54dfd2b6))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp fcf72183-7571-4ba1-a298-770fa333efdf))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 5278fb5e-f15e-42fe-84df-a59fee8119f1))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp cb232dae-017e-46a0-81d3-8ae4432055dd))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp df8f1fc7-0af7-4ef1-91a4-ae074793bf79))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp fa2253b1-674a-48db-8f5b-f4c85dcb27ae))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 100 "Net-(J11-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 3962f024-df76-4ce5-a845-a5bfd0cc118f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp cef7d52c-da57-4ad1-986b-a7d5f0d0c4c3)
    (at 170.18 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815d123")
    (attr through_hole)
    (fp_text reference "DKD56" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1310eb7b-0580-4ee4-bd04-b78acd204a90)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bbfe2648-57c8-4407-acdf-5dda24b6faf1)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8578f7d8-708f-46d2-b5a1-d310521ccabf)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3b08100-b17f-441a-a2be-bcfa82136162)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6698542-6f70-4577-a63e-b85120942a6a)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp ac289c46-f2f6-4daf-83d4-5a2a0b805e83))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 50d5a9ed-a756-4ef8-9577-53edf03bb51d))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3e693eb5-18a4-432b-a22d-d79b26d359c5))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 711e7183-50f2-471f-9b86-f60d258126ce))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9681d797-7c68-45da-9fd1-aeb1f1794ee8))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 9faf5c0a-a3b2-4041-9b87-6ce5986436ce))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 29b6733f-e2ce-499b-a093-b144f7ab4e51))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp e5b278f8-fb17-4342-b52f-c59486d024d0))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp cd829b43-652e-41a1-bca0-6b64e26c4327))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(DKD56-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a71fc6b6-6f02-46be-8bfb-7e1fb0868c2f))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp d4ad31c6-13af-4224-917b-20a4927b453d)
    (at 121.92 33.02 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006202d79a")
    (attr through_hole)
    (fp_text reference "JKD1" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d80c8609-1e2b-4689-af9a-61791d208063)
    )
    (fp_text value "ROW1" (at 0 22.86 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f2c74efe-f0c7-4f39-9a32-77a21ff7c9c0)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9e574e77-9f6f-4a8d-ac30-09d566a6071b)
    )
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 5a683acc-b7f8-43ad-a9e0-1421484e4cce))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 65ba9d29-16f5-4195-a8b8-68d5b5a71cca))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 7345524d-162d-49f9-b059-7d50670e840d))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp a45d2504-fc88-4256-b6bb-e332cc97f460))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c660ee40-b7d8-4115-8ac8-ba21761be22d))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp cf6ab688-e350-456d-b813-ab39b75be06b))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2b032b6f-8dfd-4462-a7b7-65c2c02e7815))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 819b4251-f100-46c6-a022-16e224ab5524))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp eced03e4-5e52-4ec7-83ae-f96c1918cc3c))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp f05605c4-aa50-4dc6-bfac-cff330719723))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 039c2f34-b471-4ffe-a4c7-f26dfdac7f6f))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 26985c91-87d4-4782-bbdb-d53dd6ac050e))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 59b8acca-a31d-4968-8a25-01bf543ffede))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 74d44543-bc28-457d-8af1-84d57056a44a))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp e85ae780-6638-4d64-8333-4b09a83267db))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp a30e0701-c812-4e5e-bdb9-3a97199feb5c))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp d87765f3-19d0-4d5c-a5cc-d49d1cdcafe5))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp e0588067-8ee7-4fd9-bbde-f0441c8ac6dd))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp e3138c8c-8592-4032-9731-99645833c68f))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp b7f4e6ec-9cc2-4363-843c-c94e2d7fcc0d))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp a25c1e6f-f7f4-4ca2-ab21-53b761dac575))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp c7792f8a-08bb-45bc-b38a-4b562a82fd44))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(JKD1-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp fb31939d-0485-4130-ab9d-316278cc319e))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp d554f908-c582-4391-9044-7f2d6924f2f5)
    (at 160.02 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814d4df")
    (attr through_hole)
    (fp_text reference "DKD23" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3ddb950-dd3c-4a6e-9c07-2a6518f49eb2)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f4b78e3-a175-4b37-af39-fd1905f24778)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 823a9440-55e2-4b28-a627-d362fdfb1b1c)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1c71853c-5696-40c9-a21c-a2dd7734b919)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a9d39c6-f877-4ce6-8e3a-00e6d99a1a3d)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 0093fd11-ac6f-4bf9-b8f2-690b476e4446))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp cc93ce7d-db41-4ba7-b9ae-0789db455b12))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 3223c945-14a4-494a-be13-9fa01ed61e9b))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6c8994bd-1d42-46f4-82a2-e8fb69364c75))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ac37c829-4318-4007-8276-80d14028c138))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp f69d328c-b685-4421-90e9-08f88390d6a4))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp b282b2e5-811c-4b07-92ac-08813ec42541))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp a46827eb-1e8a-476a-b0c5-6cd367424236))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(DKD15-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 8b8de74b-a6fb-4ed3-afed-26cf3e3e1736))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(DKD23-Pad2)") (pinfunction "A") (pintype "passive") (tstamp e572a874-29a2-41ff-8c1d-b55c256b6c70))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp d697b8e4-68eb-481e-bc57-2fd5df6100db)
    (at 45.72 119.38 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/d4d6afce-f368-4ed7-b36d-7c4b38bb8c62")
    (attr through_hole)
    (fp_text reference "JK15" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 538f2bd0-afec-4e97-be19-cf929eb93187)
    )
    (fp_text value "COL5" (at 0 -2.54 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b74f0ed-fd0f-47cc-a98d-90d5521842bc)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 67de83a3-095b-40a7-a0f5-dabf35170f88)
    )
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 49e03d71-3f8b-4ab2-a8ad-aea2f1ffb367))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 7da8106d-6e2d-4694-91e9-9314fbc12237))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp bc4919eb-325e-4d15-9bb4-4b77bf6a8d90))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp bebae279-1159-45c7-9b16-97da93b28a0f))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c41c44bf-5297-4bd7-b8ae-f424eca697fc))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp fbd6e139-6df1-4cfb-b2ce-185045351c35))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 1107bf25-2f8d-4872-b5bb-07976e1353c2))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 4a0cf582-a0a7-43b2-92e0-c83a4eeec326))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 649ebedc-fbdd-4922-9331-961aff816818))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp fecf7ae8-1e98-448f-b592-6fb82fd0d97b))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 1d7890f2-f49b-4081-81d3-7afd43e4e0eb))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 42d38ba6-d540-4732-b1c4-1ce68b71f912))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 8060ab5f-c0d0-4800-9f9a-c9664b906f04))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp a54675c0-0acc-4968-ac10-011864601794))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp e4812f20-3342-4241-ad8b-9fbb0b8ef8af))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 9faa421d-f6a7-41a2-aecf-fe28b3e90dcc))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 6b1e6700-5783-4142-b83c-b11d6ea16e69))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 88431cd8-35c8-4f27-a56c-98e34ac94dee))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp e038a785-3dcd-4c0e-8cd1-14376d89e66d))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 95ff33b2-1d6a-4a57-ac1a-b82d11b6c440))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 619071aa-0abe-42df-bba5-d55a5c1a4d5a))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 62905531-e4c9-49a3-ab44-d00e96f2ca58))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(JK15-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp a6368107-2128-4bc3-a9c5-43d20cb3dd97))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp d6a8f316-1392-4ab3-858a-2bdd1e8ab61d)
    (at 43.18 25.4)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/2ea45036-6908-4767-a4a0-ac16e09767ee")
    (attr through_hole)
    (fp_text reference "J12" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9858a585-1ecc-4893-a1c6-bacba18521ec)
    )
    (fp_text value "A3" (at -0.025 4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 76adfc93-1bf2-41b7-b4bf-eb835ea8821f)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cc490913-daab-4fa1-87b9-975705ee9dbd)
    )
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 480d5422-6d33-4319-a5c2-9ce1cd04fa90))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 8d3d3e35-82e0-40ba-907a-a8ab9693853e))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp d08f9431-ef8a-42b7-a850-bcd8bb770f1b))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp e82e6c3a-dba3-44b6-823e-2bd844f08cca))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp ecff6837-a08b-483d-9647-9310dfc674e3))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 3a6e1b00-aa08-416c-85dc-bf006b0a4a78))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp b825db6d-eaf6-475d-bf93-964d29afb19e))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp da1874bd-bc34-4d30-85e0-173930a32a31))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp f68ae795-1f05-4a39-94cd-eb3e2d140979))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 2b02e529-0dd1-4c56-92a3-7eb22d2ee260))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp ae5c31ab-a505-4959-ae0e-cec81fcbf815))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp deba7d89-f9a2-4354-82a6-0d3192f950f8))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp ed93faec-dea3-4b89-9648-290ad7f4effb))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 101 "Net-(J12-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 58f281db-090d-4a92-8a73-05e2a97a7ee9))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp d6fc5299-22ca-46eb-a8be-9fa35c664ef3)
    (at 175.26 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068154877")
    (attr through_hole)
    (fp_text reference "DKD38" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f78fc1fb-8cd7-4888-96b1-d7ea2954f2de)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp df66d690-159e-46b9-9da6-f59c22a881ea)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30e10ff2-5ee7-4507-93b8-8c2a20cd692f)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4b5c60ee-d38c-4b79-8956-a87daa0713e4)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fdd82b1b-99dd-43e1-919a-a4019bb7a15b)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp f5ba0b25-77ae-4a66-bb52-61c63e35bb59))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 4e05c80c-bbe9-4a72-99e7-02fef95faff8))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 950da7de-47e8-46a0-9640-a8ce7fb3ceaf))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp a168c3cd-ecda-426a-85c8-8815fa702cf0))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp ae0e8ce8-5064-4417-9bf5-4b2fc0924bb1))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp d9305564-1a8d-4c0f-b8ce-06f866d4b526))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 17698cc5-a777-4499-a764-74f4b379e8d1))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 7be23b48-7937-44ad-b456-6482fde51d0e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(DKD14-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 5510fa50-2e4f-4ff7-ab2e-aa7c8cf30c7b))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(DKD38-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 6d78a483-d734-4101-be4c-cdc802363c8a))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp db41e836-6945-404a-8e36-2d5f7579c882)
    (at 45.72 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/0a4a5095-16ff-4ec8-b82d-45b4d38ffde6")
    (attr through_hole)
    (fp_text reference "J16" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7d62d74-e40d-48f8-9eac-491ee6420441)
    )
    (fp_text value "A5" (at 0 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 77882400-606a-4159-9b6d-7be7ce590e63)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04dfc243-0f51-4603-bf53-e1e3c0de09b3)
    )
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 3397e828-549f-4d19-910c-989534dfee84))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 55d86872-e23e-4870-a2e5-31f924442b2e))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp a86ce70c-0b0b-4e00-81fd-fa720b16c5ec))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp dfcff0c6-14ab-4e61-b849-baf49cfbbd13))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp f3fc3ce5-4efa-4006-8983-46e918c0de75))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 349aae3a-4c5e-4552-af38-0bc89507f49c))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 401fab3c-23b1-4753-9559-4f10bf6840bd))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 553e83e2-46ab-4c23-99b1-63f20f063cd2))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp c73bfff6-9c34-45cb-853c-863990f11aa7))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 607bd1dc-3a6b-4b00-8871-0e4f8cbd31b4))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 7a0dea2f-98b5-4afe-8d5d-f39ea5db6892))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 9934072c-5674-4ed3-9146-61b9347f189d))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp ec870b96-a94e-4dc6-9900-ce74b92f8bb5))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 153 "Net-(J16-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp c07aea70-6106-44bf-96ff-8e775e4243b1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp df57f87b-7268-48c8-9915-991d77f6b8dd)
    (at 81.28 127 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/e736b25b-b772-4a49-88d1-cee950617bdd")
    (attr through_hole)
    (fp_text reference "JK1" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af66090f-a672-4e1c-9786-b5f80caced8b)
    )
    (fp_text value "ROW1" (at 0 20.32 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3107e0fc-47a4-49c9-a928-6a37b216ea16)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb7c71f3-f969-47eb-b17a-0f964980b243)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 00f78418-d955-47a7-93c6-46c7bd11755a))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 066a6f2a-f45d-453d-b235-f35362c1d319))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 1281fdd6-bd82-401b-abef-19586cce32d1))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 5816d80e-5db1-4789-995b-6e8c253ae7a2))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp ba1eb373-380e-4920-8150-8372ef74915e))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp ec9dedba-2d74-4975-987e-1ec055f7d26f))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 0bd211e5-2784-405b-8599-67b0c0cb9b03))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 888c1162-a54e-44f0-b269-195e01dbc865))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 9093f381-c66c-4034-824f-248f47bbde7a))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp dbbc1ab1-08bc-4057-8bd9-4ec7d4a7a905))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 1ce15c77-9268-4145-ab00-2e186578141b))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 25d1a2a4-777d-4668-bed0-fe669df52553))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 7d93dce9-e391-4d4b-8782-41af30da5f83))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp a758e3d7-001f-4777-9f13-6c834564b598))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp ce67dea8-ff14-4d6d-a114-bf427606e91e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 70ac9a14-a4ab-43d3-9d89-92ac4c47af94))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 6d208d8d-d9a4-4d11-8aa8-f13a6f31c29b))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 95f131a7-5425-48ae-8a80-7cb3391270ab))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 70b62b46-4cf5-4873-926b-95a3ba418dbf))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp ba1aba78-dbbf-4a1a-bb46-c6c27018ca0c))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp e58f5cf6-7c51-43ff-8ede-97ceb5cccbb4))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp f29a3cff-a351-40b6-b31f-d4b89c3f6876))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(JK1-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp f519647d-9142-4233-83a8-5c7efa60a024))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp e2d0f7de-130f-45fe-8137-c98d54977ba1)
    (at 53.34 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/371abc5a-52a7-4b87-8ec7-281e5dbbd659")
    (attr through_hole)
    (fp_text reference "J19" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b96b731a-92c2-4e6b-a452-39f1d33f53c2)
    )
    (fp_text value "B6" (at 0 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c517de34-4f09-44c4-870e-606e92563fb1)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 39f69e4c-3d98-4642-8cee-de7f9bf86b5e)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 0536025a-6414-4951-bfd6-905537685d7e))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 35328af0-2bbe-4eda-b255-c9bb9c6e435e))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 97d7f8c9-b0b4-436a-9b5e-5ccb959ea185))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp e794ab59-7bcd-4983-8681-ae56dc6f451c))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp f069c764-5d8d-402a-b60c-f5f2b694001c))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 74a79877-8958-41da-8944-562e6bba6c01))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8416cc67-e5d6-41f8-bce2-3d8fbd36986b))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp afcd91b3-4753-4f50-890c-aed354e976e6))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp ecc742f9-8e62-4db4-90e9-b040a131cae6))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 7d393522-d44b-4d20-8f0b-b7142987aa89))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp b7bae9c8-4fed-4c69-a28c-182e2480bcdb))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp ca677453-09f3-4d39-9e39-a44be56569d9))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp eb8c4f77-d931-4888-a754-0b09c6b8907f))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 156 "Net-(J19-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 30a8d4e5-202c-4d57-80d8-c5f2ad3ce2dd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp e4b35e05-e395-4983-bf07-109fcbe36ce1)
    (at 154.94 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814eb5a")
    (attr through_hole)
    (fp_text reference "DKD25" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e63e3327-5e15-49bc-b22c-6932c08d5044)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e82d9579-24bc-4a14-ad8f-c352caf9fc88)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed222c62-58b4-407f-aacc-1070ab2fd7b6)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b844b38d-523c-46a0-aa8a-1bbacc107f81)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f7d36ca4-290f-4081-b3c1-69e4efa11876)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 2a60beef-75e6-4e66-b421-04d31fe2e4d1))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp b5c0ad80-2073-4837-b488-d7375011969c))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1df50e61-4d11-49fa-a0f1-0149420afe56))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6dbdbe47-6c99-4e01-a2ce-464ea94c9849))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 786245cb-9bf1-4089-b9f9-d0f35442dd4f))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 8f1dae16-b004-4fb3-a96a-0e2a98da62b6))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp f4942148-fa36-49c3-ab45-d119640300f1))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 836c66db-a654-4a41-bfb7-754cacfb748d))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DKD1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp df5f9207-1476-4306-85a8-f9da06ac487e))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(DKD25-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2fe4e1e7-73d1-4d31-9e3d-7340ae19886d))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp e5c2c18c-e6d2-44b3-b64c-53f9b4355ef6)
    (at 170.18 63.5 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068147b8f")
    (attr through_hole)
    (fp_text reference "DKD10" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b8769df-a728-4ae2-bfd6-17cc6c44f24c)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c8ba574-3ee1-450e-9261-a421c9e13045)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 371a7c33-a384-4f74-a77c-9472f7755e4d)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6703983f-7dc3-4b3e-80f6-a2be36335d27)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7006061b-fcd3-4355-bf6e-3cd8f6679dcf)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 168b5073-ae89-4a9c-9d7d-7d059dce2c61))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 8dec94eb-bae8-4fd8-9cb5-f3f63554f25d))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 259411e3-13a3-4109-864b-56fc1ef714bc))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 7a8413c3-6eac-4218-90af-12ddf09717df))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp ad1379f7-6630-4690-b0de-049213729102))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp e6c72bd2-8db2-482c-96b5-aca7e2476ee9))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp eeb06c3f-f892-4ebe-b79c-c2d8eced4716))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp c05f7476-3a94-4f93-bbf2-5da176f87413))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(DKD10-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 267bc64f-3ffe-4086-8efa-28b2e21d194d))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(DKD10-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 88016da2-81fd-43bd-9302-b1527a39de7f))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp e7d77ce7-e08d-4153-a89a-1b9824a2b90c)
    (at 45.72 45.72)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/fcb79e8e-23cf-418a-85d2-2ac39e345d6c")
    (attr through_hole)
    (fp_text reference "J35" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e2def774-2363-4585-8554-cd8fc856a5ac)
    )
    (fp_text value "R5" (at -0.025 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ced3081-bcd3-4c18-bb13-ae5959f11a13)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dd30ffcc-a60d-46b3-8fe9-b2ad66829a27)
    )
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 0d419671-d27f-45c9-8ff2-99401a361b69))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 41c8d788-1f48-46e8-bcfe-ef988216a368))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 57824df1-8d76-4a17-9512-1c8039af1b39))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 9bfe2315-672f-438c-9b3a-c36cb505af51))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp fd365f0a-c3ac-4bbe-b914-0863a9d64fcf))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 85941b76-3eda-424c-9d0b-5544cc5d9dca))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp dd493107-2a31-4211-ab66-76dd1f222066))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp f0541591-b717-4bbe-a4d4-c359259e2002))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp f2185193-04f1-40b5-8f5c-b32964204dfb))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 08e3e4dd-ac21-45ec-b559-ad4d83ac9237))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 0be45535-b3a8-418c-a4c0-8474e868751a))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp 652625eb-5f74-4422-9570-47b79a3f843f))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp f547678a-8512-4a6d-b65f-f39317b3a893))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 174 "Net-(J35-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 2f8a9f91-5ed6-4cd0-a235-3880b8ab1684))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp e82c6728-328a-4fb4-b819-3d2b4377817e)
    (at 93.98 93.98)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "cimdit.kicad_sch")
    (property "Sheetname" "")
    (path "/669e5b20-562e-4901-8e1c-8d74bc81ea2f")
    (attr through_hole)
    (fp_text reference "J50" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6bf6964-cc09-4f5f-983b-04b1e934bfa4)
    )
    (fp_text value "ANALOG" (at 0 20.55) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4b2304a8-20cd-43c2-a799-196b58351e2a)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fc4187f6-7dbb-4719-9349-7babaf430eff)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 622bf153-de90-442a-8d92-619f9d89e9a5))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp a5da372c-1098-441f-9f2b-b1c04cb36489))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp b0f08cc9-acb2-4ec3-9a3c-c52b0ffd2f95))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp d5a8e7a9-bb14-41a4-b1dd-942972499bfa))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp d6ba4f66-667d-4adc-9f1c-500b6dd256f7))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp dbd72087-ee6e-48ff-8bba-ee652a08c2ca))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 15f9978f-b06c-492b-b122-a1685d2eb266))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2d718a4b-0d60-4ffe-b3dd-9c1a73541613))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 2dc5f5a9-3872-4617-a7a9-b089534e2144))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d0d36b67-b970-457a-922f-39081b891301))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 012f6773-88f4-45db-a2fb-7155abd6c07d))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 1190871e-7691-4380-bdc7-0368cef1e349))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 9e511a5e-84bc-4ad4-b33d-1ebd979f7825))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp d7a3538d-20e8-441d-a5e9-5b822e4f4836))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f00249a0-f3ae-40d6-8991-f786cf98b3d4))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/Analog Multiplexer/GND_ANALOG") (pinfunction "Pin_1") (pintype "passive") (tstamp e18627ae-70a3-4451-8b50-12824cb60a61))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/Analog Multiplexer/+5V_ANALOG") (pinfunction "Pin_2") (pintype "passive") (tstamp 36db501d-cbb1-4103-9086-3a490b32b259))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/Analog Multiplexer/ANALOG_ENABLE") (pinfunction "Pin_3") (pintype "passive") (tstamp cfe2a938-6dad-4afc-903b-03bbc128585e))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/Analog Multiplexer/ANALOG_MUX0") (pinfunction "Pin_4") (pintype "passive") (tstamp 56900597-c23d-449b-874a-34d26704a832))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/Analog Multiplexer/ANALOG_MUX1") (pinfunction "Pin_5") (pintype "passive") (tstamp dd4eb669-c7ce-455b-852f-934c4d14acea))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/Analog Multiplexer/ANALOG_MUX2") (pinfunction "Pin_6") (pintype "passive") (tstamp ddd184fd-e3ef-4a19-8e7e-515ba7538174))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/Analog Multiplexer/ANALOG_MUX3") (pinfunction "Pin_7") (pintype "passive") (tstamp 1e2b55bb-e350-4363-bf19-e50ddc9809a3))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/Analog Multiplexer/ANALOG_OUT") (pinfunction "Pin_8") (pintype "passive") (tstamp 9bc9e197-e8d1-43cd-90be-2fc9fe4d4336))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp e8317c17-1a4a-425b-8f23-fdf288c382a7)
    (at 116.84 55.88)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062dc4e20")
    (attr through_hole)
    (fp_text reference "JKD6" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a1f0e376-34aa-4668-88d9-bb1e7f0622a6)
    )
    (fp_text value "ROW6" (at 0 -5.08 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 894a2745-153b-47fb-b46e-f3edeee5a9b6)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f11db99a-858e-486c-9e5c-05717b94c043)
    )
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 166fb1f8-7980-4dba-907a-02df3da7d71d))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 31089eb0-6ba8-4dfa-8ab8-dda0cb397418))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 4a7b31ac-459f-4899-ace2-869eac029684))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 699a1a9b-78ff-4bf3-a348-d15fb3346e0d))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 8cc47162-1350-4ece-9477-38251223c654))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp e694fad5-7a7b-4706-b8d7-b9db96a5be6b))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 42ccd407-40a2-429a-b751-44c1e6b56a34))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 5a41ba35-3bcf-41dc-b027-e67b47139aa4))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b6ea5f88-446e-4ad1-9419-cef4462b24de))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d91c034f-821f-4293-b29d-764dbdb9d98d))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 1ca3994f-707a-4e43-a743-505193b328bc))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3cc4bf8b-ded9-4366-9392-1a4fc69b8af3))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 4b23ea7e-e394-42d2-adaf-c5ff5c515929))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6edc2129-5755-434e-9e4a-7df5dc6088ce))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp aec00d5e-31c3-4d95-81dc-15748ee66ac5))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp e128dc9c-b329-4778-bac1-ca48d69b815f))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 5b695b0b-89eb-415a-8a63-b3fc83206e00))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 03e1c348-a252-49ce-b0f3-aebab39b7732))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp 8ac27bb6-4f8c-4b35-aa01-c044cd8b9135))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 4a546219-c246-478b-bdc3-939bb551576d))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp ac0f05a6-a91a-4d0c-8593-07d7c499f56e))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp 258af58a-8850-474a-ab0c-f77063d877de))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(JKD6-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp 4c8d8d83-fcc4-46f1-bf50-b17947c99cc8))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp e8534302-6424-42b3-84cb-491a71f2e92e)
    (at 182.88 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814a076")
    (attr through_hole)
    (fp_text reference "DKD16" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e98b1bca-21bd-4ecc-aa50-7c55d9c2d6ac)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ae05bf4a-0091-4c6d-a251-d574b210c321)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92cc9e25-3f3d-4a56-909f-1edd5e0ba70a)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1dbfe119-2837-4ceb-9076-5a2712ad0b2e)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da9bcda3-2323-46dd-86e5-bdb53fe08f4e)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp b97eb57d-77e0-4e9b-9376-ed6bcb9e6212))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 78cb6dc8-178f-4c7a-98de-d8547ea647ab))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 056dc577-3026-403d-989b-2d5364e96d2b))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0f296070-e952-4bee-b0b6-cffc135c96b1))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c01da573-ec21-4ed3-b08b-7e24e2a71db5))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp ebed01ec-b57d-4016-98c4-b055a03f0f7b))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 9e4d5040-d5f2-4d52-ac7b-47a0859f27e8))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 2007250c-2d3f-453b-ae2c-c1b1d73c0fd0))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp e8c8c211-2bf3-4042-b050-c46dc18a018b))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "Net-(DKD16-Pad2)") (pinfunction "A") (pintype "passive") (tstamp d62cde1f-d64b-4712-a081-fa7d3b7e1340))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp ec0fcb40-9ace-44d2-b255-72e4c488785a)
    (at 152.4 43.18 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068157f69")
    (attr through_hole)
    (fp_text reference "DKD45" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d027bab4-41e5-4fdf-bea1-34eb380843dd)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fb6cfad5-b6b7-4101-990e-854319fbb28f)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ee995e8-35e1-4bb9-88d1-7fb1e3f9a7a7)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 467c0f29-bab3-4c46-9134-0b3f6e62b7b5)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6d8fde8-1d2f-48b2-909e-db350e02ca02)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 365c80bb-98d2-439c-a93d-e2720539fb8a))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp b4a11166-d330-4bf6-972c-79ef30a58405))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1f393652-410f-456c-9773-651ab76f8e76))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 43da5f6c-318c-4ecf-ade0-e8e07a798779))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4b1a9816-9a2b-4e92-a687-fa87ebae2b3a))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp ea440cff-8faf-4b3e-a539-b4228ad9238f))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 02597a6e-7382-4f87-98fd-2a49f76867b2))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp ef5824af-0db1-4b7f-9f52-7bc350cff4ba))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(DKD13-Pad1)") (pinfunction "K") (pintype "passive") (tstamp ba745b86-e05b-457d-a200-d0c835cb8dfc))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(DKD45-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 97c0089d-166b-4a85-bcdc-f6bf19f0cb31))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp eed70916-7311-45e4-bf91-e6066a8a0a16)
    (at 45.72 111.785 -90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_extdiode.kicad_sch")
    (property "Sheetname" "KeyMatrix Ext Diodes")
    (path "/7a807cd9-4b53-4d34-8616-454af4054d6a/41d61275-7588-41de-9c27-01f35f46da91")
    (attr through_hole)
    (fp_text reference "JK12" (at 0 -2.77 -270) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cc04ca3b-8673-4c68-a628-036eb7a4aaa5)
    )
    (fp_text value "COL2" (at 0 20.55 -270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ea99ef6-fe71-4339-94bd-bd4a3df23301)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 141f677b-8a0a-44fd-aa8a-2a12eea2133f)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 11b3e598-935c-4908-b3ae-43c2b4b29db9))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 5969563a-32d7-4492-b773-a96ed70f0a37))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 6f45336d-e24b-4679-9d2b-3289d902c5bd))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp b1487b24-31f8-4d10-9dcc-191485b014ad))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp b48d2eee-1de5-475e-9932-be60b0a49873))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp c5d761cf-b458-492d-80df-b662d51e7005))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 4a3a1a42-84d9-4370-abcc-d2b0c84ed7f5))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 728702e3-d0ed-44f7-9d2b-bec1d8a1e355))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp bbb8d874-c619-4cb9-9f1b-9e0c45e03639))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp c98b9d7b-e440-477e-926c-92f959d22b10))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3d9a111d-1261-4ce3-850a-87f382518705))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 78346613-414a-4661-83f1-b2d7b7511bf3))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 80f8b1d1-3bef-4c0d-9bba-380984e137d2))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp c5832b3f-2a93-4cb6-8138-104616b48af6))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp f751289e-d826-482f-9390-97167f4fb48f))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp dcd839be-d8f9-4df6-ad91-af29dba9acc7))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 2f646f6c-07bd-4eaf-837a-a0a5a9720e4d))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 5f62ba32-5712-4f57-a4ee-7984048dec20))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp cd5a4dda-c60d-4982-aa17-ed95b9351ec6))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 38e8b9a5-20dc-40ef-9db4-1ad422a4870a))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 48e3c8e6-f068-48d7-a75f-b33be9b57bef))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp c06c436c-b46a-4d20-9cd6-2916a32522ae))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JK12-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp f156067d-13ff-4a50-a39a-c4ddaa8a74d6))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp ef575fde-6a4f-4ef7-a180-7a51a7d778a9)
    (at 58.42 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/599495f8-b69f-4a68-82fa-d7c87ad23fb8")
    (attr through_hole)
    (fp_text reference "J45" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2879c5e8-aafb-4a07-849d-35933435aba2)
    )
    (fp_text value "C7" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2837c0cf-ef1b-4254-ae4b-6ef635bbb262)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fef5e210-1b1f-44df-a2da-1b5d850306f0)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 49a3599f-39f6-4cbe-9878-027f944e55d3))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 5aefd83d-adbe-4fb4-a687-1c995b5ce80f))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 735c9d48-2a48-4ae1-a7e6-9d055abe5ff9))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 888f0702-fa19-43d9-9729-eed0e4393e37))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp a62edac3-42ab-40f8-af7d-87bcea8b0bb6))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 04f5b9ae-1427-4f77-bd42-5ae27f039332))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 288829b6-4099-4ab0-84eb-8a4d43e0f81a))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 65c9b880-fe4e-4ca0-a886-40d0161c2ad9))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 8e9be0a8-e062-4904-8a28-e0ba35891aea))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 2a090783-e8f2-47c1-8e74-67e3896ac297))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 783e79f7-eca2-4551-a3b1-ad149f1459af))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp f9f94fec-8ec5-46ba-9f4a-501106495ed3))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp fda887bf-b29e-4476-b946-9b9ca4bb8ec6))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 184 "Net-(J45-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 33f6b87b-361e-4681-8f78-6d37946c6353))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp ef6a15e7-e8b3-4203-bb6b-dfba8ce753a0)
    (at 121.92 55.88)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000062e52396")
    (attr through_hole)
    (fp_text reference "JKD8" (at 0 -2.77) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5624abd2-f539-498d-9536-5c7d8e4d4e85)
    )
    (fp_text value "ROW8" (at 0 -5.08 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad2e7866-18c3-48ba-9617-033bad667762)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4035c6d5-0218-4683-a405-7b7b1fd841f8)
    )
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 0a265ffd-2d6a-406b-93a8-36c3d8ec1b7d))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 0bc477ec-347c-4723-afc2-6a435eed7f48))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 58038987-bd72-48c4-9da8-f92b5963d394))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 627f83b5-1a5f-4818-bb28-27d1eb58914e))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp a14b6ee9-d973-485f-8e68-0c830c085de8))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp a741aab0-fc8f-47b8-9a1a-ea17f8eaaa63))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 319771cb-995a-4a2b-977e-ae0015814bd4))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 37fd1c8c-38ce-4ada-a3ac-06ad259d5364))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp a5fbae09-3742-4842-bafe-eac5c02abbac))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b7c5c4af-f77b-4c11-a117-0d0d60a6dbe1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 303cc505-fb3a-4005-b77e-11fe8d831cdc))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 3858a3d5-5d9e-43e3-b5e2-b0261e68adc8))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 996fcf6e-dee9-4177-bc04-d5895b23d058))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp d9ef79be-24cd-495b-a83f-a3498cf1e5ab))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f8a4b92f-3411-41ff-82c8-b0c55f5f1a21))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp a6a578f4-d802-46e1-886a-428db4a8bb75))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_2") (pintype "passive") (tstamp 540bf389-7b7d-43ee-bd85-d086de3cb93a))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_3") (pintype "passive") (tstamp 772ac269-f1e9-4190-8952-dba4d782da1c))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_4") (pintype "passive") (tstamp f88212e3-2f28-4bf8-84a4-964383d9145e))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_5") (pintype "passive") (tstamp 85e5e046-2bb4-4c5c-ba84-43c62090d72c))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_6") (pintype "passive") (tstamp 9933035d-30aa-4140-9b9c-0b3f2ff054d3))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_7") (pintype "passive") (tstamp df748fcf-38f8-4302-a20a-3c6361e86064))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(JKD8-Pad1)") (pinfunction "Pin_8") (pintype "passive") (tstamp dc683a48-1a5a-4bef-a074-1a8971ff5d6f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp f233a730-88ea-4ba2-9ab6-f6e34c62bb31)
    (at 177.8 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068153bbd")
    (attr through_hole)
    (fp_text reference "DKD36" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f114460c-6196-4746-b633-572fc78b07b2)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ab5e540c-cbb7-4576-aa16-ad43e2889dfd)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 67982da3-9042-4932-abb2-1b2a8e19f96a)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53ea9797-0f84-4805-bf20-3bd0cc636595)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 75a11c0c-9043-4723-93bf-97178f7d2b90)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp b57aaf0c-a11f-424d-a85e-07b717725d8c))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2dcb755c-6319-4900-aefc-4f8daebd5224))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 2699f178-7eb1-43a1-8337-59fb51a70d49))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 57aacb52-c896-44ce-a486-953805d4f73c))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp b594dc5e-2b51-4b3d-8ff5-e395213f5218))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp eb07ae3a-423b-4114-99a0-4121b01f71de))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp ca169c82-b807-4d36-a0e3-1d59e4028313))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 38b8ec03-ed86-4d03-8c8a-839b3f87c6a8))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp d6dd04ad-b08d-4414-8fa8-83fac877b3cd))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(DKD36-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 5a1fde90-9626-4d77-8cd9-61b79c0d3efe))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp f27144ea-3be0-41a7-9439-aa5788ec9192)
    (at 48.26 38.1)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "rotary.kicad_sch")
    (property "Sheetname" "Rotary Encoder")
    (path "/0e0cd3f9-9e59-4187-9e69-2f18dd8368cc/c9521a26-be15-4a1e-8acc-422906829663")
    (attr through_hole)
    (fp_text reference "J17" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9dbd9e26-9782-45c4-9403-4d72b07f29de)
    )
    (fp_text value "B5" (at -0.025 -4.445) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 437250d9-eb22-42a7-a0ee-f2e6a9628e2b)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d56d28a-c4af-4430-8964-9b60bd37a4ca)
    )
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 59e90f16-96b8-49bc-86de-566bbe3dd75d))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp 6915e2da-1017-43ad-9e3e-de99af10b4da))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp da502ba4-a51e-4a20-8efb-4020dc3cfdab))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp ecebfbae-5921-4400-8c7c-d6d4cfb57f3d))
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp f3569ccd-85e3-4d52-b53d-a2b9f3673ed0))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 025b67ec-fe6a-4ee1-9f43-89b9b5fad3d7))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 3081c45f-0a62-4dc8-a706-c2b3c5e194d8))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 85705930-0850-44b9-bc2d-76e756994d34))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp aea380b3-0b16-4ad3-8281-37f0d2673e39))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 0693453a-34c3-4bfd-b360-f7994c4e507f))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 3258ef2e-7dfd-4b7b-a84c-a8f03af613a6))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp b7148d4c-a9db-4405-915a-b55a0c6f6c34))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp db1fd106-5c41-422b-b451-e2c7dd2c942d))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 154 "Net-(J17-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 62ff3f34-d3e2-41a5-ae11-1b931533f98a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420) (tstamp f28b8a8b-50c8-4e8f-8d82-601a9eca65c6)
    (at 147.335 58.395 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000063287bd8")
    (attr through_hole)
    (fp_text reference "JKD13" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a25568a-24cc-4475-a69d-114a8ab68798)
    )
    (fp_text value "COL3" (at -2.565 8.875 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 90decd66-947c-48f3-b5cc-139c72597575)
    )
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c670b608-5fc6-47e4-a03e-885c28f24324)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 18c41543-40bd-47e1-a82e-2c7f71aecc51))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 193d0481-9b37-45a3-87b9-3e1044a6cff6))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 33cb3509-99bf-43fe-a132-a1618ef07fd4))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 53a28410-0a7b-4864-ac49-ef7996aa7ab6))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer "F.SilkS") (width 0.12) (tstamp 8389c923-2068-42d3-b030-ae1ee817d1cb))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp f09b5523-c8ee-4a63-8664-b98a6b4ede0f))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 04191a3e-7b10-4a09-bfc7-e790ebcd6b47))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 55cd83cc-47a2-4ef8-bdba-2ee91c9340fa))
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 665b10ec-a198-424b-8885-689d289fd322))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer "F.CrtYd") (width 0.05) (tstamp 6a4d232c-3040-4241-8430-c6da4c521bd9))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp 60c818f8-c3a8-42c6-9aeb-4c040b67ef78))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 83e4795d-370c-423a-8599-1291edf48deb))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 908eeb2b-af96-4379-83cf-07228edc51bd))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp b1097f78-79e6-4090-b8a4-4d1f622c4bc4))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer "F.Fab") (width 0.1) (tstamp dd8ef3ea-082d-49b2-93cf-182247c5cd5a))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(DKD3-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp e2a24480-c1d5-4ce4-93d7-30c6a4960091))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(DKD11-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp bdc15c74-22ae-45df-9bae-3875cdbe204d))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(DKD19-Pad2)") (pinfunction "Pin_3") (pintype "passive") (tstamp d0ae2f0a-8052-4680-9382-bfdcb25a306e))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(DKD27-Pad2)") (pinfunction "Pin_4") (pintype "passive") (tstamp 4a0faaaa-e213-4fdf-87f4-0a84446a4cdc))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(DKD35-Pad2)") (pinfunction "Pin_5") (pintype "passive") (tstamp 70d26774-085a-41f6-a3f8-3a83b4f86d4a))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(DKD43-Pad2)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7ae187d0-c721-4218-9653-21a29684f3ad))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(DKD51-Pad2)") (pinfunction "Pin_7") (pintype "passive") (tstamp cf451772-ecd7-4a6c-a7ec-ade5b700f840))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(DKD59-Pad2)") (pinfunction "Pin_8") (pintype "passive") (tstamp e2c1a951-14d8-42e5-850d-96e2c677e3ba))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp f4ad093c-01d3-434e-983b-94c93f16ce21)
    (at 172.72 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006814be71")
    (attr through_hole)
    (fp_text reference "DKD20" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c72670d-08a8-4c2f-9f1e-ac7e05a442f9)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a7e8d126-14fa-4d62-9a04-8a686239598f)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8b02c2ee-732e-42e8-93d9-11adefad3ebc)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cee4307b-5581-4aa5-810a-e6fe0311ca35)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fca2071a-0fef-4b99-884b-63c80a1d982e)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 9e4f2798-ec8e-4bc0-af82-49ef88a00ac2))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp d644fd4c-e7fb-4fc2-86bb-756d35d73be8))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4b515717-3a2f-4465-9f2d-0c1a6d0c7d18))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 69af711a-896e-4382-9d20-867358e925f8))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 89ea4a50-99ca-4856-8e7d-1bd2dc599dcf))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp b3cf9e24-a7cb-4c3b-aacc-9797990ece3a))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp 025e38f8-95d2-4831-ba4f-e21f1dbfde64))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 1ee9dd42-97ab-4835-972f-fd74007d094b))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp cef75980-4e92-4f77-9048-750138e642ba))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(DKD20-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 24dfc7e5-67bd-48c7-a649-9fec49321fd9))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Pin:Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork" (layer "F.Cu")
    (tedit 5A1DC084) (tstamp f93318ea-75fc-439b-a84d-3325e06a4308)
    (at 43.18 58.42)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (property "Sheetfile" "keymatrix_extdiode_wire.kicad_sch")
    (property "Sheetname" "KeyMatrix wired")
    (path "/86fd0b4b-b0c8-4da7-922a-6650d5003f71/8a000d34-f9aa-4a96-b043-193e6a1c4d76")
    (attr through_hole)
    (fp_text reference "J39" (at 0 1.8) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bda3b583-fcf3-408e-a21b-ef3d435a31a4)
    )
    (fp_text value "C1" (at 0 -5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 68c30ce3-559e-432f-b064-542a6d7d824f)
    )
    (fp_text user "${REFERENCE}" (at 0 1.8) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9e2e2c12-24d4-485b-8a09-6cc5f2c61d6b)
    )
    (fp_line (start -0.95 -0.95) (end -0.95 0.95) (layer "F.SilkS") (width 0.12) (tstamp 11f24b31-83c9-4027-aae8-15fe14022316))
    (fp_line (start 0.9 -0.95) (end -0.95 -0.95) (layer "F.SilkS") (width 0.12) (tstamp 90ffcb4e-6813-4ae9-b923-cf828a0b9e25))
    (fp_line (start 0.9 -0.9) (end 0.9 -0.95) (layer "F.SilkS") (width 0.12) (tstamp cb0ac944-5fdf-4ddb-8033-c5e8bd84f4a1))
    (fp_line (start 0.9 0.95) (end 0.9 -0.9) (layer "F.SilkS") (width 0.12) (tstamp d9395ac3-ab1a-40d8-a2a4-6348105b716c))
    (fp_line (start -0.95 0.95) (end 0.9 0.95) (layer "F.SilkS") (width 0.12) (tstamp de0ad173-d7a5-4933-8ed7-987a8641b7ba))
    (fp_line (start 1.35 1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 31571f3e-b43e-4df7-bab9-6f2abfe9cb4a))
    (fp_line (start -1.4 -1.2) (end -1.4 1.2) (layer "F.CrtYd") (width 0.05) (tstamp 604c3200-28b9-4c61-a0d2-f7aa0a813f1a))
    (fp_line (start -1.4 -1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp 82e23e73-ee45-47f9-a6bf-2badcc93f90a))
    (fp_line (start 1.35 1.2) (end 1.35 -1.2) (layer "F.CrtYd") (width 0.05) (tstamp a8783df5-a72c-4d78-9adc-5920fc01bcfc))
    (fp_line (start -0.9 0.25) (end -0.9 -0.25) (layer "F.Fab") (width 0.12) (tstamp 37e7fd13-c5a7-491a-b156-387202ac29af))
    (fp_line (start 0.85 0.25) (end -0.9 0.25) (layer "F.Fab") (width 0.12) (tstamp 46c18a6c-2dc8-4a33-8531-233c2e3cb10f))
    (fp_line (start -0.9 -0.25) (end 0.85 -0.25) (layer "F.Fab") (width 0.12) (tstamp 6646907e-04e3-40d8-9e8d-5826fd162145))
    (fp_line (start 0.85 -0.25) (end 0.85 0.25) (layer "F.Fab") (width 0.12) (tstamp d2cb90bf-1cec-4aa3-b684-3da758aabd85))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 178 "Net-(J39-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 82399e9a-3ace-413e-a311-db8270bbac4b))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D0.7mm_L6.5mm_W1.8mm_FlatFork.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp f93ab8f3-48a6-45c8-8d50-c3bf6d6e9c19)
    (at 182.88 53.34 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-00006815b6ba")
    (attr through_hole)
    (fp_text reference "DKD52" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 35c98d64-89fc-4980-ae10-ed047a23805e)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6b7630e-b1bd-4ddc-8861-85fb56fee3c8)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aba92e3b-fd0f-4b5b-b6e6-89b7e5a7d7b3)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5f413ac5-c8bc-4704-9945-a67cc6543741)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a0802a64-4fc8-4c9f-b4b4-ed5b8ceeff2c)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 39c70d9c-b85f-4aab-b4a8-2cffd6c147e7))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp ba439d3b-9583-4ac9-af8f-e5b70231ec61))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 0f18d9c8-8b4f-49fd-8976-04d362cdd05c))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 4137d7bb-c388-422a-a4a4-ec98868e8e37))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp c05028dd-43dd-48b9-8bc5-78617767c09b))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp e95c9b2c-e5e9-48ae-ad2a-152cee330d9b))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp eb1a45b3-e066-44a5-aac3-78250fd1c5e2))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp d92a095b-4f1b-422f-b8a4-af648aba9cc0))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(DKD12-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 816eddcc-6cf7-4251-9a5d-132aa01b4e46))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(DKD52-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 280c4a9d-db18-4c6d-97cd-ce8ff73e9516))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp fcb6c635-dd99-4d0d-bf1e-c8d84ef23fa7)
    (at 167.64 33.02 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (property "Sheetfile" "keymatrix_diode.kicad_sch")
    (property "Sheetname" "Key Matrix Diode")
    (path "/814f65df-6ffe-42dd-b527-4f3b27cc438e/00000000-0000-0000-0000-000068161560")
    (attr through_hole)
    (fp_text reference "DKD64" (at 1.27 -2.326371 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 74e58857-ebb4-4683-b956-90e3d4528a99)
    )
    (fp_text value "1N4148" (at 1.27 3.215371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9d8daee2-797b-402b-a184-9ce119b621ab)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd949008-6d22-431e-8fcd-ccac9dbf8ec2)
    )
    (fp_text user "${REFERENCE}" (at 1.27 -2.326371 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 27f54a33-f48a-4313-b430-ae7b9acdb986)
    )
    (fp_text user "A" (at 4.34 0 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b3596439-890b-472c-95ac-eb1ee089a84b)
    )
    (fp_line (start 1.326371 0) (end 1.44 0) (layer "F.SilkS") (width 0.12) (tstamp 21a8cf8a-6763-489b-be37-5fdbe7313bdd))
    (fp_circle (center 0 0) (end 1.326371 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 51799ad2-9638-4dbc-aa09-35276d681349))
    (fp_line (start -1.25 -1.25) (end -1.25 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1368f918-4fdd-4e61-8977-94e0c8891430))
    (fp_line (start 3.59 1.25) (end 3.59 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 1c73b14f-3c46-423d-baf4-f447a779ba02))
    (fp_line (start 3.59 -1.25) (end -1.25 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5ba80fd8-ace8-49f2-8c53-01363c7e4073))
    (fp_line (start -1.25 1.25) (end 3.59 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 5d375c65-eb54-40ac-86e2-6aaffa4c24a0))
    (fp_line (start 0 0) (end 2.54 0) (layer "F.Fab") (width 0.1) (tstamp ab8b0060-0fb4-40b3-ba97-66f079235926))
    (fp_circle (center 0 0) (end 1 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 48c337f4-3f7d-451b-8bbe-ef8f912cecda))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(DKD16-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 3a3c4e33-b5eb-459b-8cc6-ff50bfa22bbe))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 150 "Net-(DKD64-Pad2)") (pinfunction "A") (pintype "passive") (tstamp a6afddd4-5d8c-4f6a-bc03-e1e91d4f1b2b))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 22.86 22.86) (end 93.98 60.96) (layer "F.SilkS") (width 0.12) (fill none) (tstamp afb8b546-2d34-49f9-b048-809d9d067ebb))
  (gr_line (start 60.96 40.64) (end 60.96 22.86) (layer "Dwgs.User") (width 0.15) (tstamp 1b0f80ce-3556-4b76-9706-d607659b7b6f))
  (gr_line (start 22.86 40.64) (end 60.96 40.64) (layer "Dwgs.User") (width 0.2) (tstamp 58fbda34-e62f-4525-a3b1-91a77c26980f))
  (gr_line (start 60.96 43.18) (end 22.86 43.18) (layer "Dwgs.User") (width 0.2) (tstamp 6c69c66f-6e3c-41e8-8da7-f4d17455a380))
  (gr_line (start 60.96 43.18) (end 60.96 60.96) (layer "Dwgs.User") (width 0.15) (tstamp 8544b55a-6739-490d-835e-4b5b67f1784f))
  (gr_line (start 162.56 78.74) (end 162.56 81.28) (layer "Dwgs.User") (width 0.15) (tstamp 9abf2699-7a67-468c-ae02-1e86c6fb7d63))
  (gr_line (start 137.16 78.74) (end 137.16 81.28) (layer "Dwgs.User") (width 0.15) (tstamp bd8c4ef8-c0b7-4ad2-8997-d8faefd4e8f0))
  (gr_line (start 93.98 22.86) (end 93.98 60.96) (layer "Edge.Cuts") (width 0.15) (tstamp 00000000-0000-0000-0000-000061fec633))
  (gr_line (start 60.96 60.96) (end 22.86 60.96) (layer "Edge.Cuts") (width 0.2) (tstamp 0d307ee3-061e-49b7-9aeb-7d710491afc9))
  (gr_line (start 22.86 91.44) (end 86.36 91.44) (layer "Edge.Cuts") (width 0.15) (tstamp 0d7333ca-0587-43cb-9af7-f59016c85820))
  (gr_line (start 60.96 22.86) (end 22.86 22.86) (layer "Edge.Cuts") (width 0.2) (tstamp 3d61f21c-8463-4865-919d-06cc81e88738))
  (gr_line (start 60.96 60.96) (end 93.98 60.96) (layer "Edge.Cuts") (width 0.2) (tstamp 46a7dba6-e84c-4e04-a72e-86e4c6e4e198))
  (gr_line (start 111.76 22.86) (end 187.96 22.86) (layer "Edge.Cuts") (width 0.2) (tstamp 57d86d0f-6776-4ecc-9849-ac260f5b0ff2))
  (gr_line (start 99.06 116.84) (end 88.9 116.84) (layer "Edge.Cuts") (width 0.05) (tstamp 582f3731-2b1d-41f9-bc19-6be19222b82f))
  (gr_line (start 187.96 76.2) (end 111.76 76.2) (layer "Edge.Cuts") (width 0.2) (tstamp 6051bc58-8dbb-4b22-97e8-7eb00f734903))
  (gr_line (start 22.86 60.96) (end 22.86 22.86) (layer "Edge.Cuts") (width 0.15) (tstamp 6597e724-ffad-43f1-9619-cca25cced87f))
  (gr_line (start 111.76 76.2) (end 111.76 22.86) (layer "Edge.Cuts") (width 0.2) (tstamp 6f358e43-79f9-4a38-b453-0c34277a27de))
  (gr_line (start 86.36 129.54) (end 22.86 129.54) (layer "Edge.Cuts") (width 0.2) (tstamp 73123040-7d91-4ece-b049-ee26e19f852f))
  (gr_line (start 86.36 129.54) (end 86.36 91.44) (layer "Edge.Cuts") (width 0.2) (tstamp aae7067d-9b5e-4a24-a5f6-2b78929cd219))
  (gr_line (start 60.96 22.86) (end 93.98 22.86) (layer "Edge.Cuts") (width 0.2) (tstamp aeae1c08-0511-41ff-896d-95b95a86eb35))
  (gr_line (start 187.96 22.86) (end 187.96 76.2) (layer "Edge.Cuts") (width 0.2) (tstamp c6151bb4-beb6-483d-8734-a5fd18c39104))
  (gr_line (start 22.86 129.54) (end 22.86 91.44) (layer "Edge.Cuts") (width 0.2) (tstamp c772e430-b260-4ff0-8e81-061edbadfc67))
  (gr_line (start 99.06 91.44) (end 99.06 116.84) (layer "Edge.Cuts") (width 0.05) (tstamp e0450c32-6c7d-418d-bc0f-aa7cbff84d35))
  (gr_line (start 88.9 91.44) (end 99.06 91.44) (layer "Edge.Cuts") (width 0.05) (tstamp e97a138c-907f-4ac2-909d-5420774bbc49))
  (gr_line (start 88.9 116.84) (end 88.9 91.44) (layer "Edge.Cuts") (width 0.05) (tstamp ee47853b-21ae-48ec-beb8-af4b8238c9b6))
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 05697a0e-112c-46cd-817f-8be0a3348a22)
    (pts (xy 22.86 60.96) (xy 93.98 60.96))
    (height 5.08)
    (gr_text "71,1200 mm" (at 58.42 64.24) (layer "Dwgs.User") (tstamp 05697a0e-112c-46cd-817f-8be0a3348a22)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 419ee62a-59be-4184-abc2-f987d6dbe27a)
    (pts (xy 111.76 22.86) (xy 187.96 22.86))
    (height -5.08)
    (gr_text "76,2000 mm" (at 149.86 15.98) (layer "Dwgs.User") (tstamp 419ee62a-59be-4184-abc2-f987d6dbe27a)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 5c7b7457-2362-4d39-9b08-119f7428e7ce)
    (pts (xy 22.86 129.54) (xy 22.86 91.44))
    (height -5.08)
    (gr_text "38,1000 mm" (at 15.98 110.49 90) (layer "Dwgs.User") (tstamp 5c7b7457-2362-4d39-9b08-119f7428e7ce)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 7da6dd22-6820-4812-8b65-ceb1440c016d)
    (pts (xy 93.98 60.96) (xy 93.98 22.86))
    (height 5.08)
    (gr_text "38.1000 mm" (at 97.26 41.91 90) (layer "Dwgs.User") (tstamp 7da6dd22-6820-4812-8b65-ceb1440c016d)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 8a67e56b-1765-48b0-ba88-e84e1861fe81)
    (pts (xy 187.96 22.86) (xy 187.96 76.2))
    (height -5.08)
    (gr_text "53,3400 mm" (at 191.24 49.53 90) (layer "Dwgs.User") (tstamp 8a67e56b-1765-48b0-ba88-e84e1861fe81)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 8dd54862-df4e-4faf-bdd6-951ae815871e)
    (pts (xy 22.86 91.44) (xy 86.36 91.44))
    (height -5.08)
    (gr_text "63,5000 mm" (at 54.61 84.56) (layer "Dwgs.User") (tstamp 8dd54862-df4e-4faf-bdd6-951ae815871e)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 9f5c7a80-7220-432e-865b-d1468e8a8d4c)
    (pts (xy 60.96 22.86) (xy 22.86 22.86))
    (height 5.08)
    (gr_text "38.1000 mm" (at 41.91 15.98) (layer "Dwgs.User") (tstamp 9f5c7a80-7220-432e-865b-d1468e8a8d4c)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp ab0384ad-0bc0-4c1a-a140-d93b08a8bb1b)
    (pts (xy 22.86 43.18) (xy 22.86 60.96))
    (height 5.079999)
    (gr_text "17,7800 mm" (at 15.980001 52.07 90) (layer "Dwgs.User") (tstamp ab0384ad-0bc0-4c1a-a140-d93b08a8bb1b)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp cc88164c-e798-4e72-b304-d7f93f5c4c65)
    (pts (xy 60.96 22.86) (xy 93.98 22.86))
    (height -5.248057)
    (gr_text "33,0200 mm" (at 77.47 15.811943) (layer "Dwgs.User") (tstamp cc88164c-e798-4e72-b304-d7f93f5c4c65)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp e04696fb-5bdb-4f42-8255-8e2001c19ba3)
    (pts (xy 22.86 40.64) (xy 22.86 22.86))
    (height -5.08)
    (gr_text "17,7800 mm" (at 15.98 31.75 90) (layer "Dwgs.User") (tstamp e04696fb-5bdb-4f42-8255-8e2001c19ba3)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 91.21 38.1) (end 91.21 27.94) (width 1) (layer "B.Cu") (net 1) (tstamp 37f1b63b-f111-472e-a1e0-cdd29eeee905))
  (segment (start 91.21 27.94) (end 76.2 27.94) (width 1) (layer "B.Cu") (net 1) (tstamp 60968a90-dfb4-40f1-955a-dc7de49bb0ab))
  (segment (start 76.2 27.94) (end 76.2 33.02) (width 1) (layer "B.Cu") (net 1) (tstamp 772de199-72ea-462b-9986-0bbdbbf5edfa))
  (segment (start 63.5 33.02) (end 71.12 33.02) (width 1) (layer "B.Cu") (net 1) (tstamp 79550362-ac1e-4c3f-ad25-45aa3bf3611a))
  (segment (start 71.12 33.02) (end 76.2 33.02) (width 1) (layer "B.Cu") (net 1) (tstamp 7ba154cb-06ee-4bab-b50e-d4eb610b0bf6))
  (segment (start 76.2 55.88) (end 76.2 33.02) (width 1) (layer "B.Cu") (net 1) (tstamp d9d8b053-e63f-4367-93b9-3af27580e0db))
  (segment (start 78.74 55.88) (end 76.2 55.88) (width 1) (layer "B.Cu") (net 1) (tstamp eb9cafe5-7c33-4cda-a85c-eab240f2ca89))
  (segment (start 66.04 40.64) (end 68.58 40.64) (width 1) (layer "B.Cu") (net 2) (tstamp 00000000-0000-0000-0000-000061fef61a))
  (segment (start 63.5 40.64) (end 66.04 40.64) (width 1) (layer "B.Cu") (net 2) (tstamp 00000000-0000-0000-0000-000061fef82d))
  (segment (start 88.9 33.02) (end 88.9 40.64) (width 1) (layer "B.Cu") (net 2) (tstamp 1ac7d70b-049b-43e6-95aa-c9bd5200fceb))
  (segment (start 63.5 40.64) (end 63.5 58.42) (width 1) (layer "B.Cu") (net 2) (tstamp 3f70548d-c145-40d7-b665-faff167579fe))
  (segment (start 81.28 58.42) (end 81.28 33.02) (width 1) (layer "B.Cu") (net 2) (tstamp 4d5d352c-980d-4805-8ecc-93bddef59b32))
  (segment (start 81.28 33.02) (end 88.9 33.02) (width 1) (layer "B.Cu") (net 2) (tstamp 793a58ac-b02d-4461-9935-6e03f855a299))
  (segment (start 63.5 58.42) (end 81.28 58.42) (width 1) (layer "B.Cu") (net 2) (tstamp a8419819-5d6a-4bca-919c-c81d99629775))
  (segment (start 88.9 40.64) (end 91.44 40.64) (width 1) (layer "B.Cu") (net 2) (tstamp ca5518eb-6e37-49c3-aac1-bc84fa41dfa6))
  (segment (start 70.89 35.56) (end 63.5 35.56) (width 1) (layer "B.Cu") (net 3) (tstamp 99e01380-6fe1-4389-b4d9-30f64a90ab1b))
  (segment (start 70.89 38.1) (end 63.5 38.1) (width 1) (layer "B.Cu") (net 4) (tstamp 4be0b938-babf-4f34-b2f0-ade9f0188d38))
  (segment (start 71.12 53.34) (end 71.12 55.88) (width 1) (layer "B.Cu") (net 9) (tstamp 84a508ab-f022-41bc-b09d-df562d10a71f))
  (segment (start 68.58 50.8) (end 68.58 55.88) (width 1) (layer "B.Cu") (net 10) (tstamp 9e5b5d5c-173e-4a46-a113-4100114e9aa0))
  (segment (start 71.12 50.8) (end 68.58 50.8) (width 1) (layer "B.Cu") (net 10) (tstamp b0394a41-fd64-45a7-8d6e-3109d76934f2))
  (segment (start 70.89 45.72) (end 73.66 45.72) (width 1) (layer "B.Cu") (net 11) (tstamp 5fbb285f-38f2-4cb3-8e9a-659d036348bb))
  (segment (start 73.66 45.72) (end 73.66 55.88) (width 1) (layer "B.Cu") (net 11) (tstamp b8e00c87-082f-49f1-a3f7-abf8106aed2f))
  (segment (start 30.48 25.4) (end 30.48 27.94) (width 1) (layer "B.Cu") (net 12) (tstamp 8918ad0e-9843-4827-b68e-6cab52806df4))
  (segment (start 27.94 27.94) (end 27.94 25.4) (width 1) (layer "B.Cu") (net 13) (tstamp 0bade7ce-1a13-4feb-803c-c3f66baf92bf))
  (segment (start 35.56 27.94) (end 35.56 25.4) (width 1) (layer "B.Cu") (net 14) (tstamp 345fa7fa-5734-400b-bf95-4810656a382e))
  (segment (start 27.94 35.585) (end 30.48 35.585) (width 1) (layer "B.Cu") (net 14) (tstamp 5c2d9a86-40d0-43a7-a065-b3cb4bcc80af))
  (segment (start 35.56 30.48) (end 35.56 27.94) (width 1) (layer "B.Cu") (net 14) (tstamp bd5adf77-acaf-4f80-9c97-26a3f93d6925))
  (segment (start 30.48 35.585) (end 30.48 30.48) (width 1) (layer "B.Cu") (net 14) (tstamp cda51170-7a58-4a3b-8284-3e801374e939))
  (segment (start 30.48 30.48) (end 35.56 30.48) (width 1) (layer "B.Cu") (net 14) (tstamp fbe51953-a661-4253-b343-75c549a50817))
  (segment (start 25.4 35.56) (end 25.4 38.1) (width 1) (layer "B.Cu") (net 15) (tstamp 5229cd57-cdd8-46bf-80cc-0a5016c831d4))
  (segment (start 38.1 27.94) (end 38.1 33.02) (width 1) (layer "B.Cu") (net 15) (tstamp 5e10ebed-e13b-4443-ae8d-93be866f9b73))
  (segment (start 38.1 33.02) (end 33.02 33.02) (width 1) (layer "B.Cu") (net 15) (tstamp 7cfb425c-f5fd-4603-b97b-2eef8a374a2d))
  (segment (start 33.02 38.1) (end 33.02 35.56) (width 1) (layer "B.Cu") (net 15) (tstamp d19130a8-d976-4407-b34d-b6f290901bb9))
  (segment (start 33.02 35.56) (end 33.02 33.02) (width 1) (layer "B.Cu") (net 15) (tstamp d570e93c-5545-48d4-af35-1e19dc141390))
  (segment (start 25.4 38.1) (end 33.02 38.1) (width 1) (layer "B.Cu") (net 15) (tstamp ee4fa114-b0a8-4583-9c63-25e46f8e5051))
  (segment (start 38.1 35.56) (end 38.1 38.1) (width 1) (layer "B.Cu") (net 16) (tstamp 20b3822b-614a-40f5-920b-cdbab9d6362d))
  (segment (start 154.94 63.5) (end 157.48 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 0667208e-872f-444a-9ed0-78a1b5f392d2))
  (segment (start 149.86 63.5) (end 147.32 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 22fd57c4-481e-4417-b920-694451210da2))
  (segment (start 134.62 53.34) (end 137.16 53.34) (width 1) (layer "B.Cu") (net 17) (tstamp 27c272da-77b4-480f-9bc8-84e4fe805cf2))
  (segment (start 137.16 58.42) (end 142.24 58.42) (width 1) (layer "B.Cu") (net 17) (tstamp 2931831a-a9e5-496a-9dc2-d28f97a136be))
  (segment (start 160.02 63.5) (end 162.56 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 524dc8d0-13b4-43fe-b274-8ac08bc4b894))
  (segment (start 142.24 63.5) (end 147.32 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 75bf6c5c-9f72-49e5-bfbf-cee24998c85f))
  (segment (start 160.02 63.5) (end 157.48 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 7aad0cca-fb50-4041-9a10-5380cb0860ac))
  (segment (start 154.94 63.5) (end 152.4 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 7fd11519-eb9e-4413-8ca2-e43e38c699f6))
  (segment (start 142.24 58.42) (end 142.24 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 8bcf6a44-9c90-494c-8000-0e24a486da16))
  (segment (start 165.1 63.5) (end 162.56 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp 969d876f-dc87-40bf-9e96-03cbb9ea5e82))
  (segment (start 137.16 53.34) (end 137.16 58.42) (width 1) (layer "B.Cu") (net 17) (tstamp b8166eaa-020c-4da1-a55e-954a75de49ab))
  (segment (start 149.86 63.5) (end 152.4 63.5) (width 1) (layer "B.Cu") (net 17) (tstamp bc29a09d-ebbe-4bab-9edb-114e75ee17a4))
  (segment (start 86.36 45.72) (end 91.44 45.72) (width 1) (layer "B.Cu") (net 19) (tstamp 00000000-0000-0000-0000-000061fef7a9))
  (segment (start 86.36 48.26) (end 91.44 48.26) (width 1) (layer "B.Cu") (net 20) (tstamp 00000000-0000-0000-0000-000061fef7a6))
  (segment (start 68.58 48.26) (end 71.12 48.26) (width 1) (layer "B.Cu") (net 21) (tstamp 767d2f0d-bfd0-43a6-b026-106981f30c14))
  (segment (start 68.58 43.18) (end 68.58 48.26) (width 1) (layer "B.Cu") (net 21) (tstamp c9b79ea2-d1f8-429e-9487-b3ffb383cb72))
  (segment (start 139.7 55.88) (end 144.78 55.88) (width 1) (layer "B.Cu") (net 24) (tstamp 0ac5faed-9e87-462c-bb1a-327838d4535d))
  (segment (start 177.8 63.5) (end 180.34 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp 11cae898-6e02-4314-87c3-bfa88f249303))
  (segment (start 180.34 63.5) (end 182.88 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp 3a4d7b94-8b26-4555-b396-f2e88aea5db3))
  (segment (start 144.78 55.88) (end 144.78 60.96) (width 1) (layer "B.Cu") (net 24) (tstamp 51cbce53-42ab-4665-b53d-29bf1c7b440f))
  (segment (start 170.18 63.5) (end 172.72 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp 60a7dcc1-b459-4b69-be02-f48b66a815f0))
  (segment (start 175.26 63.5) (end 177.8 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp 7401f61b-dc36-4f5a-ba3e-b101a22bf1fc))
  (segment (start 134.62 50.8) (end 139.7 50.8) (width 1) (layer "B.Cu") (net 24) (tstamp 7e05e373-fc2c-4f47-bb42-ec8f165d4b00))
  (segment (start 182.88 63.5) (end 185.42 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp 8c4cd1a2-9a92-4fba-aa2e-8b86c17dce10))
  (segment (start 139.7 50.8) (end 139.7 55.88) (width 1) (layer "B.Cu") (net 24) (tstamp ab6d2253-a054-4ad9-8cd2-c099c3c7d414))
  (segment (start 144.78 60.96) (end 167.64 60.96) (width 1) (layer "B.Cu") (net 24) (tstamp d03e573b-1ffd-46d8-b74d-957f306b168f))
  (segment (start 167.64 60.96) (end 167.64 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp ebbfb981-8f2f-4afa-a90c-017050d6801e))
  (segment (start 167.64 63.5) (end 170.18 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp f8df4375-570f-4eb0-868e-4f350bd24547))
  (segment (start 172.72 63.5) (end 175.26 63.5) (width 1) (layer "B.Cu") (net 24) (tstamp fbca7d5b-4a19-4f46-9697-74b3068179aa))
  (segment (start 147.32 53.34) (end 149.86 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp 00c9c1c9-df78-4bf8-a378-9edee7dafbe3))
  (segment (start 134.62 48.26) (end 142.24 48.26) (width 1) (layer "B.Cu") (net 25) (tstamp 127b0e8c-8b10-4db4-b691-908ac98caaf1))
  (segment (start 142.24 48.26) (end 142.24 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp 3019c847-3ccf-490a-9dd6-694227c3fba5))
  (segment (start 152.4 53.34) (end 154.94 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp 6428332e-b689-4aa8-86bb-3bee31b6f177))
  (segment (start 142.24 53.34) (end 147.32 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp 741561bb-6157-4c58-bb00-0f2a32b21238))
  (segment (start 149.86 53.34) (end 152.4 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp 92419cc9-1070-47aa-876c-2cf8f5a03a47))
  (segment (start 162.56 53.34) (end 165.1 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp ad4fcc27-bf1e-4e2e-ab26-9b8032da7693))
  (segment (start 157.48 53.34) (end 160.02 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp c7524402-4dbd-4d05-888d-edab7e79a150))
  (segment (start 154.94 53.34) (end 157.48 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp d5128f0b-0a4f-4337-a7f7-9a3dfe4ad4f9))
  (segment (start 160.02 53.34) (end 162.56 53.34) (width 1) (layer "B.Cu") (net 25) (tstamp fed6a1e7-e233-4dff-87e0-8992a65c8dd0))
  (segment (start 167.64 50.8) (end 167.64 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp 098afe52-27f0-4ec0-bf39-4eb766d2a851))
  (segment (start 182.88 53.34) (end 185.42 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp 1ec648ca-df29-4910-86ed-6f48e345dbdb))
  (segment (start 180.34 53.34) (end 182.88 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp 30cf5573-2ac5-4d4b-8678-7fcebe2bcd36))
  (segment (start 134.62 45.72) (end 144.78 45.72) (width 1) (layer "B.Cu") (net 26) (tstamp 5b0bc5b9-a0c7-4929-ad56-3d31300558d0))
  (segment (start 170.18 53.34) (end 172.72 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp 6b013cb8-9e09-4a62-b02d-814d5cfa604e))
  (segment (start 167.64 53.34) (end 170.18 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp 782e74f8-8e76-4e6f-bfec-df9b9d96b19d))
  (segment (start 144.78 50.8) (end 167.64 50.8) (width 1) (layer "B.Cu") (net 26) (tstamp 8a8a5a4c-988b-4f52-9e79-9ee7e26a613f))
  (segment (start 175.26 53.34) (end 177.8 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp 986fa662-6dc8-4009-9871-995c9cfdbebc))
  (segment (start 144.78 45.72) (end 144.78 50.8) (width 1) (layer "B.Cu") (net 26) (tstamp c1960af0-4a97-4f83-8219-ad58084d4586))
  (segment (start 177.8 53.34) (end 180.34 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp cd1b9f49-f6c4-4c81-a715-14d19fd506d7))
  (segment (start 172.72 53.34) (end 175.26 53.34) (width 1) (layer "B.Cu") (net 26) (tstamp de7d8275-fd45-47d5-ae9a-4b0c51b81f57))
  (segment (start 149.86 43.18) (end 152.4 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp 0de7d0e7-c8d5-482b-8e8a-d56acfc6ebd8))
  (segment (start 147.32 43.18) (end 149.86 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp 1aaf34a3-282e-4633-82fa-9d6cdf32efbb))
  (segment (start 157.48 43.18) (end 160.02 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp 3b450865-b2ef-4d25-9b34-4d42975b5e24))
  (segment (start 154.94 43.18) (end 157.48 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp 4c38e5ef-0105-4756-a059-34a9c3247d1f))
  (segment (start 160.02 43.18) (end 162.56 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp 7cc510d9-2339-42a7-bb31-eff1142f0636))
  (segment (start 162.56 43.18) (end 165.1 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp a60f8360-f38f-439d-b446-391101ae4282))
  (segment (start 152.4 43.18) (end 154.94 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp d35d7027-ac1b-44b2-9664-3d8a37ee0f4e))
  (segment (start 134.62 43.18) (end 147.32 43.18) (width 1) (layer "B.Cu") (net 27) (tstamp d7b67c11-d515-46cf-bcf0-0f0ef2d0158a))
  (segment (start 170.18 43.18) (end 172.72 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp 119c633c-175b-4b38-bbc1-1a076032c16e))
  (segment (start 134.62 40.64) (end 167.64 40.64) (width 1) (layer "B.Cu") (net 28) (tstamp 334fc29f-7949-4f5e-a341-b51e61ea0081))
  (segment (start 177.8 43.18) (end 180.34 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp 43f4cf53-1dc5-4426-bbd2-fabe9c3d45ec))
  (segment (start 167.64 40.64) (end 167.64 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp 5b29962f-685a-409c-915c-9c4a92ed442a))
  (segment (start 180.34 43.18) (end 182.88 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp 6ceb10bf-4340-4309-8250-882c2b60a70e))
  (segment (start 182.88 43.18) (end 185.42 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp 946a171e-cd55-473d-bab9-8d2c7c34161c))
  (segment (start 172.72 43.18) (end 175.26 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp c66790a8-2c84-47da-b059-a728d9f51463))
  (segment (start 175.26 43.18) (end 177.8 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp cb4b7bcd-f8cd-4398-9baf-986854c6b2ae))
  (segment (start 167.64 43.18) (end 170.18 43.18) (width 1) (layer "B.Cu") (net 28) (tstamp fb4e7351-d265-4999-adf6-bc7596c21cf3))
  (segment (start 157.48 33.02) (end 160.02 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 0d32fbdb-2a37-4863-af10-fc85c1c6174f))
  (segment (start 149.86 33.02) (end 152.4 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 18b6dcb6-5ab3-481b-b998-33e8cf6d281f))
  (segment (start 147.32 33.02) (end 149.86 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 25ca9482-069d-43de-b77e-6f2ad77fa017))
  (segment (start 144.78 33.02) (end 147.32 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 539dec9e-2c45-4201-ab13-cbbbab8fc31b))
  (segment (start 144.78 38.1) (end 144.78 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 7308e13a-4809-4e8e-af65-9905819aa376))
  (segment (start 162.56 33.02) (end 165.1 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 75d5a810-84fd-42c4-a0b7-6b82d09662a2))
  (segment (start 154.94 33.02) (end 157.48 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp 7be13a36-eb8e-440f-aaac-2fd6665d9f61))
  (segment (start 134.62 38.1) (end 144.78 38.1) (width 1) (layer "B.Cu") (net 29) (tstamp 91c69423-de51-44fe-bc70-fec455b50634))
  (segment (start 160.02 33.02) (end 162.56 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp a072347a-1cac-4ead-8c61-cfe38fd40342))
  (segment (start 152.4 33.02) (end 154.94 33.02) (width 1) (layer "B.Cu") (net 29) (tstamp fa16f237-4e21-4b18-8c54-f7de4e62bbb6))
  (segment (start 86.36 43.18) (end 91.44 43.18) (width 1) (layer "B.Cu") (net 30) (tstamp 5217593b-12c6-4e51-8978-ee739bb65a01))
  (segment (start 86.36 53.34) (end 86.36 55.88) (width 1) (layer "B.Cu") (net 31) (tstamp 6703d014-3f3c-4fce-a948-5810f768589a))
  (segment (start 86.36 50.8) (end 91.44 50.8) (width 1) (layer "B.Cu") (net 32) (tstamp 00000000-0000-0000-0000-000061fef81b))
  (segment (start 83.82 40.64) (end 83.82 55.88) (width 1) (layer "B.Cu") (net 33) (tstamp 2169a7c4-ccbe-4a75-bd5d-301b3e899865))
  (segment (start 86.36 40.64) (end 83.82 40.64) (width 1) (layer "B.Cu") (net 33) (tstamp f319a88e-154c-4208-8701-4c90befb33ca))
  (segment (start 142.24 35.56) (end 142.24 30.48) (width 1) (layer "B.Cu") (net 34) (tstamp 1b00c2af-158e-4e04-ada0-b2313f59b860))
  (segment (start 170.18 33.02) (end 172.72 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp 41fc1c23-edd4-45a5-8036-7f62b013770f))
  (segment (start 175.26 33.02) (end 177.8 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp 42b7a68a-3837-4773-af68-a35059da48c3))
  (segment (start 142.24 30.48) (end 167.64 30.48) (width 1) (layer "B.Cu") (net 34) (tstamp 871e96ce-ad88-41b6-8fea-2cbba569a65b))
  (segment (start 167.64 33.02) (end 170.18 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp 9b4851fe-4e2f-4de0-a685-8e53004d88aa))
  (segment (start 182.88 33.02) (end 185.42 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp 9e5b0177-ea58-4f76-8b57-ff1c6e52d9df))
  (segment (start 180.34 33.02) (end 182.88 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp b7340f23-0eaa-48ae-aea8-b5b53a0ae99a))
  (segment (start 134.62 35.56) (end 142.24 35.56) (width 1) (layer "B.Cu") (net 34) (tstamp df656da3-6e12-42dd-a970-65bdf2192899))
  (segment (start 177.8 33.02) (end 180.34 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp dfa2c928-7d9a-4cd3-90db-112716296421))
  (segment (start 167.64 30.48) (end 167.64 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp e8cb6cb3-dd2b-4328-8592-132e369ebb71))
  (segment (start 172.72 33.02) (end 175.26 33.02) (width 1) (layer "B.Cu") (net 34) (tstamp f9e60890-c09c-4221-9409-43a2ec4885e8))
  (segment (start 58.42 96.52) (end 63.5 96.52) (width 1) (layer "B.Cu") (net 35) (tstamp 7ffe2fe0-e283-4008-bb81-b744115763a3))
  (segment (start 60.96 99.06) (end 60.96 99.035) (width 1) (layer "B.Cu") (net 36) (tstamp 1ec1a39e-5500-45a6-85b4-b30fd51c077b))
  (segment (start 58.42 99.06) (end 60.96 99.06) (width 1) (layer "B.Cu") (net 36) (tstamp efffdc3a-c78d-4adf-816d-74eb08a95164))
  (segment (start 60.96 99.035) (end 63.5 99.035) (width 1) (layer "B.Cu") (net 36) (tstamp f8011993-5cf3-4747-8305-09d6c4cc0a7f))
  (segment (start 55.88 99.06) (end 50.8 99.06) (width 1) (layer "B.Cu") (net 37) (tstamp 04610a05-94dc-4bf1-b81f-762b61d295f9))
  (segment (start 60.96 104.115) (end 58.42 104.14) (width 1) (layer "B.Cu") (net 37) (tstamp 20771021-7905-489e-9c92-945889a3f78f))
  (segment (start 55.88 104.14) (end 55.88 99.06) (width 1) (layer "B.Cu") (net 37) (tstamp 37962402-dd9e-426a-9c92-a475328cd3a1))
  (segment (start 58.42 104.14) (end 55.88 104.14) (width 1) (layer "B.Cu") (net 37) (tstamp 73256830-9a41-4d6c-afa3-5b76e1aa47f1))
  (segment (start 50.8 93.98) (end 50.8 96.52) (width 1) (layer "B.Cu") (net 37) (tstamp 93120b4f-0606-46bd-bd3d-8a65e1b2928f))
  (segment (start 50.8 96.52) (end 50.8 99.06) (width 1) (layer "B.Cu") (net 37) (tstamp 982e1a04-c954-4d77-b933-63f53f4010bc))
  (segment (start 60.96 101.6) (end 60.985 101.575) (width 1) (layer "B.Cu") (net 37) (tstamp d63b5c76-a8e8-4ff4-8cfe-d3f696f9e893))
  (segment (start 60.96 104.115) (end 60.96 101.6) (width 1) (layer "B.Cu") (net 37) (tstamp d68426fe-0e60-4f3c-b69a-58f51622af5a))
  (segment (start 60.985 101.575) (end 63.5 101.575) (width 1) (layer "B.Cu") (net 37) (tstamp f9138fb1-4e9b-4c0a-a6f1-bc9a6cdec635))
  (segment (start 53.34 106.68) (end 58.42 106.68) (width 1) (layer "B.Cu") (net 38) (tstamp 16d0caa3-5850-4ad2-a5b4-98be779ddb19))
  (segment (start 63.5 106.68) (end 63.5 104.115) (width 1) (layer "B.Cu") (net 38) (tstamp 235a635c-ebdd-4a3f-b968-63be7d3f6e65))
  (segment (start 53.34 101.6) (end 53.34 106.68) (width 1) (layer "B.Cu") (net 38) (tstamp 3376eb55-d1c4-41fa-85f6-b25849c717c8))
  (segment (start 50.8 101.6) (end 53.34 101.6) (width 1) (layer "B.Cu") (net 38) (tstamp b7ad3053-bada-408b-853d-a64274a09935))
  (segment (start 63.5 106.68) (end 58.42 106.68) (width 1) (layer "B.Cu") (net 38) (tstamp c58acce4-a818-4c96-b08e-54e2c0d6f7b9))
  (segment (start 129.54 25.4) (end 127 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdeecc))
  (segment (start 139.7 25.4) (end 137.16 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdf5d4))
  (segment (start 132.08 25.4) (end 129.54 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdf7c6))
  (segment (start 127 25.4) (end 124.46 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdf7d8))
  (segment (start 137.16 25.4) (end 134.62 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdf8a7))
  (segment (start 124.46 25.4) (end 121.92 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdf8bf))
  (segment (start 134.62 25.4) (end 132.08 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 00000000-0000-0000-0000-000061fdfce5))
  (segment (start 114.3 25.4) (end 121.92 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 0a0346a5-cc15-49b4-b524-e2b1fe239833))
  (segment (start 127 43.18) (end 114.3 43.18) (width 1) (layer "B.Cu") (net 47) (tstamp 265edf09-7837-44bd-bbba-e573c921fdc9))
  (segment (start 114.3 43.18) (end 114.3 25.4) (width 1) (layer "B.Cu") (net 47) (tstamp 712871c5-c2b3-4736-b68a-703b64855ed4))
  (segment (start 71.12 127) (end 68.58 127) (width 1) (layer "B.Cu") (net 48) (tstamp 09651a32-2ffb-4ba7-bacf-01ea96d1be02))
  (segment (start 73.66 127) (end 71.12 127) (width 1) (layer "B.Cu") (net 48) (tstamp 5896687c-e9a8-4aef-a628-1eb2b86ccd16))
  (segment (start 76.2 127) (end 73.66 127) (width 1) (layer "B.Cu") (net 48) (tstamp 60234cff-4d98-47cd-98a4-0dd0dca159ff))
  (segment (start 68.58 127) (end 66.04 127) (width 1) (layer "B.Cu") (net 48) (tstamp 6dfab612-4b24-425c-8f62-e2bf4099b3cd))
  (segment (start 63.5 127) (end 58.42 127) (width 1) (layer "B.Cu") (net 48) (tstamp 7588450f-6150-4ede-90f2-5facd1af394d))
  (segment (start 78.74 127) (end 76.2 127) (width 1) (layer "B.Cu") (net 48) (tstamp 7cd2341d-4c64-4afc-9b2f-b50569e7f684))
  (segment (start 81.28 127) (end 78.74 127) (width 1) (layer "B.Cu") (net 48) (tstamp de894b3d-4072-496d-9305-4c90628f05b6))
  (segment (start 66.04 127) (end 63.5 127) (width 1) (layer "B.Cu") (net 48) (tstamp fdaa131a-bfa4-4876-a88c-d3cb6f2d3c38))
  (segment (start 81.28 124.46) (end 58.42 124.46) (width 1) (layer "B.Cu") (net 49) (tstamp fc3db889-c906-4cf5-b504-823c88b3b3b8))
  (segment (start 81.28 121.92) (end 58.42 121.92) (width 1) (layer "B.Cu") (net 50) (tstamp 98b78fdb-608b-4db7-a3ce-1a416d1d2ad0))
  (segment (start 58.42 119.38) (end 81.28 119.38) (width 1) (layer "B.Cu") (net 51) (tstamp 14a8f7d1-6e93-4bd3-b053-b00fed2e7fb8))
  (segment (start 81.28 116.84) (end 58.42 116.84) (width 1) (layer "B.Cu") (net 52) (tstamp 49184143-0723-474b-9715-ecd741597af4))
  (segment (start 58.42 114.3) (end 81.28 114.3) (width 1) (layer "B.Cu") (net 57) (tstamp 4266ce3d-7d9d-47df-8fbe-f0a6c2411338))
  (segment (start 58.42 111.76) (end 81.28 111.76) (width 1) (layer "B.Cu") (net 58) (tstamp a0126f95-0f49-4b8f-876a-762ac24812eb))
  (segment (start 58.42 109.22) (end 81.28 109.22) (width 1) (layer "B.Cu") (net 59) (tstamp d73c318c-aaba-4f18-8520-b7020fa6e453))
  (segment (start 50.8 109.22) (end 27.94 109.22) (width 1) (layer "B.Cu") (net 60) (tstamp ea54c124-b52d-492a-bf9b-15af7fdd574e))
  (segment (start 50.8 111.76) (end 27.965 111.76) (width 1) (layer "B.Cu") (net 61) (tstamp 6c2622f0-9263-4638-987a-a92f72d6c5bf))
  (segment (start 27.965 111.76) (end 27.94 111.785) (width 1) (layer "B.Cu") (net 61) (tstamp 816f643a-39ec-45bd-beb5-7993889300ec))
  (segment (start 50.8 114.3) (end 27.94 114.3) (width 1) (layer "B.Cu") (net 62) (tstamp 7847e806-7e06-4653-a19e-a5bb4381303d))
  (segment (start 50.8 116.84) (end 27.94 116.84) (width 1) (layer "B.Cu") (net 63) (tstamp cf3da0fe-0dd1-4725-8c77-123d09e9cc1d))
  (segment (start 50.8 119.38) (end 27.94 119.38) (width 1) (layer "B.Cu") (net 64) (tstamp 578792be-bc65-40ac-9353-2bbbe538bafc))
  (segment (start 50.8 121.92) (end 27.94 121.92) (width 1) (layer "B.Cu") (net 65) (tstamp 29cf7012-6e45-4cf4-a2ea-811cf0d6a07a))
  (segment (start 50.8 124.46) (end 27.94 124.46) (width 1) (layer "B.Cu") (net 66) (tstamp f929717e-253f-475a-95b7-793433223175))
  (segment (start 50.8 127) (end 27.94 127) (width 1) (layer "B.Cu") (net 67) (tstamp 7638e151-4aaf-4c29-af58-18220e898536))
  (segment (start 121.92 33.02) (end 124.46 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-00006201033b))
  (segment (start 134.62 33.02) (end 137.16 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-00006201033e))
  (segment (start 132.08 33.02) (end 134.62 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-000062010341))
  (segment (start 124.46 33.02) (end 127 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-000062010344))
  (segment (start 129.54 33.02) (end 132.08 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-000062010347))
  (segment (start 127 33.02) (end 129.54 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-00006201034a))
  (segment (start 137.16 33.02) (end 139.7 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 00000000-0000-0000-0000-00006201034d))
  (segment (start 127 35.56) (end 127 33.02) (width 1) (layer "B.Cu") (net 68) (tstamp 151c2a68-0d91-4cba-8b9c-7df5e146d184))
  (segment (start 137.16 30.48) (end 134.62 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103d4))
  (segment (start 127 30.48) (end 124.46 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103d7))
  (segment (start 134.62 30.48) (end 132.08 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103da))
  (segment (start 124.46 30.48) (end 121.92 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103dd))
  (segment (start 132.08 30.48) (end 129.54 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103e0))
  (segment (start 139.7 30.48) (end 137.16 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103e3))
  (segment (start 129.54 30.48) (end 127 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 00000000-0000-0000-0000-0000620103e6))
  (segment (start 119.38 30.48) (end 121.92 30.48) (width 1) (layer "B.Cu") (net 69) (tstamp 3db00451-fbc3-4980-9f8f-a31cdc894554))
  (segment (start 119.38 30.48) (end 119.38 38.1) (width 1) (layer "B.Cu") (net 69) (tstamp acb23d9e-cd27-4f6b-895f-05861dc7fc17))
  (segment (start 119.38 38.1) (end 127 38.1) (width 1) (layer "B.Cu") (net 69) (tstamp ad337a6e-604f-4455-8e33-0bb2e41f8410))
  (segment (start 127 27.94) (end 124.46 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fde5a2))
  (segment (start 121.92 27.94) (end 124.46 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fde8d5))
  (segment (start 134.62 27.94) (end 132.08 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fdf7b4))
  (segment (start 137.16 27.94) (end 134.62 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fdf8a4))
  (segment (start 127 27.94) (end 129.54 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fdf8b6))
  (segment (start 139.7 27.94) (end 137.16 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fdf9be))
  (segment (start 132.08 27.94) (end 129.54 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 00000000-0000-0000-0000-000061fdfc9d))
  (segment (start 116.84 27.94) (end 121.92 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 6dc7fba1-3835-4780-95f9-514a460ad0bb))
  (segment (start 127 40.64) (end 116.84 40.64) (width 1) (layer "B.Cu") (net 70) (tstamp 93e34d46-eb02-484a-9d7d-0d282e60f159))
  (segment (start 116.84 40.64) (end 116.84 27.94) (width 1) (layer "B.Cu") (net 70) (tstamp 9b68f0db-4a03-4221-adc1-2670068a903e))
  (segment (start 114.3 45.72) (end 127 45.72) (width 1) (layer "B.Cu") (net 71) (tstamp 2875450c-a944-4d7e-bd18-6e20b5a70be1))
  (segment (start 114.3 73.66) (end 114.3 45.72) (width 1) (layer "B.Cu") (net 71) (tstamp 36115100-58a3-48fc-9859-463a97d4b58e))
  (segment (start 116.84 48.26) (end 116.84 73.66) (width 1) (layer "B.Cu") (net 72) (tstamp 32362359-f9a6-4cc8-a646-cc3a73028d36))
  (segment (start 127 48.26) (end 116.84 48.26) (width 1) (layer "B.Cu") (net 72) (tstamp 445e806a-62f7-4075-acfb-9683f9833ffb))
  (segment (start 119.38 50.8) (end 119.38 73.66) (width 1) (layer "B.Cu") (net 73) (tstamp 2119e7e9-140d-48f6-bf32-c6a02e29b4bb))
  (segment (start 127 50.8) (end 119.38 50.8) (width 1) (layer "B.Cu") (net 73) (tstamp d39a7a74-952d-40f3-9f04-e89c4c44bee1))
  (segment (start 121.92 68.58) (end 121.92 66.04) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fde4df))
  (segment (start 121.92 58.42) (end 121.92 55.88) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fde5a5))
  (segment (start 121.92 63.5) (end 121.92 60.96) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fdeec3))
  (segment (start 121.92 53.34) (end 121.92 55.88) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fdf052))
  (segment (start 121.92 66.04) (end 121.92 63.5) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fdf277))
  (segment (start 121.92 60.96) (end 121.92 58.42) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fdf28c))
  (segment (start 121.92 73.66) (end 121.92 71.12) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fdf2fb))
  (segment (start 121.92 71.12) (end 121.92 68.58) (width 1) (layer "B.Cu") (net 74) (tstamp 00000000-0000-0000-0000-000061fdf9b5))
  (segment (start 127 53.34) (end 121.92 53.34) (width 1) (layer "B.Cu") (net 74) (tstamp a1223b95-aa11-427a-b201-9190a86a68be))
  (segment (start 58.42 27.94) (end 58.42 25.4) (width 1) (layer "B.Cu") (net 75) (tstamp 97d666e9-392b-4f0c-93ba-3e0d45dca2b3))
  (segment (start 55.88 27.94) (end 55.88 25.4) (width 1) (layer "B.Cu") (net 76) (tstamp 9fd33adc-e4ce-4d70-8686-06f7043353d9))
  (segment (start 53.34 27.94) (end 53.34 25.4) (width 1) (layer "B.Cu") (net 77) (tstamp 32a54804-75d5-42bd-a73c-9926aaef52c9))
  (segment (start 50.8 27.94) (end 50.8 25.4) (width 1) (layer "B.Cu") (net 78) (tstamp 862cd59a-2451-440d-b853-4aefbbb15454))
  (segment (start 134.62 60.96) (end 132.08 60.96) (width 1) (layer "B.Cu") (net 79) (tstamp 023aac86-48c5-42f5-b426-074128ded4b1))
  (segment (start 134.62 60.96) (end 137.16 60.96) (width 1) (layer "B.Cu") (net 79) (tstamp 569eec56-192f-4f3d-85de-66112d72b628))
  (segment (start 132.08 60.96) (end 132.08 55.88) (width 1) (layer "B.Cu") (net 79) (tstamp 7cf14c0f-d8a6-4f0b-bb50-32fbcf4700c0))
  (segment (start 132.08 55.88) (end 127 55.88) (width 1) (layer "B.Cu") (net 79) (tstamp 9908135f-2fd0-42c2-a2be-20fb90581cac))
  (segment (start 137.16 60.96) (end 137.16 71.12) (width 1) (layer "B.Cu") (net 79) (tstamp ad24b7c6-0b86-413a-bdaf-b80a361ca852))
  (segment (start 134.62 63.5) (end 134.62 66.04) (width 1) (layer "B.Cu") (net 80) (tstamp 00000000-0000-0000-0000-000061fdea49))
  (segment (start 134.62 66.04) (end 134.62 68.58) (width 1) (layer "B.Cu") (net 80) (tstamp 00000000-0000-0000-0000-000061fdee30))
  (segment (start 134.62 73.66) (end 134.62 68.58) (width 1) (layer "B.Cu") (net 80) (tstamp 61778803-c6dd-423d-8dac-10290d90c589))
  (segment (start 127 58.42) (end 124.46 58.42) (width 1) (layer "B.Cu") (net 80) (tstamp 823f5009-69dc-4625-9377-7516b5c0efb3))
  (segment (start 124.46 58.42) (end 124.46 73.66) (width 1) (layer "B.Cu") (net 80) (tstamp 8981568a-e0a3-4153-b9a3-2c632ebd312a))
  (segment (start 124.46 73.66) (end 134.62 73.66) (width 1) (layer "B.Cu") (net 80) (tstamp d1dcf9d7-584b-4ea5-b882-50872338fa8c))
  (segment (start 132.08 63.5) (end 132.08 71.12) (width 1) (layer "B.Cu") (net 81) (tstamp b9447259-ddad-453e-8cc7-4823b1562d51))
  (segment (start 127 63.5) (end 132.08 63.5) (width 1) (layer "B.Cu") (net 81) (tstamp c17b1776-266f-4ea3-b7d9-46cd1c9c1cfb))
  (segment (start 127 66.04) (end 129.54 66.04) (width 1) (layer "B.Cu") (net 82) (tstamp 5159b070-54aa-425c-a184-02e41b96e11d))
  (segment (start 129.54 66.04) (end 129.54 71.12) (width 1) (layer "B.Cu") (net 82) (tstamp ad28057c-41ec-44a4-ae80-6ce05070caa6))
  (segment (start 147.32 66.04) (end 147.32 68.58) (width 1) (layer "B.Cu") (net 83) (tstamp 0a83f85d-78ad-480a-a5ba-773caced8f09))
  (segment (start 149.86 68.58) (end 149.86 66.04) (width 1) (layer "B.Cu") (net 84) (tstamp a6460cc6-b11c-4dff-a0ea-9de680e68ca8))
  (segment (start 167.64 68.58) (end 167.64 66.04) (width 1) (layer "B.Cu") (net 85) (tstamp 9116f42f-8d27-4055-8fab-af8b6ed6959f))
  (segment (start 170.18 66.04) (end 170.18 68.58) (width 1) (layer "B.Cu") (net 86) (tstamp 3aec5e23-e675-4bcf-9a9e-48cb59d51927))
  (segment (start 147.32 55.88) (end 147.32 58.42) (width 1) (layer "B.Cu") (net 87) (tstamp c14f4f41-991c-47f8-ba74-4a4e89170acf))
  (segment (start 149.86 58.42) (end 149.86 55.88) (width 1) (layer "B.Cu") (net 88) (tstamp 01657d30-6f8e-4bbd-a3dd-6a0742c69aca))
  (segment (start 167.64 55.88) (end 167.64 58.42) (width 1) (layer "B.Cu") (net 89) (tstamp 8afefa03-006b-4e40-b19e-6596c7cc472e))
  (segment (start 170.18 55.88) (end 170.18 58.42) (width 1) (layer "B.Cu") (net 90) (tstamp 72729c20-0465-4f8c-be80-3c22bb337ef7))
  (segment (start 165.1 48.26) (end 165.1 45.72) (width 1) (layer "B.Cu") (net 91) (tstamp 2d0719fe-fc0f-4bd0-a1ce-e486f29e1feb))
  (segment (start 162.56 45.72) (end 162.56 48.26) (width 1) (layer "B.Cu") (net 92) (tstamp 946f7900-583b-43e2-82dd-f42361bcb50e))
  (segment (start 185.42 45.72) (end 185.42 48.26) (width 1) (layer "B.Cu") (net 93) (tstamp 8e247c2e-b63e-4a70-8c32-64933e91ced0))
  (segment (start 182.88 45.72) (end 182.88 48.26) (width 1) (layer "B.Cu") (net 94) (tstamp 086ab04d-4086-427c-992f-819b91a9021d))
  (segment (start 165.1 35.56) (end 165.1 38.1) (width 1) (layer "B.Cu") (net 95) (tstamp 00e39da0-4b3e-4884-a91e-86d729914953))
  (segment (start 162.56 35.56) (end 162.56 38.1) (width 1) (layer "B.Cu") (net 96) (tstamp 59246647-4e57-4b5f-9f1e-b0cc1fb90bb2))
  (segment (start 185.42 35.56) (end 185.42 38.1) (width 1) (layer "B.Cu") (net 97) (tstamp f58742f8-e57e-4646-a6f5-0463e0eceeb8))
  (segment (start 182.88 35.56) (end 182.88 38.1) (width 1) (layer "B.Cu") (net 98) (tstamp 51bdd1cb-8a01-4b1c-940a-3ff4dd1de87c))
  (segment (start 48.26 27.94) (end 48.26 25.4) (width 1) (layer "B.Cu") (net 99) (tstamp 96ff7901-397b-4805-be63-a50021c1204e))
  (segment (start 45.72 27.94) (end 45.72 25.4) (width 1) (layer "B.Cu") (net 100) (tstamp c1cf7bb0-c2ea-4f94-962c-ac20c4c0f2a7))
  (segment (start 43.18 27.94) (end 43.18 25.4) (width 1) (layer "B.Cu") (net 101) (tstamp 6cbce139-87df-4554-a528-17f1ab2ac3fd))
  (segment (start 40.64 27.94) (end 40.64 25.4) (width 1) (layer "B.Cu") (net 102) (tstamp adb36798-0fe9-413e-b035-edd5622ed7a9))
  (segment (start 152.4 66.04) (end 152.4 68.58) (width 1) (layer "B.Cu") (net 103) (tstamp 054f8e07-0141-451f-a3c4-ea786b83b680))
  (segment (start 172.72 68.58) (end 172.72 66.04) (width 1) (layer "B.Cu") (net 104) (tstamp ed6caead-58a0-4a37-97cf-621d3ffb0ca4))
  (segment (start 152.4 55.88) (end 152.4 58.42) (width 1) (layer "B.Cu") (net 105) (tstamp 62af6e3c-7d06-438a-b62f-014ae3262ea1))
  (segment (start 172.72 55.88) (end 172.72 58.42) (width 1) (layer "B.Cu") (net 106) (tstamp afc1392c-4488-4251-8167-de520abba754))
  (segment (start 160.02 48.26) (end 160.02 45.72) (width 1) (layer "B.Cu") (net 107) (tstamp f60dae52-c28c-46c1-b027-f3d548cb9533))
  (segment (start 180.34 45.72) (end 180.34 48.26) (width 1) (layer "B.Cu") (net 108) (tstamp e7c8f673-e523-47ce-91b8-92cf1c7605ce))
  (segment (start 160.02 35.56) (end 160.02 38.1) (width 1) (layer "B.Cu") (net 109) (tstamp eb06cbed-9a37-40e7-bc33-37acd0ee650a))
  (segment (start 180.34 35.56) (end 180.34 38.1) (width 1) (layer "B.Cu") (net 110) (tstamp 172b515f-13aa-42a2-b6ac-db67c2e524e7))
  (segment (start 154.94 68.58) (end 154.94 66.04) (width 1) (layer "B.Cu") (net 111) (tstamp 3c5840eb-164e-426c-ab78-faa89624b9dc))
  (segment (start 175.26 66.04) (end 175.26 68.58) (width 1) (layer "B.Cu") (net 112) (tstamp 43b7aab0-ec9b-4c58-bfa1-8dda8fccb53f))
  (segment (start 154.94 58.42) (end 154.94 55.88) (width 1) (layer "B.Cu") (net 113) (tstamp 5968c877-7376-4e25-b8db-5e755d570d06))
  (segment (start 175.26 58.42) (end 175.26 55.88) (width 1) (layer "B.Cu") (net 114) (tstamp 1cd85cce-d94a-4a92-8af2-23d3a2b66793))
  (segment (start 157.48 45.72) (end 157.48 48.26) (width 1) (layer "B.Cu") (net 115) (tstamp 48cf037b-c0bb-47d5-960f-7e5c24fc1376))
  (segment (start 177.8 45.72) (end 177.8 48.26) (width 1) (layer "B.Cu") (net 116) (tstamp d40ed1bf-6a69-492a-acf3-f71f1c7a81f2))
  (segment (start 157.48 35.56) (end 157.48 38.1) (width 1) (layer "B.Cu") (net 117) (tstamp 67320774-1745-4c89-bec7-2213f7bb7ecc))
  (segment (start 177.8 35.56) (end 177.8 38.1) (width 1) (layer "B.Cu") (net 118) (tstamp cab0d0a9-e089-4f0b-8483-22b4e0addcae))
  (segment (start 157.48 66.04) (end 157.48 68.58) (width 1) (layer "B.Cu") (net 119) (tstamp a5c35670-98af-44c6-a3f4-bbad7ffecfd3))
  (segment (start 177.8 68.58) (end 177.8 66.04) (width 1) (layer "B.Cu") (net 120) (tstamp 5bd90e77-727e-49e2-881e-09f4ce3768d4))
  (segment (start 157.48 55.88) (end 157.48 58.42) (width 1) (layer "B.Cu") (net 121) (tstamp af7ccd5a-4c05-4a49-a412-ca568e4c81d2))
  (segment (start 177.8 55.88) (end 177.8 58.42) (width 1) (layer "B.Cu") (net 122) (tstamp 911557e5-adec-4d13-9794-a18b325eb4ea))
  (segment (start 154.94 48.26) (end 154.94 45.72) (width 1) (layer "B.Cu") (net 123) (tstamp 2efefeab-092e-4142-9694-74d47d2fb517))
  (segment (start 175.26 45.72) (end 175.26 48.26) (width 1) (layer "B.Cu") (net 124) (tstamp a26bc030-7d8a-4b19-aa84-9206cc0de2b0))
  (segment (start 154.94 35.56) (end 154.94 38.1) (width 1) (layer "B.Cu") (net 125) (tstamp d66c8b0e-b6b3-43ea-8c6d-9724edcc57d6))
  (segment (start 175.26 35.56) (end 175.26 38.1) (width 1) (layer "B.Cu") (net 126) (tstamp 3d19e22b-2666-4e7d-825d-37a04ed07fa1))
  (segment (start 160.02 68.58) (end 160.02 66.04) (width 1) (layer "B.Cu") (net 127) (tstamp 6025c071-1487-4c03-a645-f67437519813))
  (segment (start 180.34 66.04) (end 180.34 68.58) (width 1) (layer "B.Cu") (net 128) (tstamp b79d8d99-88b5-4d84-a010-b6d768d67ec8))
  (segment (start 160.02 58.42) (end 160.02 55.88) (width 1) (layer "B.Cu") (net 129) (tstamp a2c0fc07-9ed2-42e8-8fef-f02fce3412ee))
  (segment (start 180.34 58.42) (end 180.34 55.88) (width 1) (layer "B.Cu") (net 130) (tstamp 0d678ff1-21aa-4e6f-ae06-abf24406f3c8))
  (segment (start 152.4 45.72) (end 152.4 48.26) (width 1) (layer "B.Cu") (net 131) (tstamp ec468e5f-028c-4af9-8f4a-d9867986f0db))
  (segment (start 172.72 45.72) (end 172.72 48.26) (width 1) (layer "B.Cu") (net 132) (tstamp 248d15cd-dd0c-425d-94cb-b44ccf865457))
  (segment (start 152.4 35.56) (end 152.4 38.1) (width 1) (layer "B.Cu") (net 133) (tstamp 42688fc6-3e24-4a56-9963-828da46dcdfb))
  (segment (start 172.72 35.56) (end 172.72 38.1) (width 1) (layer "B.Cu") (net 134) (tstamp c546008e-7661-419e-94b3-0bbb9fd14ec8))
  (segment (start 162.56 66.04) (end 162.56 68.58) (width 1) (layer "B.Cu") (net 135) (tstamp 40962e92-90b6-487d-b0dc-0a6c42b5ebc2))
  (segment (start 182.88 68.58) (end 182.88 66.04) (width 1) (layer "B.Cu") (net 136) (tstamp 25b39db8-8576-4473-b331-b912323e85f4))
  (segment (start 162.56 55.88) (end 162.56 58.42) (width 1) (layer "B.Cu") (net 137) (tstamp ffde4898-4c0e-4c24-bd8c-aadcd7279172))
  (segment (start 182.88 55.88) (end 182.88 58.42) (width 1) (layer "B.Cu") (net 138) (tstamp 5aa0e472-160b-49ac-864f-0fa7cd9cf9b0))
  (segment (start 149.86 48.26) (end 149.86 45.72) (width 1) (layer "B.Cu") (net 139) (tstamp 49cfc58a-a40a-4afa-88e7-b4479026992a))
  (segment (start 170.18 45.72) (end 170.18 48.26) (width 1) (layer "B.Cu") (net 140) (tstamp a5fcd820-f4f0-487d-8e2f-6defe7618982))
  (segment (start 149.86 35.56) (end 149.86 38.1) (width 1) (layer "B.Cu") (net 141) (tstamp bf67f245-1714-4d39-b76d-53f1523ab5f8))
  (segment (start 170.18 35.56) (end 170.18 38.1) (width 1) (layer "B.Cu") (net 142) (tstamp ccd45da3-3d73-496d-8f2e-5edf69377f63))
  (segment (start 165.1 68.58) (end 165.1 66.04) (width 1) (layer "B.Cu") (net 143) (tstamp 31e2d26e-842a-4694-a3ae-7642d792727c))
  (segment (start 185.42 66.04) (end 185.42 68.58) (width 1) (layer "B.Cu") (net 144) (tstamp da151d0a-a1fa-4865-aa78-eb4b6082fbfd))
  (segment (start 165.1 58.42) (end 165.1 55.88) (width 1) (layer "B.Cu") (net 145) (tstamp 76a87642-211c-44f2-a488-190d6dc3728e))
  (segment (start 185.42 58.42) (end 185.42 55.88) (width 1) (layer "B.Cu") (net 146) (tstamp 2ff15691-c9f8-4e08-a694-3230522780fc))
  (segment (start 147.32 45.72) (end 147.32 48.26) (width 1) (layer "B.Cu") (net 147) (tstamp 4713a3a2-2b78-4e82-ab5e-15cd752078e0))
  (segment (start 167.64 45.72) (end 167.64 48.26) (width 1) (layer "B.Cu") (net 148) (tstamp a6386af6-d744-458e-b19d-8fd97b5ad9f9))
  (segment (start 147.32 38.1) (end 147.32 35.56) (width 1) (layer "B.Cu") (net 149) (tstamp 01600802-66c5-45a2-be7f-4fa2327d845b))
  (segment (start 167.64 35.56) (end 167.64 38.1) (width 1) (layer "B.Cu") (net 150) (tstamp fc80fa5b-8c07-4dda-8002-331dcafd556b))
  (segment (start 40.64 35.56) (end 40.64 38.1) (width 1) (layer "B.Cu") (net 151) (tstamp 4ad5f6bc-6ae6-4e1c-8525-1e31a01a7930))
  (segment (start 43.18 38.1) (end 43.18 35.56) (width 1) (layer "B.Cu") (net 152) (tstamp 6802b5d4-85bc-4506-b915-e3373f657648))
  (segment (start 45.72 38.1) (end 45.72 35.56) (width 1) (layer "B.Cu") (net 153) (tstamp 68551524-5d23-4a54-a0a7-07cbb43d361d))
  (segment (start 48.26 38.1) (end 48.26 35.56) (width 1) (layer "B.Cu") (net 154) (tstamp caf5789c-8255-4529-8b56-f7568ad55af7))
  (segment (start 50.8 38.1) (end 50.8 35.56) (width 1) (layer "B.Cu") (net 155) (tstamp bb27c4a8-d58e-4c64-9502-0f15c15c3b43))
  (segment (start 53.34 38.1) (end 53.34 35.56) (width 1) (layer "B.Cu") (net 156) (tstamp fafeafcb-685f-41f2-bbe7-a18250d8fbe4))
  (segment (start 55.88 38.1) (end 55.88 35.56) (width 1) (layer "B.Cu") (net 157) (tstamp 98f16e8d-7d53-4d1e-b2b5-936f535e3a6d))
  (segment (start 58.42 38.1) (end 58.42 35.56) (width 1) (layer "B.Cu") (net 158) (tstamp f08bd128-ad91-4e83-b37f-2ad975a540cc))
  (segment (start 33.02 58.42) (end 33.02 55.88) (width 1) (layer "B.Cu") (net 168) (tstamp 52d06145-6ecc-4258-8b28-5673da5da386))
  (segment (start 38.1 53.34) (end 33.02 53.34) (width 1) (layer "B.Cu") (net 168) (tstamp 6fafa09f-b34f-4183-bceb-868b804308f9))
  (segment (start 33.02 53.34) (end 33.02 55.88) (width 1) (layer "B.Cu") (net 168) (tstamp a9ab623c-bc91-4cfd-9357-bc71cc66025d))
  (segment (start 38.1 48.26) (end 38.1 53.34) (width 1) (layer "B.Cu") (net 168) (tstamp bbe5c00c-19fc-4d57-bdaf-434080a9cd15))
  (segment (start 58.42 45.72) (end 58.42 48.26) (width 1) (layer "B.Cu") (net 169) (tstamp 7a58c66d-88d7-4c34-b31f-f5cdfcab923a))
  (segment (start 55.88 45.72) (end 55.88 48.26) (width 1) (layer "B.Cu") (net 170) (tstamp 0ac0dc2c-1ce5-4a62-8531-b68c56f41095))
  (segment (start 53.34 48.26) (end 53.34 45.72) (width 1) (layer "B.Cu") (net 171) (tstamp bd46998a-ae54-421c-b8e7-d6d07c32ea52))
  (segment (start 50.8 45.72) (end 50.8 48.26) (width 1) (layer "B.Cu") (net 172) (tstamp 94c5169c-6d89-4cf1-acdb-0202793b2ea9))
  (segment (start 48.26 48.26) (end 48.26 45.72) (width 1) (layer "B.Cu") (net 173) (tstamp e02127e7-d232-4387-af9b-628b71d0b8e7))
  (segment (start 45.72 45.72) (end 45.72 48.26) (width 1) (layer "B.Cu") (net 174) (tstamp 9c8a1312-b716-4c8c-a328-252fb4259147))
  (segment (start 43.18 45.72) (end 43.18 48.26) (width 1) (layer "B.Cu") (net 175) (tstamp e6848f87-9e82-4a77-aeab-3ae292f7cd81))
  (segment (start 40.64 48.26) (end 40.64 45.72) (width 1) (layer "B.Cu") (net 176) (tstamp 1f389677-5a99-494f-944d-9214759c9831))
  (segment (start 40.64 55.88) (end 40.64 58.42) (width 1) (layer "B.Cu") (net 177) (tstamp 26691fec-9520-43b2-81cf-de094d98c49a))
  (segment (start 43.18 58.42) (end 43.18 55.88) (width 1) (layer "B.Cu") (net 178) (tstamp 255814d5-4e4b-46be-908d-7c96cb244ba6))
  (segment (start 45.72 55.88) (end 45.72 58.42) (width 1) (layer "B.Cu") (net 179) (tstamp 37bb33b3-24da-4276-ad68-63e4a18e9d06))
  (segment (start 48.26 58.42) (end 48.26 55.88) (width 1) (layer "B.Cu") (net 180) (tstamp e64bacd0-33c2-44b7-8376-5dca0e0fd988))
  (segment (start 50.8 55.88) (end 50.8 58.42) (width 1) (layer "B.Cu") (net 181) (tstamp c840e95b-4463-4596-a8ff-6ce79851566f))
  (segment (start 53.34 58.42) (end 53.34 55.88) (width 1) (layer "B.Cu") (net 182) (tstamp cfcf3410-f022-4731-a1da-2b5d60e67189))
  (segment (start 55.88 58.42) (end 55.88 55.88) (width 1) (layer "B.Cu") (net 183) (tstamp 6cfdc61e-9238-4bf1-8adc-0aa2afd5e23c))
  (segment (start 58.42 55.88) (end 58.42 58.42) (width 1) (layer "B.Cu") (net 184) (tstamp 9d665c46-7e87-4633-b424-129725306384))
  (segment (start 35.56 45.72) (end 35.56 48.26) (width 1) (layer "B.Cu") (net 185) (tstamp 2a1c651e-004a-4460-ab24-57dd24aad133))
  (segment (start 30.48 55.88) (end 27.94 55.88) (width 1) (layer "B.Cu") (net 185) (tstamp 395876dc-25ca-4ac6-b54f-626217f82dba))
  (segment (start 30.48 50.8) (end 30.48 55.88) (width 1) (layer "B.Cu") (net 185) (tstamp 7a8688d7-8605-4222-91a0-983384c364c9))
  (segment (start 35.56 50.8) (end 30.48 50.8) (width 1) (layer "B.Cu") (net 185) (tstamp 8acd8a3e-3426-488b-89ed-18ed2111896e))
  (segment (start 35.56 48.26) (end 35.56 50.8) (width 1) (layer "B.Cu") (net 185) (tstamp bd614e74-ba37-45d1-97aa-35ec67b9eb29))
  (segment (start 27.94 55.88) (end 25.4 55.88) (width 1) (layer "B.Cu") (net 185) (tstamp df75c386-3877-4b84-8d39-8cba635c1f49))
  (segment (start 27.94 48.26) (end 27.94 45.72) (width 1) (layer "B.Cu") (net 186) (tstamp 14e60353-3e9b-4f93-afec-271fdf3266fa))
  (segment (start 30.48 45.72) (end 30.48 48.26) (width 1) (layer "B.Cu") (net 187) (tstamp db4945a1-1cda-4739-a221-abd106873083))

)
